(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu16.04.1-stable)
  (general
    (links 1707)
    (no_connects 989)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 0)
    (tracks 6)
    (zones 0)
    (modules 595)
    (nets 1179)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(B1/CTL3709-PadP$1)")
  (net 2 "Net-(B1/CTL3709-PadP$2)")
  (net 3 "Net-(B12/FN3709-PadP$1)")
  (net 4 "Net-(B2/CTL2301-PadP$2)")
  (net 5 "Net-(B13/SPC2301-PadP$1)")
  (net 6 "Net-(B10/OK3709-PadP$2)")
  (net 7 "Net-(B14/SPC2301-PadP$1)")
  (net 8 "Net-(B15/M3709-PadP$1)")
  (net 9 "Net-(B16/,3709-PadP$1)")
  (net 10 "Net-(B17/PGDN3709-PadP$1)")
  (net 11 "Net-(B18/END3709-PadP$1)")
  (net 12 "Net-(B19/LEFT3709-PadP$1)")
  (net 13 "Net-(B10/OK3709-PadP$1)")
  (net 14 "Net-(B11/ALT3709-PadP$2)")
  (net 15 "Net-(B12/FN3709-PadP$2)")
  (net 16 "Net-(B13/SPC2301-PadP$2)")
  (net 17 "Net-(B21/DEL3709-PadP$2)")
  (net 18 "Net-(B22/3709-PadP$2)")
  (net 19 "Net-(B23/TAB3709-PadP$2)")
  (net 20 "Net-(B31/ALT2301-PadP$2)")
  (net 21 "Net-(B32/SHLCK3709-PadP$2)")
  (net 22 "Net-(B33/ESC3709-PadP$2)")
  (net 23 "Net-(B60/^2301-PadP$2)")
  (net 24 "Net-(B69/O3709-PadP$2)")
  (net 25 "Net-(B79/2301-PadP$2)")
  (net 26 "Net-(BATT+3709-PadP)")
  (net 27 "/Fuel Gauge/BGND")
  (net 28 "Net-(BATT-ID3709-PadP)")
  (net 29 VBUS)
  (net 30 GND)
  (net 31 "Net-(C301-Pad1)")
  (net 32 "Net-(C301-Pad2)")
  (net 33 "Net-(C303-Pad2)")
  (net 34 VSYS)
  (net 35 "Net-(C305-Pad1)")
  (net 36 "Net-(C401-Pad1)")
  (net 37 "Net-(C402-Pad1)")
  (net 38 "Net-(C403-Pad1)")
  (net 39 "Net-(C404-Pad1)")
  (net 40 "Net-(C405-Pad1)")
  (net 41 "Net-(C406-Pad1)")
  (net 42 BATT)
  (net 43 "Net-(C502-Pad1)")
  (net 44 "Net-(C503-Pad1)")
  (net 45 "Net-(C504-Pad1)")
  (net 46 "Net-(C505-Pad1)")
  (net 47 "Net-(C506-Pad1)")
  (net 48 "Net-(C508-Pad1)")
  (net 49 "Net-(C601-Pad1)")
  (net 50 VMODEM3)
  (net 51 VMODEM1)
  (net 52 VMODEM2)
  (net 53 "Net-(C611-Pad1)")
  (net 54 SIM-RST)
  (net 55 VGNSS)
  (net 56 "Net-(C802-Pad1)")
  (net 57 "Net-(C802-Pad2)")
  (net 58 "Net-(C803-Pad1)")
  (net 59 "Net-(C803-Pad2)")
  (net 60 ADC1)
  (net 61 2V7)
  (net 62 ADC2)
  (net 63 "Net-(C808-Pad2)")
  (net 64 "Net-(C809-Pad2)")
  (net 65 3V3)
  (net 66 FM-RX)
  (net 67 "Net-(C901-Pad2)")
  (net 68 1V8)
  (net 69 "Net-(C1011-Pad1)")
  (net 70 "Net-(C1101-Pad1)")
  (net 71 "Net-(C1101-Pad2)")
  (net 72 "Net-(C1102-Pad1)")
  (net 73 "Net-(C1104-Pad1)")
  (net 74 HSL+)
  (net 75 HSL-)
  (net 76 "Net-(C1107-Pad1)")
  (net 77 HSR+)
  (net 78 HSR-)
  (net 79 HFL+)
  (net 80 HFL-)
  (net 81 HFR+)
  (net 82 HFR-)
  (net 83 AGND)
  (net 84 "Net-(C1201-Pad2)")
  (net 85 "Net-(C1203-Pad1)")
  (net 86 "Net-(C1203-Pad2)")
  (net 87 "Net-(C1204-Pad2)")
  (net 88 "Net-(C1205-Pad1)")
  (net 89 "Net-(C1206-Pad2)")
  (net 90 "Net-(C1207-Pad2)")
  (net 91 "Net-(C1208-Pad1)")
  (net 92 "Net-(C1209-Pad2)")
  (net 93 "Net-(C1210-Pad1)")
  (net 94 VMMC2)
  (net 95 "Net-(C1212-Pad1)")
  (net 96 MIC+)
  (net 97 "Net-(C1213-Pad2)")
  (net 98 MIC-)
  (net 99 "Net-(C1214-Pad2)")
  (net 100 "Net-(C1217-Pad1)")
  (net 101 "Net-(C1404-Pad2)")
  (net 102 "Net-(C1405-Pad2)")
  (net 103 "Net-(C1406-Pad2)")
  (net 104 "Net-(C1407-Pad2)")
  (net 105 "Net-(C1408-Pad2)")
  (net 106 "Net-(C1409-Pad2)")
  (net 107 "Net-(C1410-Pad1)")
  (net 108 "/Audio Handsfree/SPKRR+")
  (net 109 "Net-(C1603-Pad2)")
  (net 110 "Net-(C1605-Pad1)")
  (net 111 "Net-(C1605-Pad2)")
  (net 112 NFC-ANT)
  (net 113 "Net-(C1607-Pad1)")
  (net 114 "Net-(C1607-Pad2)")
  (net 115 "Net-(C1610-Pad1)")
  (net 116 "Net-(C1611-Pad2)")
  (net 117 "Net-(C1614-Pad2)")
  (net 118 "Net-(C1623-Pad1)")
  (net 119 "Net-(C1625-Pad1)")
  (net 120 "Net-(C1626-Pad1)")
  (net 121 "Net-(C1627-Pad1)")
  (net 122 "Net-(C1701-Pad1)")
  (net 123 AUDIOIN)
  (net 124 "Net-(C1901-Pad2)")
  (net 125 "Net-(C1902-Pad1)")
  (net 126 UART3-TX_IRTX)
  (net 127 "Net-(C1903-Pad2)")
  (net 128 UART3-CTS_RCTX)
  (net 129 "Net-(C1904-Pad2)")
  (net 130 "/uSD Breakout Board/USD-3V3")
  (net 131 GND2)
  (net 132 "Net-(C2103-Pad1)")
  (net 133 "Net-(C2104-Pad1)")
  (net 134 "Net-(C2105-Pad1)")
  (net 135 1V8-CPU)
  (net 136 GND3)
  (net 137 "Net-(C2402-Pad1)")
  (net 138 DMIC_CLOCK)
  (net 139 "Net-(C2404-Pad1)")
  (net 140 "Net-(C2406-Pad1)")
  (net 141 "Net-(C2407-Pad1)")
  (net 142 "Net-(C2408-Pad1)")
  (net 143 "Net-(C2409-Pad1)")
  (net 144 "Net-(C2410-Pad1)")
  (net 145 VBATT_UPPER)
  (net 146 "Net-(C2502-Pad1)")
  (net 147 "Net-(C2801-Pad1)")
  (net 148 "Net-(C2802-Pad1)")
  (net 149 "Net-(C3001-Pad1)")
  (net 150 VCSI=VAUX2???)
  (net 151 VDDA)
  (net 152 "Net-(C3101-Pad1)")
  (net 153 "Net-(C3101-Pad2)")
  (net 154 "Net-(C3102-Pad1)")
  (net 155 "Net-(C3102-Pad2)")
  (net 156 "Net-(C3103-Pad1)")
  (net 157 VSYS_UPPER)
  (net 158 "Net-(C3205-Pad2)")
  (net 159 "Net-(C3206-Pad2)")
  (net 160 "Net-(C3207-Pad2)")
  (net 161 "Net-(C3208-Pad2)")
  (net 162 BB-5V)
  (net 163 GND4)
  (net 164 "/BB-XM Adapter (CPU)/BB-VSYS")
  (net 165 "Net-(CD3709-PadP)")
  (net 166 UART?-RTS)
  (net 167 USB-WWAN-D+)
  (net 168 USB-WWAN-D-)
  (net 169 LOCK-GPIO)
  (net 170 GPIO-VOL+)
  (net 171 GPIO-VOL-)
  (net 172 POWERON)
  (net 173 CAM1-GPIO)
  (net 174 CAM2-GPIO)
  (net 175 "/WLAN, Bluetooth, FM/LOOP")
  (net 176 "Net-(D1201-Pad1)")
  (net 177 "Net-(D1203-Pad2)")
  (net 178 "Net-(D1204-Pad2)")
  (net 179 "Net-(D1205-Pad2)")
  (net 180 "/RFID/NFC Controller/NFC_LED")
  (net 181 "Net-(D1902-PadA)")
  (net 182 "Net-(D1902-PadK)")
  (net 183 "Net-(D2102-PadA)")
  (net 184 "Net-(D2501-PadA)")
  (net 185 "Net-(D2502-PadA)")
  (net 186 "Net-(D3201-PadA)")
  (net 187 "Net-(D3201-PadK)")
  (net 188 "Net-(D3202-PadA)")
  (net 189 "Net-(D3202-PadK)")
  (net 190 "Net-(DCD3709-PadP)")
  (net 191 "Net-(DSR3709-PadP)")
  (net 192 "Net-(DTR3709-PadP)")
  (net 193 GPIO-MODEM_IGT)
  (net 194 "Net-(GPS-ANT3709-Pad1)")
  (net 195 "Net-(HS-1201-PadP)")
  (net 196 "Net-(HS-1204-PadP)")
  (net 197 "Net-(HS-1206-PadP)")
  (net 198 "Net-(L801-Pad1)")
  (net 199 "Net-(L801-Pad2)")
  (net 200 "Net-(L901-Pad1)")
  (net 201 "Net-(L901-Pad2)")
  (net 202 "Net-(L1401-Pad2)")
  (net 203 "Net-(L1402-Pad2)")
  (net 204 "Net-(L1403-Pad2)")
  (net 205 "Net-(L1404-Pad2)")
  (net 206 "/uSD Breakout Board/USD-VBATT")
  (net 207 DMIC_BIAS)
  (net 208 /Display-Panel&Power/CDP-D0+_UPPER)
  (net 209 /Display-Panel&Power/CDP-D0-_UPPER)
  (net 210 "Net-(L2502-Pad3)")
  (net 211 "Net-(L2502-Pad4)")
  (net 212 /Display-Panel&Power/CDP-D1+_UPPER)
  (net 213 /Display-Panel&Power/CDP-D1-_UPPER)
  (net 214 "Net-(L2503-Pad3)")
  (net 215 "Net-(L2503-Pad4)")
  (net 216 /Display-Panel&Power/CDP-CLK+_UPPER)
  (net 217 /Display-Panel&Power/CDP-CLK-_UPPER)
  (net 218 "Net-(L2504-Pad3)")
  (net 219 "Net-(L2504-Pad4)")
  (net 220 VAUX??)
  (net 221 LC_IND)
  (net 222 "Net-(LED2101-Pad1)")
  (net 223 "Net-(LED2102-PadK)")
  (net 224 "Net-(LED2103-Pad1)")
  (net 225 "Net-(LED3101-Pad1)")
  (net 226 "Net-(LED3101-Pad2)")
  (net 227 "Net-(LED3101-Pad3)")
  (net 228 "Net-(LED3102-Pad1)")
  (net 229 "Net-(LED3102-Pad2)")
  (net 230 "Net-(LED3102-Pad3)")
  (net 231 "Net-(LED3201-Pad1)")
  (net 232 "Net-(LED3201-Pad2)")
  (net 233 "Net-(LED3201-Pad3)")
  (net 234 "Net-(LED3202-Pad1)")
  (net 235 "Net-(LED3202-Pad2)")
  (net 236 "Net-(LED3202-Pad3)")
  (net 237 "Net-(LED3203-Pad1)")
  (net 238 "Net-(LED3203-Pad2)")
  (net 239 "Net-(LED3203-Pad3)")
  (net 240 "Net-(LED3204-Pad1)")
  (net 241 "Net-(LED3204-Pad2)")
  (net 242 "Net-(LED3204-Pad3)")
  (net 243 "Net-(LED3205-Pad1)")
  (net 244 "Net-(LED3205-Pad2)")
  (net 245 "Net-(LED3205-Pad3)")
  (net 246 "Net-(LED3206-Pad4)")
  (net 247 "Net-(LED3206-Pad5)")
  (net 248 "Net-(LED3206-Pad6)")
  (net 249 "Net-(LED3207-PadK)")
  (net 250 "Net-(LED3208-Pad1)")
  (net 251 "Net-(LED3208-Pad2)")
  (net 252 "Net-(LED3208-Pad3)")
  (net 253 "Net-(LED3209-PadK)")
  (net 254 CHG_IND)
  (net 255 GSM-ANT-DRX)
  (net 256 STATUS)
  (net 257 "Net-(M601-PadC14)")
  (net 258 ANT-GNSS-DC)
  (net 259 "Net-(M601-PadD15)")
  (net 260 "Net-(M601-PadD16)")
  (net 261 GNSS-IN)
  (net 262 "Net-(M601-PadE15)")
  (net 263 "Net-(M601-PadE16)")
  (net 264 3G-WOE)
  (net 265 GSM-ANT-TRX)
  (net 266 MODEM_DATA_A)
  (net 267 MODEM_RST_A)
  (net 268 MODEM_CLK_A)
  (net 269 "/3G/4G Modem + SIM/ON_KEY")
  (net 270 PWR_IND)
  (net 271 "Net-(M601-PadM5)")
  (net 272 MCBSP4-DX)
  (net 273 MCBSP4-CLKX)
  (net 274 MCBSP4-FSX)
  (net 275 MCBSP4-DR)
  (net 276 MODEM-CD_A)
  (net 277 VBUS-MODEM)
  (net 278 "Net-(M601-PadN6)")
  (net 279 "Net-(M601-PadN7)")
  (net 280 UART?-CTS)
  (net 281 EMERG_OFF)
  (net 282 "Net-(M601-PadP6)")
  (net 283 "Net-(M601-PadP7)")
  (net 284 RING)
  (net 285 UART?-TX)
  (net 286 UART?-RX)
  (net 287 "Net-(M901-Pad2)")
  (net 288 "Net-(M901-Pad3)")
  (net 289 "Net-(M901-Pad4)")
  (net 290 "Net-(M901-Pad5)")
  (net 291 "/WLAN, Bluetooth, FM/N$82")
  (net 292 "/WLAN, Bluetooth, FM/N$97")
  (net 293 "/WLAN, Bluetooth, FM/N$63")
  (net 294 "/WLAN, Bluetooth, FM/N$62")
  (net 295 "/WLAN, Bluetooth, FM/N$59")
  (net 296 "/WLAN, Bluetooth, FM/N$61")
  (net 297 WLAN-IRQ)
  (net 298 "/WLAN, Bluetooth, FM/ANT2")
  (net 299 "Net-(M901-Pad25)")
  (net 300 "Net-(M901-Pad26)")
  (net 301 "Net-(M901-Pad27)")
  (net 302 "/WLAN, Bluetooth, FM/N$9")
  (net 303 32KHZ)
  (net 304 WLAN-EN)
  (net 305 BT-EN)
  (net 306 "Net-(M901-Pad42)")
  (net 307 "Net-(M901-Pad43)")
  (net 308 VBATT)
  (net 309 "/WLAN, Bluetooth, FM/N$57")
  (net 310 "/WLAN, Bluetooth, FM/N$15")
  (net 311 "/WLAN, Bluetooth, FM/N$36")
  (net 312 "/WLAN, Bluetooth, FM/N$13")
  (net 313 "/WLAN, Bluetooth, FM/BT-PCM-DX")
  (net 314 "/WLAN, Bluetooth, FM/BT-PCM-DR")
  (net 315 "/WLAN, Bluetooth, FM/N$319")
  (net 316 "/WLAN, Bluetooth, FM/N$312")
  (net 317 DMIC_DATA)
  (net 318 3V3-CPU)
  (net 319 VMMC2-CPU)
  (net 320 EAR-_UPPER)
  (net 321 EAR+_UPPER)
  (net 322 "Net-(P-DISP3709-Pad8)")
  (net 323 2V5_UPPER)
  (net 324 "Net-(P-DISP3709-Pad10)")
  (net 325 I2C2-SDA-CPU)
  (net 326 I2C2-SCL-CPU)
  (net 327 GPIO97)
  (net 328 N$49_UPPER)
  (net 329 N$50_UPPER)
  (net 330 N$41_UPPER)
  (net 331 2V8_UPPER)
  (net 332 "Net-(P-DISP3709-Pad29)")
  (net 333 "Net-(P-DISP3709-Pad30)")
  (net 334 "Net-(P-DISP3709-Pad34)")
  (net 335 "Net-(P-DISP3709-Pad35)")
  (net 336 "Net-(P-DISP3709-Pad36)")
  (net 337 "Net-(P-DISP3709-Pad37)")
  (net 338 "Net-(P-DISP3709-Pad38)")
  (net 339 /Camera/CSI-B-C-_UPPER)
  (net 340 /Camera/CSI-B-C+_UPPER)
  (net 341 /Camera/CSI-B-D-_UPPER)
  (net 342 /Camera/CSI-B-D+_UPPER)
  (net 343 CAM-CLK)
  (net 344 "Net-(P-DISP3709-Pad61)")
  (net 345 "Net-(P-DISP3709-Pad62)")
  (net 346 "Net-(P-DISP3709-Pad63)")
  (net 347 "Net-(P-INT801-PadSIG)")
  (net 348 "Net-(P-MICRO-SD3709-Pad1)")
  (net 349 "Net-(P-MICRO-SD3709-Pad2)")
  (net 350 "Net-(P-MICRO-SD3709-Pad3)")
  (net 351 "Net-(P-MICRO-SD3709-Pad5)")
  (net 352 "Net-(P-MICRO-SD3709-Pad7)")
  (net 353 "Net-(P-MICRO-SD3709-Pad8)")
  (net 354 VBUS-MODEM-CPU)
  (net 355 MODEM-CPU-D-)
  (net 356 MODEM-CPU-D+)
  (net 357 "Net-(P-MODEM3709-OTG2-Pad4/ID)")
  (net 358 OTG-D-)
  (net 359 OTG-D+)
  (net 360 OTG-ID)
  (net 361 "Net-(P-SIM701-PadC1)")
  (net 362 "/Dual SIM switch/N$224")
  (net 363 "/Dual SIM switch/N$137")
  (net 364 "/Dual SIM switch/N$342")
  (net 365 "/Dual SIM switch/N$338")
  (net 366 SIM-CLK)
  (net 367 SIM-DATA)
  (net 368 SD-DAT2)
  (net 369 I2C2-SDA)
  (net 370 SD-DAT3)
  (net 371 I2C2-SCL)
  (net 372 SD-CMD)
  (net 373 GPIO-FLASH-STR)
  (net 374 SD-VDD)
  (net 375 GPIO-FLASH-EN)
  (net 376 SD-CLK)
  (net 377 GPIO-FLASH-INT)
  (net 378 GPIO-CAM-COVER)
  (net 379 SD-DAT1)
  (net 380 SD-DAT0)
  (net 381 GPIO-BATT-LID)
  (net 382 SD-CD)
  (net 383 "Net-(P2001-Pad3)")
  (net 384 "Net-(P2001-Pad4)")
  (net 385 "Net-(P2001-Pad5)")
  (net 386 "Net-(P2001-Pad6)")
  (net 387 "Net-(P2001-Pad7)")
  (net 388 "Net-(P2001-Pad8)")
  (net 389 "Net-(P2001-Pad9)")
  (net 390 "Net-(P2001-Pad10)")
  (net 391 "Net-(P2001-Pad11)")
  (net 392 "Net-(P2001-Pad12)")
  (net 393 "Net-(P2001-Pad13)")
  (net 394 "Net-(P2001-Pad14)")
  (net 395 "Net-(P2001-Pad15)")
  (net 396 "Net-(P2001-Pad16)")
  (net 397 "Net-(P2001-Pad17)")
  (net 398 "Net-(P2001-Pad18)")
  (net 399 "Net-(P2001-Pad19)")
  (net 400 "Net-(P2001-Pad20)")
  (net 401 "Net-(P2001-Pad21)")
  (net 402 "Net-(P2001-Pad22)")
  (net 403 "Net-(P2001-Pad23)")
  (net 404 "Net-(P2001-Pad24)")
  (net 405 "Net-(P2001-Pad25)")
  (net 406 "Net-(P2001-Pad26)")
  (net 407 "Net-(P2001-Pad27)")
  (net 408 "Net-(P2001-Pad28)")
  (net 409 "Net-(P2001-Pad33)")
  (net 410 "Net-(P2001-Pad34)")
  (net 411 "Net-(P2001-Pad35)")
  (net 412 "Net-(P2001-Pad36)")
  (net 413 "Net-(P2001-Pad37)")
  (net 414 "Net-(P2001-Pad38)")
  (net 415 "Net-(P2001-Pad39)")
  (net 416 "Net-(P2001-Pad40)")
  (net 417 "Net-(P2001-Pad41)")
  (net 418 "Net-(P2001-Pad42)")
  (net 419 "Net-(P2001-Pad43)")
  (net 420 "Net-(P2001-Pad44)")
  (net 421 "Net-(P2001-Pad45)")
  (net 422 "Net-(P2001-Pad46)")
  (net 423 "Net-(P2001-Pad47)")
  (net 424 "Net-(P2001-Pad48)")
  (net 425 "Net-(P2001-Pad49)")
  (net 426 "Net-(P2001-Pad50)")
  (net 427 "Net-(P2001-Pad51)")
  (net 428 "Net-(P2001-Pad52)")
  (net 429 "Net-(P2001-Pad53)")
  (net 430 "Net-(P2001-Pad54)")
  (net 431 "Net-(P2001-Pad55)")
  (net 432 "Net-(P2001-Pad56)")
  (net 433 "Net-(P2001-Pad57)")
  (net 434 "Net-(P2001-Pad58)")
  (net 435 "Net-(P2002-Pad3)")
  (net 436 "Net-(P2002-Pad4)")
  (net 437 "Net-(P2002-Pad5)")
  (net 438 "Net-(P2002-Pad6)")
  (net 439 "Net-(P2002-Pad7)")
  (net 440 "Net-(P2002-Pad8)")
  (net 441 "Net-(P2002-Pad9)")
  (net 442 "Net-(P2002-Pad10)")
  (net 443 "Net-(P2002-Pad11)")
  (net 444 "Net-(P2002-Pad12)")
  (net 445 "Net-(P2002-Pad13)")
  (net 446 "Net-(P2002-Pad14)")
  (net 447 "Net-(P2002-Pad15)")
  (net 448 "Net-(P2002-Pad16)")
  (net 449 "Net-(P2002-Pad17)")
  (net 450 "Net-(P2002-Pad18)")
  (net 451 "Net-(P2002-Pad19)")
  (net 452 "Net-(P2002-Pad20)")
  (net 453 "Net-(P2002-Pad21)")
  (net 454 "Net-(P2002-Pad22)")
  (net 455 "Net-(P2002-Pad23)")
  (net 456 "Net-(P2002-Pad24)")
  (net 457 "Net-(P2002-Pad25)")
  (net 458 "Net-(P2002-Pad26)")
  (net 459 "Net-(P2002-Pad27)")
  (net 460 "Net-(P2002-Pad28)")
  (net 461 "Net-(P2002-Pad33)")
  (net 462 "Net-(P2002-Pad34)")
  (net 463 "Net-(P2002-Pad35)")
  (net 464 "Net-(P2002-Pad36)")
  (net 465 "Net-(P2002-Pad37)")
  (net 466 "Net-(P2002-Pad38)")
  (net 467 "Net-(P2002-Pad39)")
  (net 468 "Net-(P2002-Pad40)")
  (net 469 "Net-(P2002-Pad41)")
  (net 470 "Net-(P2002-Pad42)")
  (net 471 "Net-(P2002-Pad43)")
  (net 472 "Net-(P2002-Pad44)")
  (net 473 "Net-(P2002-Pad45)")
  (net 474 "Net-(P2002-Pad46)")
  (net 475 "Net-(P2002-Pad47)")
  (net 476 "Net-(P2002-Pad48)")
  (net 477 "Net-(P2002-Pad49)")
  (net 478 "Net-(P2002-Pad50)")
  (net 479 "Net-(P2002-Pad51)")
  (net 480 "Net-(P2002-Pad52)")
  (net 481 "Net-(P2002-Pad53)")
  (net 482 "Net-(P2002-Pad54)")
  (net 483 "Net-(P2002-Pad55)")
  (net 484 "Net-(P2002-Pad56)")
  (net 485 "Net-(P2002-Pad57)")
  (net 486 "Net-(P2002-Pad58)")
  (net 487 "/uSD Breakout Board/USD-I2C2-SDA")
  (net 488 "/uSD Breakout Board/USD-I2C2-SCL")
  (net 489 "/uSD Breakout Board/USD-STR")
  (net 490 "/uSD Breakout Board/USD-EN")
  (net 491 "/uSD Breakout Board/USD-INT")
  (net 492 "Net-(P2101-Pad13)")
  (net 493 "/uSD Breakout Board/LID")
  (net 494 "Net-(P2201-Pad3)")
  (net 495 "Net-(P2201-Pad4)")
  (net 496 "Net-(P2201-Pad5)")
  (net 497 "Net-(P2201-Pad6)")
  (net 498 "Net-(P2201-Pad7)")
  (net 499 "Net-(P2201-Pad8)")
  (net 500 "Net-(P2201-Pad9)")
  (net 501 "Net-(P2201-Pad10)")
  (net 502 "Net-(P2201-Pad11)")
  (net 503 "Net-(P2201-Pad12)")
  (net 504 "Net-(P2201-Pad13)")
  (net 505 "Net-(P2201-Pad14)")
  (net 506 "Net-(P2201-Pad15)")
  (net 507 "Net-(P2201-Pad16)")
  (net 508 "Net-(P2201-Pad17)")
  (net 509 "Net-(P2201-Pad18)")
  (net 510 "Net-(P2201-Pad19)")
  (net 511 "Net-(P2201-Pad20)")
  (net 512 "Net-(P2201-Pad21)")
  (net 513 "Net-(P2201-Pad22)")
  (net 514 "Net-(P2201-Pad23)")
  (net 515 "Net-(P2201-Pad24)")
  (net 516 "Net-(P2201-Pad25)")
  (net 517 "Net-(P2201-Pad26)")
  (net 518 "Net-(P2201-Pad27)")
  (net 519 "Net-(P2201-Pad28)")
  (net 520 "Net-(P2201-Pad33)")
  (net 521 "Net-(P2201-Pad34)")
  (net 522 "Net-(P2201-Pad35)")
  (net 523 "Net-(P2201-Pad36)")
  (net 524 "Net-(P2201-Pad37)")
  (net 525 "Net-(P2201-Pad38)")
  (net 526 "Net-(P2201-Pad39)")
  (net 527 "Net-(P2201-Pad40)")
  (net 528 "Net-(P2201-Pad41)")
  (net 529 "Net-(P2201-Pad42)")
  (net 530 "Net-(P2201-Pad43)")
  (net 531 "Net-(P2201-Pad44)")
  (net 532 "Net-(P2201-Pad45)")
  (net 533 "Net-(P2201-Pad46)")
  (net 534 "Net-(P2201-Pad47)")
  (net 535 "Net-(P2201-Pad48)")
  (net 536 "Net-(P2201-Pad49)")
  (net 537 "Net-(P2201-Pad50)")
  (net 538 "Net-(P2201-Pad51)")
  (net 539 "Net-(P2201-Pad52)")
  (net 540 "Net-(P2201-Pad53)")
  (net 541 "Net-(P2201-Pad54)")
  (net 542 "Net-(P2201-Pad55)")
  (net 543 "Net-(P2201-Pad56)")
  (net 544 "Net-(P2201-Pad57)")
  (net 545 "Net-(P2201-Pad58)")
  (net 546 "Net-(P2202-Pad3)")
  (net 547 "Net-(P2202-Pad4)")
  (net 548 "Net-(P2202-Pad5)")
  (net 549 "Net-(P2202-Pad6)")
  (net 550 "Net-(P2202-Pad7)")
  (net 551 "Net-(P2202-Pad8)")
  (net 552 "Net-(P2202-Pad9)")
  (net 553 "Net-(P2202-Pad10)")
  (net 554 "Net-(P2202-Pad11)")
  (net 555 "Net-(P2202-Pad12)")
  (net 556 "Net-(P2202-Pad13)")
  (net 557 "Net-(P2202-Pad14)")
  (net 558 "Net-(P2202-Pad15)")
  (net 559 "Net-(P2202-Pad16)")
  (net 560 "Net-(P2202-Pad17)")
  (net 561 "Net-(P2202-Pad18)")
  (net 562 "Net-(P2202-Pad19)")
  (net 563 "Net-(P2202-Pad20)")
  (net 564 "Net-(P2202-Pad21)")
  (net 565 "Net-(P2202-Pad22)")
  (net 566 "Net-(P2202-Pad23)")
  (net 567 "Net-(P2202-Pad24)")
  (net 568 "Net-(P2202-Pad25)")
  (net 569 "Net-(P2202-Pad26)")
  (net 570 "Net-(P2202-Pad27)")
  (net 571 "Net-(P2202-Pad28)")
  (net 572 "Net-(P2202-Pad30)")
  (net 573 "Net-(P2202-Pad33)")
  (net 574 "Net-(P2202-Pad34)")
  (net 575 "Net-(P2202-Pad35)")
  (net 576 "Net-(P2202-Pad36)")
  (net 577 "Net-(P2202-Pad37)")
  (net 578 "Net-(P2202-Pad38)")
  (net 579 "Net-(P2202-Pad39)")
  (net 580 "Net-(P2202-Pad40)")
  (net 581 "Net-(P2202-Pad41)")
  (net 582 "Net-(P2202-Pad42)")
  (net 583 "Net-(P2202-Pad43)")
  (net 584 "Net-(P2202-Pad44)")
  (net 585 "Net-(P2202-Pad45)")
  (net 586 "Net-(P2202-Pad46)")
  (net 587 "Net-(P2202-Pad47)")
  (net 588 "Net-(P2202-Pad48)")
  (net 589 "Net-(P2202-Pad49)")
  (net 590 "Net-(P2202-Pad50)")
  (net 591 "Net-(P2202-Pad51)")
  (net 592 "Net-(P2202-Pad52)")
  (net 593 "Net-(P2202-Pad53)")
  (net 594 "Net-(P2202-Pad54)")
  (net 595 "Net-(P2202-Pad55)")
  (net 596 "Net-(P2202-Pad56)")
  (net 597 "Net-(P2202-Pad57)")
  (net 598 "Net-(P2202-Pad58)")
  (net 599 "Net-(P3001-Pad1)")
  (net 600 "Net-(P3001-Pad6)")
  (net 601 "Net-(P3001-Pad7)")
  (net 602 "Net-(P3001-Pad9)")
  (net 603 "Net-(P3001-Pad10)")
  (net 604 /Camera/GPIO102)
  (net 605 I2C3-SCL-CPU)
  (net 606 I2C3-SDA-CPU)
  (net 607 "Net-(P3301-Pad5)")
  (net 608 "Net-(P3301-Pad6)")
  (net 609 "Net-(P3301-Pad11)")
  (net 610 "Net-(P3301-Pad12)")
  (net 611 "Net-(P3301-Pad13)")
  (net 612 "Net-(P3301-Pad14)")
  (net 613 "Net-(P3301-Pad15)")
  (net 614 "Net-(P3301-Pad16)")
  (net 615 "Net-(P3301-Pad17)")
  (net 616 "Net-(P3301-Pad18)")
  (net 617 "Net-(P3301-Pad19)")
  (net 618 "Net-(P3301-Pad20)")
  (net 619 "Net-(P3301-Pad21)")
  (net 620 "Net-(P3301-Pad22)")
  (net 621 "Net-(P3301-Pad23)")
  (net 622 "Net-(P3301-Pad24)")
  (net 623 "Net-(P3301-Pad25)")
  (net 624 "Net-(P3301-Pad26)")
  (net 625 "Net-(P3301-Pad27)")
  (net 626 "Net-(P3301-Pad28)")
  (net 627 "Net-(P3301-Pad29)")
  (net 628 "Net-(P3301-Pad30)")
  (net 629 "Net-(P3301-Pad31)")
  (net 630 "Net-(P3301-Pad32)")
  (net 631 "Net-(P3301-Pad33)")
  (net 632 "Net-(P3301-Pad34)")
  (net 633 "Net-(P3301-Pad35)")
  (net 634 "Net-(P3301-Pad36)")
  (net 635 NRESWARM-CPU)
  (net 636 "Net-(P3302-Pad1)")
  (net 637 "Net-(P3302-Pad2)")
  (net 638 "Net-(P3302-Pad3)")
  (net 639 "Net-(P3302-Pad8)")
  (net 640 "Net-(P3302-Pad9)")
  (net 641 "Net-(P3302-Pad12)")
  (net 642 "Net-(P3302-Pad13)")
  (net 643 "Net-(P3302-Pad14)")
  (net 644 "Net-(P3302-Pad15)")
  (net 645 "Net-(P3302-Pad16)")
  (net 646 "Net-(P3302-Pad17)")
  (net 647 "Net-(P3302-Pad18)")
  (net 648 "Net-(P3302-Pad19)")
  (net 649 "Net-(P3302-Pad20)")
  (net 650 "Net-(P3302-Pad21)")
  (net 651 "Net-(P3302-Pad22)")
  (net 652 "Net-(P3302-Pad23)")
  (net 653 "Net-(P3302-Pad24)")
  (net 654 "Net-(P3302-Pad25)")
  (net 655 "Net-(P3302-Pad26)")
  (net 656 "Net-(P3302-Pad27)")
  (net 657 "Net-(P3302-Pad28)")
  (net 658 "Net-(P3302-Pad29)")
  (net 659 "Net-(P3302-Pad30)")
  (net 660 "Net-(P3302-Pad31)")
  (net 661 "Net-(P3302-Pad32)")
  (net 662 "Net-(P3302-Pad33)")
  (net 663 "Net-(P3302-Pad34)")
  (net 664 "Net-(P3302-Pad35)")
  (net 665 "Net-(P3302-Pad36)")
  (net 666 "Net-(P3302-Pad37)")
  (net 667 "Net-(P3302-Pad38)")
  (net 668 "Net-(P3302-Pad39)")
  (net 669 "Net-(P3303-Pad1)")
  (net 670 "Net-(P3303-Pad2)")
  (net 671 "Net-(P3303-Pad3)")
  (net 672 "Net-(P3303-Pad4)")
  (net 673 "Net-(P3303-Pad5)")
  (net 674 "Net-(P3303-Pad6)")
  (net 675 "Net-(P3303-Pad7)")
  (net 676 "Net-(P3303-Pad8)")
  (net 677 "Net-(P3303-Pad9)")
  (net 678 "Net-(P3303-Pad10)")
  (net 679 "Net-(P3303-Pad11)")
  (net 680 "Net-(P3303-Pad12)")
  (net 681 "Net-(P3303-Pad13)")
  (net 682 "Net-(P3303-Pad14)")
  (net 683 "Net-(P3303-Pad15)")
  (net 684 "Net-(P3303-Pad16)")
  (net 685 "Net-(P3303-Pad17)")
  (net 686 "Net-(P3303-Pad18)")
  (net 687 "Net-(P3303-Pad19)")
  (net 688 "Net-(P3303-Pad20)")
  (net 689 "Net-(P3303-Pad21)")
  (net 690 "Net-(P3303-Pad23)")
  (net 691 "Net-(P3303-Pad24)")
  (net 692 "Net-(P3303-Pad25)")
  (net 693 "Net-(P3303-Pad26)")
  (net 694 "Net-(P3303-Pad27)")
  (net 695 "Net-(P3303-Pad28)")
  (net 696 "Net-(P3303-Pad29)")
  (net 697 "Net-(P3303-Pad30)")
  (net 698 "Net-(P3303-Pad31)")
  (net 699 "Net-(P3303-Pad32)")
  (net 700 "Net-(P3303-Pad33)")
  (net 701 "Net-(P3303-Pad34)")
  (net 702 "Net-(P3303-Pad35)")
  (net 703 VAUX4)
  (net 704 VAUX3)
  (net 705 "/BB-XM Adapter (DISP)/BB-DSS1")
  (net 706 "/BB-XM Adapter (DISP)/BB-DSS0")
  (net 707 "/BB-XM Adapter (DISP)/BB-DSS3")
  (net 708 "/BB-XM Adapter (DISP)/BB-DSS2")
  (net 709 "/BB-XM Adapter (DISP)/BB-DSS5")
  (net 710 "/BB-XM Adapter (DISP)/BB-DSS4")
  (net 711 "/BB-XM Adapter (DISP)/BB-DSS12")
  (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL")
  (net 713 "/BB-XM Adapter (DISP)/BB-DSS20")
  (net 714 "/BB-XM Adapter (DISP)/BB-DSS21")
  (net 715 "/BB-XM Adapter (DISP)/BB-DSS17")
  (net 716 "/BB-XM Adapter (DISP)/BB-DSS18")
  (net 717 "/BB-XM Adapter (DISP)/BB-DSS15")
  (net 718 "/BB-XM Adapter (DISP)/BB-DSS16")
  (net 719 "/BB-XM Adapter (DISP)/BB-DSS7")
  (net 720 "/BB-XM Adapter (CPU)/BB-159")
  (net 721 "/BB-XM Adapter (CPU)/BB-156")
  (net 722 "/BB-XM Adapter (CPU)/BB-139")
  (net 723 "/BB-XM Adapter (CPU)/BB-144")
  (net 724 "/BB-XM Adapter (CPU)/BB-138")
  (net 725 "/BB-XM Adapter (CPU)/BB-146")
  (net 726 "/BB-XM Adapter (CPU)/BB-137")
  (net 727 "/BB-XM Adapter (CPU)/BB-143")
  (net 728 "/BB-XM Adapter (CPU)/BB-136")
  (net 729 "/BB-XM Adapter (CPU)/BB-NRESWARM")
  (net 730 "/BB-XM Adapter (CPU)/BB-I2C2SCL")
  (net 731 "/BB-XM Adapter (CPU)/BB-I2C2SDA")
  (net 732 "Net-(P3402-Pad4)")
  (net 733 "Net-(P3402-Pad5)")
  (net 734 "/BB-XM Adapter (CPU)/BB-130")
  (net 735 "/BB-XM Adapter (CPU)/BB-131")
  (net 736 "/BB-XM Adapter (CPU)/BB-132")
  (net 737 "/BB-XM Adapter (CPU)/BB-133")
  (net 738 "/BB-XM Adapter (CPU)/BB-134")
  (net 739 "/BB-XM Adapter (CPU)/BB-135")
  (net 740 "Net-(P3402-Pad16)")
  (net 741 "/BB-XM Adapter (CPU)/BB-145")
  (net 742 "Net-(P3402-Pad21)")
  (net 743 "/BB-XM Adapter (CPU)/BB-157")
  (net 744 "/BB-XM Adapter (CPU)/BB-158")
  (net 745 "Net-(P3402-Pad26)")
  (net 746 "/BB-XM Adapter (CPU)/BB-161")
  (net 747 "/BB-XM Adapter (CPU)/BB-162")
  (net 748 BB-1V8)
  (net 749 "/BB-XM Adapter (DISP)/BB-DSS6")
  (net 750 "/BB-XM Adapter (DISP)/BB-DSS8")
  (net 751 "/BB-XM Adapter (DISP)/BB-DSS9")
  (net 752 "/BB-XM Adapter (DISP)/BB-DSS10")
  (net 753 "/BB-XM Adapter (DISP)/BB-DSS11")
  (net 754 "/BB-XM Adapter (DISP)/BB-DSS13")
  (net 755 "/BB-XM Adapter (DISP)/BB-DSS14")
  (net 756 "/BB-XM Adapter (DISP)/BB-DSS19")
  (net 757 "/BB-XM Adapter (DISP)/BB-DSS22")
  (net 758 "/BB-XM Adapter (DISP)/BB-DSS23")
  (net 759 "/BB-XM Adapter (DISP)/BB-DSSHS")
  (net 760 "/BB-XM Adapter (DISP)/BB-DSSVS")
  (net 761 "/BB-XM Adapter (DISP)/BB-DSSCK")
  (net 762 "/BB-XM Adapter (DISP)/BB-DSSDE")
  (net 763 "/BB-XM Adapter (DISP)/BB-I2C3SDA")
  (net 764 BB-3V3)
  (net 765 "Net-(P3601-Pad2)")
  (net 766 "Net-(P3601-Pad3)")
  (net 767 "Net-(P3601-Pad4)")
  (net 768 "Net-(P3601-Pad5)")
  (net 769 "Net-(P3601-Pad6)")
  (net 770 "Net-(P3601-Pad7)")
  (net 771 "Net-(P3601-Pad8)")
  (net 772 "Net-(P3601-Pad9)")
  (net 773 "Net-(P3601-Pad10)")
  (net 774 "Net-(P3601-Pad11)")
  (net 775 "Net-(P3601-Pad12)")
  (net 776 "Net-(P3601-Pad13)")
  (net 777 "Net-(P3601-Pad14)")
  (net 778 "Net-(P3601-Pad15)")
  (net 779 "Net-(P3601-Pad16)")
  (net 780 "Net-(P3601-Pad17)")
  (net 781 "Net-(P3601-Pad18)")
  (net 782 "Net-(P3601-Pad19)")
  (net 783 "Net-(P3601-Pad20)")
  (net 784 "Net-(P3601-Pad21)")
  (net 785 "Net-(P3601-Pad23)")
  (net 786 "Net-(P3601-Pad24)")
  (net 787 "Net-(P3601-Pad25)")
  (net 788 "Net-(P3601-Pad26)")
  (net 789 "Net-(P3601-Pad27)")
  (net 790 "Net-(P3601-Pad28)")
  (net 791 "Net-(P3601-Pad29)")
  (net 792 "Net-(P3601-Pad30)")
  (net 793 "Net-(P3601-Pad31)")
  (net 794 "Net-(P3601-Pad32)")
  (net 795 "Net-(P3601-Pad33)")
  (net 796 "Net-(P3601-Pad34)")
  (net 797 "Net-(P3601-Pad35)")
  (net 798 "Net-(P3601-Pad36)")
  (net 799 "Net-(P3601-Pad37)")
  (net 800 "Net-(PGM3709-PadP$1)")
  (net 801 "Net-(R301-Pad2)")
  (net 802 BATTEMP)
  (net 803 "/Modem Power/VMODEM")
  (net 804 HDQ)
  (net 805 BATTID)
  (net 806 GPIO$52)
  (net 807 "Net-(R806-Pad1)")
  (net 808 "Net-(R807-Pad1)")
  (net 809 "Net-(R901-Pad1)")
  (net 810 "Net-(R901-Pad2)")
  (net 811 "Net-(R902-Pad1)")
  (net 812 "Net-(R902-Pad2)")
  (net 813 "Net-(R903-Pad1)")
  (net 814 "Net-(R903-Pad2)")
  (net 815 "Net-(R905-Pad1)")
  (net 816 "Net-(R905-Pad2)")
  (net 817 "Net-(R906-Pad1)")
  (net 818 "Net-(R906-Pad2)")
  (net 819 "Net-(R1001-Pad1)")
  (net 820 "Net-(R1002-Pad1)")
  (net 821 ACCEL-INT)
  (net 822 DMIC-CLOCK)
  (net 823 "Net-(R1101-Pad2)")
  (net 824 "Net-(R1102-Pad1)")
  (net 825 "Net-(R1103-Pad1)")
  (net 826 "Net-(R1104-Pad1)")
  (net 827 "Net-(R1105-Pad1)")
  (net 828 "Net-(R1106-Pad1)")
  (net 829 "Net-(R1107-Pad1)")
  (net 830 "Net-(R1108-Pad1)")
  (net 831 "Net-(R1109-Pad1)")
  (net 832 "Net-(R1110-Pad1)")
  (net 833 "Net-(R1111-Pad1)")
  (net 834 GPIO177)
  (net 835 MIC-BIAS)
  (net 836 MIC-ECI)
  (net 837 "Net-(R1207-Pad2)")
  (net 838 "Net-(R1301-Pad1)")
  (net 839 /ECI/2V5)
  (net 840 "Net-(R1302-Pad1)")
  (net 841 "Net-(R1303-Pad1)")
  (net 842 GPIO-ECI1)
  (net 843 GPIO-ECI0)
  (net 844 "Net-(R1307-Pad2)")
  (net 845 ECI-ADC)
  (net 846 "/RFID/NFC Controller/SWP_1_S1")
  (net 847 SWIO-1)
  (net 848 "/RFID/NFC Controller/SWP_2_S1")
  (net 849 SWIO-2)
  (net 850 "Net-(R1902-Pad1)")
  (net 851 "Net-(R1902-Pad2)")
  (net 852 UART3-RX_IRRX)
  (net 853 "Net-(R1908-Pad2)")
  (net 854 "Net-(R2101-Pad1)")
  (net 855 "Net-(R2402-Pad2)")
  (net 856 "Net-(R2403-Pad2)")
  (net 857 PWM_UPPER)
  (net 858 "VBAT(->TPS65950)_UPPER")
  (net 859 "Net-(R3001-Pad1)")
  (net 860 "Net-(R3003-Pad1)")
  (net 861 "Net-(R3003-Pad2)")
  (net 862 "Net-(R3004-Pad1)")
  (net 863 "Net-(R3004-Pad2)")
  (net 864 "Net-(R3201-Pad2)")
  (net 865 "Net-(R3202-Pad2)")
  (net 866 "Net-(R3203-Pad2)")
  (net 867 "Net-(R3204-Pad2)")
  (net 868 VBUS-CPU)
  (net 869 OTG-CPU-D-)
  (net 870 OTG-CPU-D+)
  (net 871 "/BB-XM Adapter (CPU)/N$68")
  (net 872 GPIO$55)
  (net 873 GPIO$56)
  (net 874 I2C3-SDA)
  (net 875 I2C3-SCL)
  (net 876 GPIO56)
  (net 877 "Net-(S1002-Pad5)")
  (net 878 "Net-(S1002-Pad12)")
  (net 879 GPIN115)
  (net 880 "Net-(S1003-Pad3)")
  (net 881 GPIO$51)
  (net 882 "Net-(S1003-Pad5)")
  (net 883 "Net-(S1003-Pad12)")
  (net 884 "Net-(S1004-Pad4)")
  (net 885 "Net-(S1004-Pad17)")
  (net 886 "Net-(S1004-Pad26)")
  (net 887 "Net-(S1004-Pad27)")
  (net 888 GPIO-MODEM_EMERG)
  (net 889 BQ.GPIO)
  (net 890 /Hackerbus/UART3_CTS)
  (net 891 /Hackerbus/UART3_TX)
  (net 892 /Hackerbus/N$341)
  (net 893 /Hackerbus/N$340)
  (net 894 /Hackerbus/N$339)
  (net 895 /Hackerbus/UART3_RTS)
  (net 896 /Hackerbus/UART3_RX)
  (net 897 /Hackerbus/N$347)
  (net 898 /Hackerbus/N$349)
  (net 899 /Hackerbus/N$351)
  (net 900 "Net-(U201-Pad5)")
  (net 901 "Net-(U301-Pad7)")
  (net 902 "Net-(U301-Pad8)")
  (net 903 "Net-(U301-Pad9)")
  (net 904 "Net-(U301-Pad12)")
  (net 905 GPIO-EN-MODEM)
  (net 906 INA231-INT)
  (net 907 "Net-(U502-PadA1)")
  (net 908 "/Dual SIM switch/N$344")
  (net 909 "/Dual SIM switch/N$353")
  (net 910 "/Dual SIM switch/N$354")
  (net 911 "/Dual SIM switch/MODEM_RST_B")
  (net 912 "/Dual SIM switch/MODEM_CLK_B")
  (net 913 "/Dual SIM switch/MODEM_DATA_B")
  (net 914 "/Dual SIM switch/N$343")
  (net 915 "/Dual SIM switch/N$352")
  (net 916 "/Dual SIM switch/N$20")
  (net 917 "/Dual SIM switch/N$40")
  (net 918 "/Dual SIM switch/N$65")
  (net 919 "/Dual SIM switch/N$53")
  (net 920 "Net-(U702-Pad6)")
  (net 921 "Net-(U702-Pad7)")
  (net 922 "Net-(U702-Pad8)")
  (net 923 "Net-(U702-Pad9)")
  (net 924 "/Dual SIM switch/N$346")
  (net 925 "/Antenna connections/ANT-GNSS")
  (net 926 GPIO$70)
  (net 927 "Net-(U803-Pad2)")
  (net 928 "Net-(U803-Pad6)")
  (net 929 N$229)
  (net 930 "Net-(U804-Pad5)")
  (net 931 N$19)
  (net 932 "Net-(U805-Pad5)")
  (net 933 GPIO$110)
  (net 934 ADC$114)
  (net 935 NRESWARM)
  (net 936 "Net-(U902-Pad18)")
  (net 937 "Net-(U902-Pad19)")
  (net 938 "Net-(U1101-PadA1)")
  (net 939 "Net-(U1101-PadA5)")
  (net 940 "Net-(U1101-PadA6)")
  (net 941 EAR-)
  (net 942 EAR+)
  (net 943 "Net-(U1101-PadB1)")
  (net 944 DMIC-BIAS)
  (net 945 MICBIAS)
  (net 946 "Net-(U1101-PadC1)")
  (net 947 "Net-(U1101-PadC10)")
  (net 948 "Net-(U1101-PadC11)")
  (net 949 "Net-(U1101-PadD1)")
  (net 950 "Net-(U1101-PadE1)")
  (net 951 "Net-(U1101-PadE10)")
  (net 952 "Net-(U1101-PadF1)")
  (net 953 FM-R-OUT)
  (net 954 N$129)
  (net 955 "Net-(U1101-PadG10)")
  (net 956 "Net-(U1101-PadG11)")
  (net 957 "Net-(U1101-PadH1)")
  (net 958 DMIC-DATA)
  (net 959 FM-L-OUT)
  (net 960 "Net-(U1101-PadH11)")
  (net 961 "Net-(U1101-PadJ1)")
  (net 962 N$148)
  (net 963 N$153)
  (net 964 N$154)
  (net 965 N$149)
  (net 966 N$150)
  (net 967 "Net-(U1101-PadK8)")
  (net 968 "Net-(U1101-PadL1)")
  (net 969 "Net-(U1101-PadL2)")
  (net 970 "Net-(U1101-PadL3)")
  (net 971 "Net-(U1101-PadL4)")
  (net 972 "Net-(U1101-PadL5)")
  (net 973 "Net-(U1101-PadL7)")
  (net 974 "Net-(U1101-PadL8)")
  (net 975 "Net-(U1101-PadL11)")
  (net 976 GPIO-HP-EN)
  (net 977 GPIO$60)
  (net 978 "Net-(U1301-Pad4)")
  (net 979 GPIO-HF-EN)
  (net 980 NFC-ASKOOK)
  (net 981 NFC-IRQ)
  (net 982 NFC-TXD/MOD)
  (net 983 NFC-IO1)
  (net 984 NFC-TXEN)
  (net 985 NFC-SS)
  (net 986 NFC-TRXCLK)
  (net 987 NFC-MISO)
  (net 988 NFC-MOSI)
  (net 989 NFC-SCLK)
  (net 990 NFC-CLK)
  (net 991 NFC-EN)
  (net 992 OMAP_NFC_nRESET)
  (net 993 "Net-(U1701-Pad20)")
  (net 994 "Net-(U1701-Pad21)")
  (net 995 OMAP_NFC_INT)
  (net 996 SWP_nRESET)
  (net 997 "/RFID/NFC Controller/SELF")
  (net 998 "Net-(U1901-Pad4)")
  (net 999 "Net-(U1901-Pad5)")
  (net 1000 "Net-(U1901-Pad6)")
  (net 1001 "Net-(U1901-Pad7)")
  (net 1002 "Net-(U1901-Pad8)")
  (net 1003 "Net-(U1902G$1-Pad1)")
  (net 1004 "Net-(U1902G$1-Pad2)")
  (net 1005 "Net-(U1902G$1-Pad4)")
  (net 1006 "Net-(U1902G$1-Pad5)")
  (net 1007 "Net-(U1902G$1-Pad6)")
  (net 1008 "Net-(U2102-Pad1)")
  (net 1009 "Net-(U2301-Pad4)")
  (net 1010 RESET_UPPER)
  (net 1011 KEYIRQ_UPPER)
  (net 1012 PENIRQ_UPPER)
  (net 1013 "Net-(U2402-Pad3)")
  (net 1014 "Net-(U2402-Pad12)")
  (net 1015 "Net-(U2402-Pad13)")
  (net 1016 "Net-(U2402-Pad16)")
  (net 1017 "Net-(U2402-Pad18)")
  (net 1018 "Net-(U2402-Pad19)")
  (net 1019 "Net-(U2402-Pad20)")
  (net 1020 "Net-(U2402-Pad22)")
  (net 1021 "Net-(U2402-Pad28)")
  (net 1022 "Net-(U2402-Pad29)")
  (net 1023 "Net-(U2402-Pad30)")
  (net 1024 "Net-(U2402-Pad31)")
  (net 1025 "Net-(U2402-Pad32)")
  (net 1026 "Net-(U2502-PadA23)")
  (net 1027 "Net-(U2502-PadA24)")
  (net 1028 "Net-(U2502-PadA25)")
  (net 1029 "Net-(U2502-PadAA27)")
  (net 1030 "Net-(U2502-PadAA28)")
  (net 1031 "Net-(U2502-PadAE2)")
  (net 1032 "Net-(U2502-PadAE14)")
  (net 1033 "Net-(U2502-PadAE21)")
  (net 1034 "Net-(U2502-PadAF4)")
  (net 1035 "Net-(U2502-PadAF18)")
  (net 1036 "Net-(U2502-PadAF19)")
  (net 1037 "Net-(U2502-PadAF21)")
  (net 1038 "Net-(U2502-PadAF26)")
  (net 1039 "Net-(U2502-PadAG4)")
  (net 1040 "Net-(U2502-PadAG5)")
  (net 1041 "Net-(U2502-PadAG17)")
  (net 1042 "Net-(U2502-PadAG23)")
  (net 1043 "Net-(U2502-PadAG24)")
  (net 1044 "Net-(U2502-PadAG26)")
  (net 1045 "Net-(U2502-PadAH4)")
  (net 1046 "Net-(U2502-PadAH5)")
  (net 1047 "Net-(U2502-PadAH17)")
  (net 1048 "Net-(U2502-PadAH22)")
  (net 1049 "Net-(U2502-PadAH23)")
  (net 1050 "Net-(U2502-PadAH24)")
  (net 1051 "Net-(U2502-PadAH25)")
  (net 1052 "Net-(U2502-PadAH26)")
  (net 1053 /Camera/GPIO167)
  (net 1054 "Net-(U2502-PadB24)")
  (net 1055 "Net-(U2502-PadB25)")
  (net 1056 "Net-(U2502-PadB26)")
  (net 1057 "Net-(U2502-PadC23)")
  (net 1058 "Net-(U2502-PadC26)")
  (net 1059 "Net-(U2502-PadD24)")
  (net 1060 /Camera/CAM-STR)
  (net 1061 "Net-(U2502-PadD26)")
  (net 1062 "Net-(U2502-PadD27)")
  (net 1063 "Net-(U2502-PadD28)")
  (net 1064 "Net-(U2502-PadE26)")
  (net 1065 "Net-(U2502-PadE27)")
  (net 1066 "Net-(U2502-PadF27)")
  (net 1067 "Net-(U2502-PadF28)")
  (net 1068 "Net-(U2502-PadG25)")
  (net 1069 "Net-(U2502-PadG26)")
  (net 1070 "Net-(U2502-PadH26)")
  (net 1071 "Net-(U2502-PadH27)")
  (net 1072 "Net-(U2502-PadJ26)")
  (net 1073 "Net-(U2502-PadM27)")
  (net 1074 "Net-(U2502-PadN25)")
  (net 1075 "Net-(U2502-PadN26)")
  (net 1076 "Net-(U2502-PadN27)")
  (net 1077 "Net-(U2502-PadN28)")
  (net 1078 "Net-(U2502-PadP26)")
  (net 1079 "Net-(U2502-PadP27)")
  (net 1080 "Net-(U2502-PadP28)")
  (net 1081 "Net-(U2502-PadR25)")
  (net 1082 "Net-(U2502-PadR27)")
  (net 1083 "Net-(U2701-PadH3)")
  (net 1084 "Net-(U2701-PadH4)")
  (net 1085 "Net-(U2701-PadH5)")
  (net 1086 "Net-(U2701-PadJ2)")
  (net 1087 "Net-(U2701-PadJ3)")
  (net 1088 "Net-(U2701-PadJ4)")
  (net 1089 "Net-(U2701-PadJ5)")
  (net 1090 "Net-(U2701-PadJ6)")
  (net 1091 "Net-(U2701-PadK2)")
  (net 1092 "Net-(U2701-PadW5)")
  (net 1093 "Net-(U2701-PadW6)")
  (net 1094 "Net-(U2802-PadA1)")
  (net 1095 "Net-(U2802-PadA2)")
  (net 1096 "Net-(U2802-PadA3)")
  (net 1097 "Net-(U2802-PadA4)")
  (net 1098 "Net-(U2802-PadA5)")
  (net 1099 "Net-(U2802-PadB1)")
  (net 1100 "Net-(U2802-PadB2)")
  (net 1101 "Net-(U2802-PadB3)")
  (net 1102 "Net-(U2802-PadB4)")
  (net 1103 "Net-(U2802-PadB5)")
  (net 1104 "Net-(U2802-PadC1)")
  (net 1105 "Net-(U2802-PadC3)")
  (net 1106 "Net-(U2802-PadC4)")
  (net 1107 "Net-(U2802-PadC5)")
  (net 1108 "Net-(U2802-PadD2)")
  (net 1109 "Net-(U2802-PadD3)")
  (net 1110 "Net-(U2802-PadD4)")
  (net 1111 "Net-(U2802-PadD5)")
  (net 1112 "Net-(U2802-PadE2)")
  (net 1113 "Net-(U2802-PadE3)")
  (net 1114 "Net-(U2802-PadE4)")
  (net 1115 "Net-(U2802-PadE5)")
  (net 1116 "Net-(U2803-PadA2)")
  (net 1117 "Net-(U2803-PadA14)")
  (net 1118 "Net-(U2803-PadB14)")
  (net 1119 "Net-(U2803-PadC6)")
  (net 1120 "Net-(U2803-PadC8)")
  (net 1121 "Net-(U2803-PadD7)")
  (net 1122 "Net-(U2803-PadD13)")
  (net 1123 "Net-(U2803-PadF13)")
  (net 1124 "Net-(U2803-PadF14)")
  (net 1125 "Net-(U2803-PadF15)")
  (net 1126 "Net-(U2803-PadF16)")
  (net 1127 "Net-(U2803-PadG3)")
  (net 1128 "Net-(U2803-PadG10)")
  (net 1129 "Net-(U2803-PadG11)")
  (net 1130 "Net-(U2803-PadG13)")
  (net 1131 "Net-(U2803-PadG14)")
  (net 1132 "Net-(U2803-PadG15)")
  (net 1133 "Net-(U2803-PadH4)")
  (net 1134 "Net-(U2803-PadH8)")
  (net 1135 "Net-(U2803-PadJ3)")
  (net 1136 "Net-(U2803-PadJ9)")
  (net 1137 "Net-(U2803-PadJ13)")
  (net 1138 "Net-(U2803-PadJ14)")
  (net 1139 "Net-(U2803-PadK13)")
  (net 1140 "Net-(U2803-PadK14)")
  (net 1141 "Net-(U2803-PadL13)")
  (net 1142 "Net-(U2803-PadL14)")
  (net 1143 "Net-(U2803-PadL15)")
  (net 1144 "Net-(U2803-PadM13)")
  (net 1145 "Net-(U2803-PadN1)")
  (net 1146 "Net-(U2803-PadN2)")
  (net 1147 "Net-(U2803-PadN4)")
  (net 1148 "Net-(U2803-PadN5)")
  (net 1149 "Net-(U2803-PadN6)")
  (net 1150 "Net-(U2803-PadN7)")
  (net 1151 "Net-(U2803-PadN10)")
  (net 1152 "Net-(U2803-PadN15)")
  (net 1153 "Net-(U2803-PadN16)")
  (net 1154 "Net-(U2803-PadP1)")
  (net 1155 "Net-(U2803-PadP2)")
  (net 1156 "Net-(U2803-PadP4)")
  (net 1157 "Net-(U2803-PadP5)")
  (net 1158 "Net-(U2803-PadP6)")
  (net 1159 "Net-(U2803-PadP15)")
  (net 1160 "Net-(U2803-PadP16)")
  (net 1161 "Net-(U2803-PadR5)")
  (net 1162 OTG-CPU-ID)
  (net 1163 "Net-(U2803-PadR12)")
  (net 1164 "Net-(U2901-Pad4)")
  (net 1165 "Net-(U2902-Pad4)")
  (net 1166 GPIO-LED-EN_UPPER)
  (net 1167 32KHZ_UPPER)
  (net 1168 GPIO-RGB-INT_UPPER)
  (net 1169 "Net-(U3201-PadB4)")
  (net 1170 "Net-(U3201-PadD2)")
  (net 1171 "Net-(U3201-PadD4)")
  (net 1172 "Net-(U3201-PadF2)")
  (net 1173 "Net-(U3202-PadB4)")
  (net 1174 "Net-(U3202-PadD2)")
  (net 1175 "Net-(U3202-PadD4)")
  (net 1176 "Net-(U3202-PadF2)")
  (net 1177 VIB+)
  (net 1178 VIB-)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "/3G/4G Modem + SIM/ON_KEY")
    (add_net "/Antenna connections/ANT-GNSS")
    (add_net "/Audio Handsfree/SPKRR+")
    (add_net "/BB-XM Adapter (CPU)/BB-131")
    (add_net "/BB-XM Adapter (CPU)/BB-133")
    (add_net "/BB-XM Adapter (CPU)/BB-134")
    (add_net "/BB-XM Adapter (CPU)/BB-135")
    (add_net "/BB-XM Adapter (CPU)/BB-136")
    (add_net "/BB-XM Adapter (CPU)/BB-137")
    (add_net "/BB-XM Adapter (CPU)/BB-138")
    (add_net "/BB-XM Adapter (CPU)/BB-139")
    (add_net "/BB-XM Adapter (CPU)/BB-143")
    (add_net "/BB-XM Adapter (CPU)/BB-144")
    (add_net "/BB-XM Adapter (CPU)/BB-145")
    (add_net "/BB-XM Adapter (CPU)/BB-146")
    (add_net "/BB-XM Adapter (CPU)/BB-156")
    (add_net "/BB-XM Adapter (CPU)/BB-157")
    (add_net "/BB-XM Adapter (CPU)/BB-158")
    (add_net "/BB-XM Adapter (CPU)/BB-159")
    (add_net "/BB-XM Adapter (CPU)/BB-161")
    (add_net "/BB-XM Adapter (CPU)/BB-162")
    (add_net "/BB-XM Adapter (CPU)/BB-I2C2SCL")
    (add_net "/BB-XM Adapter (CPU)/BB-I2C2SDA")
    (add_net "/BB-XM Adapter (CPU)/BB-NRESWARM")
    (add_net "/BB-XM Adapter (CPU)/BB-VSYS")
    (add_net "/BB-XM Adapter (CPU)/N$68")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS0")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS1")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS10")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS11")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS12")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS13")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS14")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS15")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS16")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS17")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS18")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS19")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS2")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS20")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS21")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS22")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS23")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS3")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS4")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS5")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS6")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS7")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS8")
    (add_net "/BB-XM Adapter (DISP)/BB-DSS9")
    (add_net "/BB-XM Adapter (DISP)/BB-DSSCK")
    (add_net "/BB-XM Adapter (DISP)/BB-DSSDE")
    (add_net "/BB-XM Adapter (DISP)/BB-DSSHS")
    (add_net "/BB-XM Adapter (DISP)/BB-DSSVS")
    (add_net "/BB-XM Adapter (DISP)/BB-I2C3SCL")
    (add_net "/BB-XM Adapter (DISP)/BB-I2C3SDA")
    (add_net /Camera/CAM-STR)
    (add_net /Camera/CSI-B-C+_UPPER)
    (add_net /Camera/CSI-B-C-_UPPER)
    (add_net /Camera/CSI-B-D+_UPPER)
    (add_net /Camera/CSI-B-D-_UPPER)
    (add_net /Camera/GPIO102)
    (add_net /Camera/GPIO167)
    (add_net /Display-Panel&Power/CDP-CLK+_UPPER)
    (add_net /Display-Panel&Power/CDP-CLK-_UPPER)
    (add_net /Display-Panel&Power/CDP-D0+_UPPER)
    (add_net /Display-Panel&Power/CDP-D0-_UPPER)
    (add_net /Display-Panel&Power/CDP-D1+_UPPER)
    (add_net /Display-Panel&Power/CDP-D1-_UPPER)
    (add_net "/Dual SIM switch/MODEM_CLK_B")
    (add_net "/Dual SIM switch/MODEM_DATA_B")
    (add_net "/Dual SIM switch/MODEM_RST_B")
    (add_net "/Dual SIM switch/N$137")
    (add_net "/Dual SIM switch/N$20")
    (add_net "/Dual SIM switch/N$224")
    (add_net "/Dual SIM switch/N$338")
    (add_net "/Dual SIM switch/N$342")
    (add_net "/Dual SIM switch/N$343")
    (add_net "/Dual SIM switch/N$344")
    (add_net "/Dual SIM switch/N$346")
    (add_net "/Dual SIM switch/N$352")
    (add_net "/Dual SIM switch/N$353")
    (add_net "/Dual SIM switch/N$354")
    (add_net "/Dual SIM switch/N$40")
    (add_net "/Dual SIM switch/N$53")
    (add_net "/Dual SIM switch/N$65")
    (add_net /ECI/2V5)
    (add_net "/Fuel Gauge/BGND")
    (add_net /Hackerbus/N$339)
    (add_net /Hackerbus/N$340)
    (add_net /Hackerbus/N$341)
    (add_net /Hackerbus/N$347)
    (add_net /Hackerbus/N$349)
    (add_net /Hackerbus/N$351)
    (add_net /Hackerbus/UART3_CTS)
    (add_net /Hackerbus/UART3_RTS)
    (add_net /Hackerbus/UART3_RX)
    (add_net /Hackerbus/UART3_TX)
    (add_net "/Modem Power/VMODEM")
    (add_net "/RFID/NFC Controller/NFC_LED")
    (add_net "/RFID/NFC Controller/SELF")
    (add_net "/RFID/NFC Controller/SWP_1_S1")
    (add_net "/RFID/NFC Controller/SWP_2_S1")
    (add_net "/WLAN, Bluetooth, FM/ANT2")
    (add_net "/WLAN, Bluetooth, FM/BT-PCM-DR")
    (add_net "/WLAN, Bluetooth, FM/BT-PCM-DX")
    (add_net "/WLAN, Bluetooth, FM/LOOP")
    (add_net "/WLAN, Bluetooth, FM/N$13")
    (add_net "/WLAN, Bluetooth, FM/N$15")
    (add_net "/WLAN, Bluetooth, FM/N$312")
    (add_net "/WLAN, Bluetooth, FM/N$319")
    (add_net "/WLAN, Bluetooth, FM/N$36")
    (add_net "/WLAN, Bluetooth, FM/N$57")
    (add_net "/WLAN, Bluetooth, FM/N$59")
    (add_net "/WLAN, Bluetooth, FM/N$61")
    (add_net "/WLAN, Bluetooth, FM/N$62")
    (add_net "/WLAN, Bluetooth, FM/N$63")
    (add_net "/WLAN, Bluetooth, FM/N$82")
    (add_net "/WLAN, Bluetooth, FM/N$9")
    (add_net "/WLAN, Bluetooth, FM/N$97")
    (add_net "/uSD Breakout Board/LID")
    (add_net "/uSD Breakout Board/USD-3V3")
    (add_net "/uSD Breakout Board/USD-EN")
    (add_net "/uSD Breakout Board/USD-I2C2-SCL")
    (add_net "/uSD Breakout Board/USD-I2C2-SDA")
    (add_net "/uSD Breakout Board/USD-INT")
    (add_net "/uSD Breakout Board/USD-STR")
    (add_net "/uSD Breakout Board/USD-VBATT")
    (add_net 1V8)
    (add_net 1V8-CPU)
    (add_net 2V5_UPPER)
    (add_net 2V7)
    (add_net 2V8_UPPER)
    (add_net 32KHZ)
    (add_net 32KHZ_UPPER)
    (add_net 3G-WOE)
    (add_net 3V3)
    (add_net 3V3-CPU)
    (add_net ACCEL-INT)
    (add_net ADC$114)
    (add_net ADC1)
    (add_net ADC2)
    (add_net AGND)
    (add_net ANT-GNSS-DC)
    (add_net AUDIOIN)
    (add_net BATT)
    (add_net BATTEMP)
    (add_net BATTID)
    (add_net BB-1V8)
    (add_net BB-3V3)
    (add_net BB-5V)
    (add_net BQ.GPIO)
    (add_net BT-EN)
    (add_net CAM-CLK)
    (add_net CAM1-GPIO)
    (add_net CAM2-GPIO)
    (add_net CHG_IND)
    (add_net DMIC-BIAS)
    (add_net DMIC-CLOCK)
    (add_net DMIC-DATA)
    (add_net DMIC_BIAS)
    (add_net DMIC_CLOCK)
    (add_net DMIC_DATA)
    (add_net EAR+)
    (add_net EAR+_UPPER)
    (add_net EAR-)
    (add_net EAR-_UPPER)
    (add_net ECI-ADC)
    (add_net EMERG_OFF)
    (add_net FM-L-OUT)
    (add_net FM-R-OUT)
    (add_net FM-RX)
    (add_net GND)
    (add_net GND2)
    (add_net GND3)
    (add_net GND4)
    (add_net GNSS-IN)
    (add_net GPIN115)
    (add_net GPIO$110)
    (add_net GPIO$51)
    (add_net GPIO$52)
    (add_net GPIO$55)
    (add_net GPIO$56)
    (add_net GPIO$60)
    (add_net GPIO$70)
    (add_net GPIO-BATT-LID)
    (add_net GPIO-CAM-COVER)
    (add_net GPIO-ECI0)
    (add_net GPIO-ECI1)
    (add_net GPIO-EN-MODEM)
    (add_net GPIO-FLASH-EN)
    (add_net GPIO-FLASH-INT)
    (add_net GPIO-FLASH-STR)
    (add_net GPIO-HF-EN)
    (add_net GPIO-HP-EN)
    (add_net GPIO-LED-EN_UPPER)
    (add_net GPIO-MODEM_EMERG)
    (add_net GPIO-MODEM_IGT)
    (add_net GPIO-RGB-INT_UPPER)
    (add_net GPIO-VOL+)
    (add_net GPIO-VOL-)
    (add_net GPIO177)
    (add_net GPIO56)
    (add_net GPIO97)
    (add_net GSM-ANT-DRX)
    (add_net GSM-ANT-TRX)
    (add_net HDQ)
    (add_net HFL+)
    (add_net HFL-)
    (add_net HFR+)
    (add_net HFR-)
    (add_net HSL+)
    (add_net HSL-)
    (add_net HSR+)
    (add_net HSR-)
    (add_net I2C2-SCL)
    (add_net I2C2-SCL-CPU)
    (add_net I2C2-SDA)
    (add_net I2C2-SDA-CPU)
    (add_net I2C3-SCL)
    (add_net I2C3-SCL-CPU)
    (add_net I2C3-SDA)
    (add_net I2C3-SDA-CPU)
    (add_net INA231-INT)
    (add_net KEYIRQ_UPPER)
    (add_net LC_IND)
    (add_net LOCK-GPIO)
    (add_net MCBSP4-CLKX)
    (add_net MCBSP4-DR)
    (add_net MCBSP4-DX)
    (add_net MCBSP4-FSX)
    (add_net MIC+)
    (add_net MIC-)
    (add_net MIC-BIAS)
    (add_net MIC-ECI)
    (add_net MICBIAS)
    (add_net MODEM-CD_A)
    (add_net MODEM-CPU-D+)
    (add_net MODEM-CPU-D-)
    (add_net MODEM_CLK_A)
    (add_net MODEM_DATA_A)
    (add_net MODEM_RST_A)
    (add_net N$129)
    (add_net N$148)
    (add_net N$149)
    (add_net N$150)
    (add_net N$153)
    (add_net N$154)
    (add_net N$19)
    (add_net N$229)
    (add_net N$41_UPPER)
    (add_net N$49_UPPER)
    (add_net N$50_UPPER)
    (add_net NFC-ANT)
    (add_net NFC-ASKOOK)
    (add_net NFC-CLK)
    (add_net NFC-EN)
    (add_net NFC-IO1)
    (add_net NFC-IRQ)
    (add_net NFC-MISO)
    (add_net NFC-MOSI)
    (add_net NFC-SCLK)
    (add_net NFC-SS)
    (add_net NFC-TRXCLK)
    (add_net NFC-TXD/MOD)
    (add_net NFC-TXEN)
    (add_net NRESWARM)
    (add_net NRESWARM-CPU)
    (add_net "Net-(B1/CTL3709-PadP$1)")
    (add_net "Net-(B1/CTL3709-PadP$2)")
    (add_net "Net-(B10/OK3709-PadP$1)")
    (add_net "Net-(B10/OK3709-PadP$2)")
    (add_net "Net-(B11/ALT3709-PadP$2)")
    (add_net "Net-(B12/FN3709-PadP$1)")
    (add_net "Net-(B12/FN3709-PadP$2)")
    (add_net "Net-(B13/SPC2301-PadP$1)")
    (add_net "Net-(B13/SPC2301-PadP$2)")
    (add_net "Net-(B14/SPC2301-PadP$1)")
    (add_net "Net-(B15/M3709-PadP$1)")
    (add_net "Net-(B16/,3709-PadP$1)")
    (add_net "Net-(B17/PGDN3709-PadP$1)")
    (add_net "Net-(B18/END3709-PadP$1)")
    (add_net "Net-(B19/LEFT3709-PadP$1)")
    (add_net "Net-(B2/CTL2301-PadP$2)")
    (add_net "Net-(B21/DEL3709-PadP$2)")
    (add_net "Net-(B22/3709-PadP$2)")
    (add_net "Net-(B23/TAB3709-PadP$2)")
    (add_net "Net-(B31/ALT2301-PadP$2)")
    (add_net "Net-(B32/SHLCK3709-PadP$2)")
    (add_net "Net-(B33/ESC3709-PadP$2)")
    (add_net "Net-(B60/^2301-PadP$2)")
    (add_net "Net-(B69/O3709-PadP$2)")
    (add_net "Net-(B79/2301-PadP$2)")
    (add_net "Net-(BATT+3709-PadP)")
    (add_net "Net-(BATT-ID3709-PadP)")
    (add_net "Net-(C1011-Pad1)")
    (add_net "Net-(C1101-Pad1)")
    (add_net "Net-(C1101-Pad2)")
    (add_net "Net-(C1102-Pad1)")
    (add_net "Net-(C1104-Pad1)")
    (add_net "Net-(C1107-Pad1)")
    (add_net "Net-(C1201-Pad2)")
    (add_net "Net-(C1203-Pad1)")
    (add_net "Net-(C1203-Pad2)")
    (add_net "Net-(C1204-Pad2)")
    (add_net "Net-(C1205-Pad1)")
    (add_net "Net-(C1206-Pad2)")
    (add_net "Net-(C1207-Pad2)")
    (add_net "Net-(C1208-Pad1)")
    (add_net "Net-(C1209-Pad2)")
    (add_net "Net-(C1210-Pad1)")
    (add_net "Net-(C1212-Pad1)")
    (add_net "Net-(C1213-Pad2)")
    (add_net "Net-(C1214-Pad2)")
    (add_net "Net-(C1217-Pad1)")
    (add_net "Net-(C1404-Pad2)")
    (add_net "Net-(C1405-Pad2)")
    (add_net "Net-(C1406-Pad2)")
    (add_net "Net-(C1407-Pad2)")
    (add_net "Net-(C1408-Pad2)")
    (add_net "Net-(C1409-Pad2)")
    (add_net "Net-(C1410-Pad1)")
    (add_net "Net-(C1603-Pad2)")
    (add_net "Net-(C1605-Pad1)")
    (add_net "Net-(C1605-Pad2)")
    (add_net "Net-(C1607-Pad1)")
    (add_net "Net-(C1607-Pad2)")
    (add_net "Net-(C1610-Pad1)")
    (add_net "Net-(C1611-Pad2)")
    (add_net "Net-(C1614-Pad2)")
    (add_net "Net-(C1623-Pad1)")
    (add_net "Net-(C1625-Pad1)")
    (add_net "Net-(C1626-Pad1)")
    (add_net "Net-(C1627-Pad1)")
    (add_net "Net-(C1701-Pad1)")
    (add_net "Net-(C1901-Pad2)")
    (add_net "Net-(C1902-Pad1)")
    (add_net "Net-(C1903-Pad2)")
    (add_net "Net-(C1904-Pad2)")
    (add_net "Net-(C2103-Pad1)")
    (add_net "Net-(C2104-Pad1)")
    (add_net "Net-(C2105-Pad1)")
    (add_net "Net-(C2402-Pad1)")
    (add_net "Net-(C2404-Pad1)")
    (add_net "Net-(C2406-Pad1)")
    (add_net "Net-(C2407-Pad1)")
    (add_net "Net-(C2408-Pad1)")
    (add_net "Net-(C2409-Pad1)")
    (add_net "Net-(C2410-Pad1)")
    (add_net "Net-(C2502-Pad1)")
    (add_net "Net-(C2801-Pad1)")
    (add_net "Net-(C2802-Pad1)")
    (add_net "Net-(C3001-Pad1)")
    (add_net "Net-(C301-Pad1)")
    (add_net "Net-(C301-Pad2)")
    (add_net "Net-(C303-Pad2)")
    (add_net "Net-(C305-Pad1)")
    (add_net "Net-(C3101-Pad1)")
    (add_net "Net-(C3101-Pad2)")
    (add_net "Net-(C3102-Pad1)")
    (add_net "Net-(C3102-Pad2)")
    (add_net "Net-(C3103-Pad1)")
    (add_net "Net-(C3205-Pad2)")
    (add_net "Net-(C3206-Pad2)")
    (add_net "Net-(C3207-Pad2)")
    (add_net "Net-(C3208-Pad2)")
    (add_net "Net-(C401-Pad1)")
    (add_net "Net-(C402-Pad1)")
    (add_net "Net-(C403-Pad1)")
    (add_net "Net-(C404-Pad1)")
    (add_net "Net-(C405-Pad1)")
    (add_net "Net-(C406-Pad1)")
    (add_net "Net-(C502-Pad1)")
    (add_net "Net-(C503-Pad1)")
    (add_net "Net-(C504-Pad1)")
    (add_net "Net-(C505-Pad1)")
    (add_net "Net-(C506-Pad1)")
    (add_net "Net-(C508-Pad1)")
    (add_net "Net-(C601-Pad1)")
    (add_net "Net-(C611-Pad1)")
    (add_net "Net-(C802-Pad1)")
    (add_net "Net-(C802-Pad2)")
    (add_net "Net-(C803-Pad1)")
    (add_net "Net-(C803-Pad2)")
    (add_net "Net-(C808-Pad2)")
    (add_net "Net-(C809-Pad2)")
    (add_net "Net-(C901-Pad2)")
    (add_net "Net-(CD3709-PadP)")
    (add_net "Net-(D1201-Pad1)")
    (add_net "Net-(D1203-Pad2)")
    (add_net "Net-(D1204-Pad2)")
    (add_net "Net-(D1205-Pad2)")
    (add_net "Net-(D1902-PadA)")
    (add_net "Net-(D1902-PadK)")
    (add_net "Net-(D2102-PadA)")
    (add_net "Net-(D2501-PadA)")
    (add_net "Net-(D2502-PadA)")
    (add_net "Net-(D3201-PadA)")
    (add_net "Net-(D3201-PadK)")
    (add_net "Net-(D3202-PadA)")
    (add_net "Net-(D3202-PadK)")
    (add_net "Net-(DCD3709-PadP)")
    (add_net "Net-(DSR3709-PadP)")
    (add_net "Net-(DTR3709-PadP)")
    (add_net "Net-(GPS-ANT3709-Pad1)")
    (add_net "Net-(HS-1201-PadP)")
    (add_net "Net-(HS-1204-PadP)")
    (add_net "Net-(HS-1206-PadP)")
    (add_net "Net-(L1401-Pad2)")
    (add_net "Net-(L1402-Pad2)")
    (add_net "Net-(L1403-Pad2)")
    (add_net "Net-(L1404-Pad2)")
    (add_net "Net-(L2502-Pad3)")
    (add_net "Net-(L2502-Pad4)")
    (add_net "Net-(L2503-Pad3)")
    (add_net "Net-(L2503-Pad4)")
    (add_net "Net-(L2504-Pad3)")
    (add_net "Net-(L2504-Pad4)")
    (add_net "Net-(L801-Pad1)")
    (add_net "Net-(L801-Pad2)")
    (add_net "Net-(L901-Pad1)")
    (add_net "Net-(L901-Pad2)")
    (add_net "Net-(LED2101-Pad1)")
    (add_net "Net-(LED2102-PadK)")
    (add_net "Net-(LED2103-Pad1)")
    (add_net "Net-(LED3101-Pad1)")
    (add_net "Net-(LED3101-Pad2)")
    (add_net "Net-(LED3101-Pad3)")
    (add_net "Net-(LED3102-Pad1)")
    (add_net "Net-(LED3102-Pad2)")
    (add_net "Net-(LED3102-Pad3)")
    (add_net "Net-(LED3201-Pad1)")
    (add_net "Net-(LED3201-Pad2)")
    (add_net "Net-(LED3201-Pad3)")
    (add_net "Net-(LED3202-Pad1)")
    (add_net "Net-(LED3202-Pad2)")
    (add_net "Net-(LED3202-Pad3)")
    (add_net "Net-(LED3203-Pad1)")
    (add_net "Net-(LED3203-Pad2)")
    (add_net "Net-(LED3203-Pad3)")
    (add_net "Net-(LED3204-Pad1)")
    (add_net "Net-(LED3204-Pad2)")
    (add_net "Net-(LED3204-Pad3)")
    (add_net "Net-(LED3205-Pad1)")
    (add_net "Net-(LED3205-Pad2)")
    (add_net "Net-(LED3205-Pad3)")
    (add_net "Net-(LED3206-Pad4)")
    (add_net "Net-(LED3206-Pad5)")
    (add_net "Net-(LED3206-Pad6)")
    (add_net "Net-(LED3207-PadK)")
    (add_net "Net-(LED3208-Pad1)")
    (add_net "Net-(LED3208-Pad2)")
    (add_net "Net-(LED3208-Pad3)")
    (add_net "Net-(LED3209-PadK)")
    (add_net "Net-(M601-PadC14)")
    (add_net "Net-(M601-PadD15)")
    (add_net "Net-(M601-PadD16)")
    (add_net "Net-(M601-PadE15)")
    (add_net "Net-(M601-PadE16)")
    (add_net "Net-(M601-PadM5)")
    (add_net "Net-(M601-PadN6)")
    (add_net "Net-(M601-PadN7)")
    (add_net "Net-(M601-PadP6)")
    (add_net "Net-(M601-PadP7)")
    (add_net "Net-(M901-Pad2)")
    (add_net "Net-(M901-Pad25)")
    (add_net "Net-(M901-Pad26)")
    (add_net "Net-(M901-Pad27)")
    (add_net "Net-(M901-Pad3)")
    (add_net "Net-(M901-Pad4)")
    (add_net "Net-(M901-Pad42)")
    (add_net "Net-(M901-Pad43)")
    (add_net "Net-(M901-Pad5)")
    (add_net "Net-(P-DISP3709-Pad10)")
    (add_net "Net-(P-DISP3709-Pad29)")
    (add_net "Net-(P-DISP3709-Pad30)")
    (add_net "Net-(P-DISP3709-Pad34)")
    (add_net "Net-(P-DISP3709-Pad35)")
    (add_net "Net-(P-DISP3709-Pad36)")
    (add_net "Net-(P-DISP3709-Pad37)")
    (add_net "Net-(P-DISP3709-Pad38)")
    (add_net "Net-(P-DISP3709-Pad61)")
    (add_net "Net-(P-DISP3709-Pad62)")
    (add_net "Net-(P-DISP3709-Pad63)")
    (add_net "Net-(P-DISP3709-Pad8)")
    (add_net "Net-(P-INT801-PadSIG)")
    (add_net "Net-(P-MICRO-SD3709-Pad1)")
    (add_net "Net-(P-MICRO-SD3709-Pad2)")
    (add_net "Net-(P-MICRO-SD3709-Pad3)")
    (add_net "Net-(P-MICRO-SD3709-Pad5)")
    (add_net "Net-(P-MICRO-SD3709-Pad7)")
    (add_net "Net-(P-MICRO-SD3709-Pad8)")
    (add_net "Net-(P-MODEM3709-OTG2-Pad4/ID)")
    (add_net "Net-(P-SIM701-PadC1)")
    (add_net "Net-(P2001-Pad10)")
    (add_net "Net-(P2001-Pad11)")
    (add_net "Net-(P2001-Pad12)")
    (add_net "Net-(P2001-Pad13)")
    (add_net "Net-(P2001-Pad14)")
    (add_net "Net-(P2001-Pad15)")
    (add_net "Net-(P2001-Pad16)")
    (add_net "Net-(P2001-Pad17)")
    (add_net "Net-(P2001-Pad18)")
    (add_net "Net-(P2001-Pad19)")
    (add_net "Net-(P2001-Pad20)")
    (add_net "Net-(P2001-Pad21)")
    (add_net "Net-(P2001-Pad22)")
    (add_net "Net-(P2001-Pad23)")
    (add_net "Net-(P2001-Pad24)")
    (add_net "Net-(P2001-Pad25)")
    (add_net "Net-(P2001-Pad26)")
    (add_net "Net-(P2001-Pad27)")
    (add_net "Net-(P2001-Pad28)")
    (add_net "Net-(P2001-Pad3)")
    (add_net "Net-(P2001-Pad33)")
    (add_net "Net-(P2001-Pad34)")
    (add_net "Net-(P2001-Pad35)")
    (add_net "Net-(P2001-Pad36)")
    (add_net "Net-(P2001-Pad37)")
    (add_net "Net-(P2001-Pad38)")
    (add_net "Net-(P2001-Pad39)")
    (add_net "Net-(P2001-Pad4)")
    (add_net "Net-(P2001-Pad40)")
    (add_net "Net-(P2001-Pad41)")
    (add_net "Net-(P2001-Pad42)")
    (add_net "Net-(P2001-Pad43)")
    (add_net "Net-(P2001-Pad44)")
    (add_net "Net-(P2001-Pad45)")
    (add_net "Net-(P2001-Pad46)")
    (add_net "Net-(P2001-Pad47)")
    (add_net "Net-(P2001-Pad48)")
    (add_net "Net-(P2001-Pad49)")
    (add_net "Net-(P2001-Pad5)")
    (add_net "Net-(P2001-Pad50)")
    (add_net "Net-(P2001-Pad51)")
    (add_net "Net-(P2001-Pad52)")
    (add_net "Net-(P2001-Pad53)")
    (add_net "Net-(P2001-Pad54)")
    (add_net "Net-(P2001-Pad55)")
    (add_net "Net-(P2001-Pad56)")
    (add_net "Net-(P2001-Pad57)")
    (add_net "Net-(P2001-Pad58)")
    (add_net "Net-(P2001-Pad6)")
    (add_net "Net-(P2001-Pad7)")
    (add_net "Net-(P2001-Pad8)")
    (add_net "Net-(P2001-Pad9)")
    (add_net "Net-(P2002-Pad10)")
    (add_net "Net-(P2002-Pad11)")
    (add_net "Net-(P2002-Pad12)")
    (add_net "Net-(P2002-Pad13)")
    (add_net "Net-(P2002-Pad14)")
    (add_net "Net-(P2002-Pad15)")
    (add_net "Net-(P2002-Pad16)")
    (add_net "Net-(P2002-Pad17)")
    (add_net "Net-(P2002-Pad18)")
    (add_net "Net-(P2002-Pad19)")
    (add_net "Net-(P2002-Pad20)")
    (add_net "Net-(P2002-Pad21)")
    (add_net "Net-(P2002-Pad22)")
    (add_net "Net-(P2002-Pad23)")
    (add_net "Net-(P2002-Pad24)")
    (add_net "Net-(P2002-Pad25)")
    (add_net "Net-(P2002-Pad26)")
    (add_net "Net-(P2002-Pad27)")
    (add_net "Net-(P2002-Pad28)")
    (add_net "Net-(P2002-Pad3)")
    (add_net "Net-(P2002-Pad33)")
    (add_net "Net-(P2002-Pad34)")
    (add_net "Net-(P2002-Pad35)")
    (add_net "Net-(P2002-Pad36)")
    (add_net "Net-(P2002-Pad37)")
    (add_net "Net-(P2002-Pad38)")
    (add_net "Net-(P2002-Pad39)")
    (add_net "Net-(P2002-Pad4)")
    (add_net "Net-(P2002-Pad40)")
    (add_net "Net-(P2002-Pad41)")
    (add_net "Net-(P2002-Pad42)")
    (add_net "Net-(P2002-Pad43)")
    (add_net "Net-(P2002-Pad44)")
    (add_net "Net-(P2002-Pad45)")
    (add_net "Net-(P2002-Pad46)")
    (add_net "Net-(P2002-Pad47)")
    (add_net "Net-(P2002-Pad48)")
    (add_net "Net-(P2002-Pad49)")
    (add_net "Net-(P2002-Pad5)")
    (add_net "Net-(P2002-Pad50)")
    (add_net "Net-(P2002-Pad51)")
    (add_net "Net-(P2002-Pad52)")
    (add_net "Net-(P2002-Pad53)")
    (add_net "Net-(P2002-Pad54)")
    (add_net "Net-(P2002-Pad55)")
    (add_net "Net-(P2002-Pad56)")
    (add_net "Net-(P2002-Pad57)")
    (add_net "Net-(P2002-Pad58)")
    (add_net "Net-(P2002-Pad6)")
    (add_net "Net-(P2002-Pad7)")
    (add_net "Net-(P2002-Pad8)")
    (add_net "Net-(P2002-Pad9)")
    (add_net "Net-(P2101-Pad13)")
    (add_net "Net-(P2201-Pad10)")
    (add_net "Net-(P2201-Pad11)")
    (add_net "Net-(P2201-Pad12)")
    (add_net "Net-(P2201-Pad13)")
    (add_net "Net-(P2201-Pad14)")
    (add_net "Net-(P2201-Pad15)")
    (add_net "Net-(P2201-Pad16)")
    (add_net "Net-(P2201-Pad17)")
    (add_net "Net-(P2201-Pad18)")
    (add_net "Net-(P2201-Pad19)")
    (add_net "Net-(P2201-Pad20)")
    (add_net "Net-(P2201-Pad21)")
    (add_net "Net-(P2201-Pad22)")
    (add_net "Net-(P2201-Pad23)")
    (add_net "Net-(P2201-Pad24)")
    (add_net "Net-(P2201-Pad25)")
    (add_net "Net-(P2201-Pad26)")
    (add_net "Net-(P2201-Pad27)")
    (add_net "Net-(P2201-Pad28)")
    (add_net "Net-(P2201-Pad3)")
    (add_net "Net-(P2201-Pad33)")
    (add_net "Net-(P2201-Pad34)")
    (add_net "Net-(P2201-Pad35)")
    (add_net "Net-(P2201-Pad36)")
    (add_net "Net-(P2201-Pad37)")
    (add_net "Net-(P2201-Pad38)")
    (add_net "Net-(P2201-Pad39)")
    (add_net "Net-(P2201-Pad4)")
    (add_net "Net-(P2201-Pad40)")
    (add_net "Net-(P2201-Pad41)")
    (add_net "Net-(P2201-Pad42)")
    (add_net "Net-(P2201-Pad43)")
    (add_net "Net-(P2201-Pad44)")
    (add_net "Net-(P2201-Pad45)")
    (add_net "Net-(P2201-Pad46)")
    (add_net "Net-(P2201-Pad47)")
    (add_net "Net-(P2201-Pad48)")
    (add_net "Net-(P2201-Pad49)")
    (add_net "Net-(P2201-Pad5)")
    (add_net "Net-(P2201-Pad50)")
    (add_net "Net-(P2201-Pad51)")
    (add_net "Net-(P2201-Pad52)")
    (add_net "Net-(P2201-Pad53)")
    (add_net "Net-(P2201-Pad54)")
    (add_net "Net-(P2201-Pad55)")
    (add_net "Net-(P2201-Pad56)")
    (add_net "Net-(P2201-Pad57)")
    (add_net "Net-(P2201-Pad58)")
    (add_net "Net-(P2201-Pad6)")
    (add_net "Net-(P2201-Pad7)")
    (add_net "Net-(P2201-Pad8)")
    (add_net "Net-(P2201-Pad9)")
    (add_net "Net-(P2202-Pad10)")
    (add_net "Net-(P2202-Pad11)")
    (add_net "Net-(P2202-Pad12)")
    (add_net "Net-(P2202-Pad13)")
    (add_net "Net-(P2202-Pad14)")
    (add_net "Net-(P2202-Pad15)")
    (add_net "Net-(P2202-Pad16)")
    (add_net "Net-(P2202-Pad17)")
    (add_net "Net-(P2202-Pad18)")
    (add_net "Net-(P2202-Pad19)")
    (add_net "Net-(P2202-Pad20)")
    (add_net "Net-(P2202-Pad21)")
    (add_net "Net-(P2202-Pad22)")
    (add_net "Net-(P2202-Pad23)")
    (add_net "Net-(P2202-Pad24)")
    (add_net "Net-(P2202-Pad25)")
    (add_net "Net-(P2202-Pad26)")
    (add_net "Net-(P2202-Pad27)")
    (add_net "Net-(P2202-Pad28)")
    (add_net "Net-(P2202-Pad3)")
    (add_net "Net-(P2202-Pad30)")
    (add_net "Net-(P2202-Pad33)")
    (add_net "Net-(P2202-Pad34)")
    (add_net "Net-(P2202-Pad35)")
    (add_net "Net-(P2202-Pad36)")
    (add_net "Net-(P2202-Pad37)")
    (add_net "Net-(P2202-Pad38)")
    (add_net "Net-(P2202-Pad39)")
    (add_net "Net-(P2202-Pad4)")
    (add_net "Net-(P2202-Pad40)")
    (add_net "Net-(P2202-Pad41)")
    (add_net "Net-(P2202-Pad42)")
    (add_net "Net-(P2202-Pad43)")
    (add_net "Net-(P2202-Pad44)")
    (add_net "Net-(P2202-Pad45)")
    (add_net "Net-(P2202-Pad46)")
    (add_net "Net-(P2202-Pad47)")
    (add_net "Net-(P2202-Pad48)")
    (add_net "Net-(P2202-Pad49)")
    (add_net "Net-(P2202-Pad5)")
    (add_net "Net-(P2202-Pad50)")
    (add_net "Net-(P2202-Pad51)")
    (add_net "Net-(P2202-Pad52)")
    (add_net "Net-(P2202-Pad53)")
    (add_net "Net-(P2202-Pad54)")
    (add_net "Net-(P2202-Pad55)")
    (add_net "Net-(P2202-Pad56)")
    (add_net "Net-(P2202-Pad57)")
    (add_net "Net-(P2202-Pad58)")
    (add_net "Net-(P2202-Pad6)")
    (add_net "Net-(P2202-Pad7)")
    (add_net "Net-(P2202-Pad8)")
    (add_net "Net-(P2202-Pad9)")
    (add_net "Net-(P3001-Pad1)")
    (add_net "Net-(P3001-Pad10)")
    (add_net "Net-(P3001-Pad6)")
    (add_net "Net-(P3001-Pad7)")
    (add_net "Net-(P3001-Pad9)")
    (add_net "Net-(P3301-Pad11)")
    (add_net "Net-(P3301-Pad12)")
    (add_net "Net-(P3301-Pad13)")
    (add_net "Net-(P3301-Pad14)")
    (add_net "Net-(P3301-Pad15)")
    (add_net "Net-(P3301-Pad16)")
    (add_net "Net-(P3301-Pad17)")
    (add_net "Net-(P3301-Pad18)")
    (add_net "Net-(P3301-Pad19)")
    (add_net "Net-(P3301-Pad20)")
    (add_net "Net-(P3301-Pad21)")
    (add_net "Net-(P3301-Pad22)")
    (add_net "Net-(P3301-Pad23)")
    (add_net "Net-(P3301-Pad24)")
    (add_net "Net-(P3301-Pad25)")
    (add_net "Net-(P3301-Pad26)")
    (add_net "Net-(P3301-Pad27)")
    (add_net "Net-(P3301-Pad28)")
    (add_net "Net-(P3301-Pad29)")
    (add_net "Net-(P3301-Pad30)")
    (add_net "Net-(P3301-Pad31)")
    (add_net "Net-(P3301-Pad32)")
    (add_net "Net-(P3301-Pad33)")
    (add_net "Net-(P3301-Pad34)")
    (add_net "Net-(P3301-Pad35)")
    (add_net "Net-(P3301-Pad36)")
    (add_net "Net-(P3301-Pad5)")
    (add_net "Net-(P3301-Pad6)")
    (add_net "Net-(P3302-Pad1)")
    (add_net "Net-(P3302-Pad12)")
    (add_net "Net-(P3302-Pad13)")
    (add_net "Net-(P3302-Pad14)")
    (add_net "Net-(P3302-Pad15)")
    (add_net "Net-(P3302-Pad16)")
    (add_net "Net-(P3302-Pad17)")
    (add_net "Net-(P3302-Pad18)")
    (add_net "Net-(P3302-Pad19)")
    (add_net "Net-(P3302-Pad2)")
    (add_net "Net-(P3302-Pad20)")
    (add_net "Net-(P3302-Pad21)")
    (add_net "Net-(P3302-Pad22)")
    (add_net "Net-(P3302-Pad23)")
    (add_net "Net-(P3302-Pad24)")
    (add_net "Net-(P3302-Pad25)")
    (add_net "Net-(P3302-Pad26)")
    (add_net "Net-(P3302-Pad27)")
    (add_net "Net-(P3302-Pad28)")
    (add_net "Net-(P3302-Pad29)")
    (add_net "Net-(P3302-Pad3)")
    (add_net "Net-(P3302-Pad30)")
    (add_net "Net-(P3302-Pad31)")
    (add_net "Net-(P3302-Pad32)")
    (add_net "Net-(P3302-Pad33)")
    (add_net "Net-(P3302-Pad34)")
    (add_net "Net-(P3302-Pad35)")
    (add_net "Net-(P3302-Pad36)")
    (add_net "Net-(P3302-Pad37)")
    (add_net "Net-(P3302-Pad38)")
    (add_net "Net-(P3302-Pad39)")
    (add_net "Net-(P3302-Pad8)")
    (add_net "Net-(P3302-Pad9)")
    (add_net "Net-(P3303-Pad1)")
    (add_net "Net-(P3303-Pad10)")
    (add_net "Net-(P3303-Pad11)")
    (add_net "Net-(P3303-Pad12)")
    (add_net "Net-(P3303-Pad13)")
    (add_net "Net-(P3303-Pad14)")
    (add_net "Net-(P3303-Pad15)")
    (add_net "Net-(P3303-Pad16)")
    (add_net "Net-(P3303-Pad17)")
    (add_net "Net-(P3303-Pad18)")
    (add_net "Net-(P3303-Pad19)")
    (add_net "Net-(P3303-Pad2)")
    (add_net "Net-(P3303-Pad20)")
    (add_net "Net-(P3303-Pad21)")
    (add_net "Net-(P3303-Pad23)")
    (add_net "Net-(P3303-Pad24)")
    (add_net "Net-(P3303-Pad25)")
    (add_net "Net-(P3303-Pad26)")
    (add_net "Net-(P3303-Pad27)")
    (add_net "Net-(P3303-Pad28)")
    (add_net "Net-(P3303-Pad29)")
    (add_net "Net-(P3303-Pad3)")
    (add_net "Net-(P3303-Pad30)")
    (add_net "Net-(P3303-Pad31)")
    (add_net "Net-(P3303-Pad32)")
    (add_net "Net-(P3303-Pad33)")
    (add_net "Net-(P3303-Pad34)")
    (add_net "Net-(P3303-Pad35)")
    (add_net "Net-(P3303-Pad4)")
    (add_net "Net-(P3303-Pad5)")
    (add_net "Net-(P3303-Pad6)")
    (add_net "Net-(P3303-Pad7)")
    (add_net "Net-(P3303-Pad8)")
    (add_net "Net-(P3303-Pad9)")
    (add_net "Net-(P3402-Pad16)")
    (add_net "Net-(P3402-Pad21)")
    (add_net "Net-(P3402-Pad26)")
    (add_net "Net-(P3402-Pad4)")
    (add_net "Net-(P3402-Pad5)")
    (add_net "Net-(P3601-Pad10)")
    (add_net "Net-(P3601-Pad11)")
    (add_net "Net-(P3601-Pad12)")
    (add_net "Net-(P3601-Pad13)")
    (add_net "Net-(P3601-Pad14)")
    (add_net "Net-(P3601-Pad15)")
    (add_net "Net-(P3601-Pad16)")
    (add_net "Net-(P3601-Pad17)")
    (add_net "Net-(P3601-Pad18)")
    (add_net "Net-(P3601-Pad19)")
    (add_net "Net-(P3601-Pad2)")
    (add_net "Net-(P3601-Pad20)")
    (add_net "Net-(P3601-Pad21)")
    (add_net "Net-(P3601-Pad23)")
    (add_net "Net-(P3601-Pad24)")
    (add_net "Net-(P3601-Pad25)")
    (add_net "Net-(P3601-Pad26)")
    (add_net "Net-(P3601-Pad27)")
    (add_net "Net-(P3601-Pad28)")
    (add_net "Net-(P3601-Pad29)")
    (add_net "Net-(P3601-Pad3)")
    (add_net "Net-(P3601-Pad30)")
    (add_net "Net-(P3601-Pad31)")
    (add_net "Net-(P3601-Pad32)")
    (add_net "Net-(P3601-Pad33)")
    (add_net "Net-(P3601-Pad34)")
    (add_net "Net-(P3601-Pad35)")
    (add_net "Net-(P3601-Pad36)")
    (add_net "Net-(P3601-Pad37)")
    (add_net "Net-(P3601-Pad4)")
    (add_net "Net-(P3601-Pad5)")
    (add_net "Net-(P3601-Pad6)")
    (add_net "Net-(P3601-Pad7)")
    (add_net "Net-(P3601-Pad8)")
    (add_net "Net-(P3601-Pad9)")
    (add_net "Net-(PGM3709-PadP$1)")
    (add_net "Net-(R1001-Pad1)")
    (add_net "Net-(R1002-Pad1)")
    (add_net "Net-(R1101-Pad2)")
    (add_net "Net-(R1102-Pad1)")
    (add_net "Net-(R1103-Pad1)")
    (add_net "Net-(R1104-Pad1)")
    (add_net "Net-(R1105-Pad1)")
    (add_net "Net-(R1106-Pad1)")
    (add_net "Net-(R1107-Pad1)")
    (add_net "Net-(R1108-Pad1)")
    (add_net "Net-(R1109-Pad1)")
    (add_net "Net-(R1110-Pad1)")
    (add_net "Net-(R1111-Pad1)")
    (add_net "Net-(R1207-Pad2)")
    (add_net "Net-(R1301-Pad1)")
    (add_net "Net-(R1302-Pad1)")
    (add_net "Net-(R1303-Pad1)")
    (add_net "Net-(R1307-Pad2)")
    (add_net "Net-(R1902-Pad1)")
    (add_net "Net-(R1902-Pad2)")
    (add_net "Net-(R1908-Pad2)")
    (add_net "Net-(R2101-Pad1)")
    (add_net "Net-(R2402-Pad2)")
    (add_net "Net-(R2403-Pad2)")
    (add_net "Net-(R3001-Pad1)")
    (add_net "Net-(R3003-Pad1)")
    (add_net "Net-(R3003-Pad2)")
    (add_net "Net-(R3004-Pad1)")
    (add_net "Net-(R3004-Pad2)")
    (add_net "Net-(R301-Pad2)")
    (add_net "Net-(R3201-Pad2)")
    (add_net "Net-(R3202-Pad2)")
    (add_net "Net-(R3203-Pad2)")
    (add_net "Net-(R3204-Pad2)")
    (add_net "Net-(R806-Pad1)")
    (add_net "Net-(R807-Pad1)")
    (add_net "Net-(R901-Pad1)")
    (add_net "Net-(R901-Pad2)")
    (add_net "Net-(R902-Pad1)")
    (add_net "Net-(R902-Pad2)")
    (add_net "Net-(R903-Pad1)")
    (add_net "Net-(R903-Pad2)")
    (add_net "Net-(R905-Pad1)")
    (add_net "Net-(R905-Pad2)")
    (add_net "Net-(R906-Pad1)")
    (add_net "Net-(R906-Pad2)")
    (add_net "Net-(S1002-Pad12)")
    (add_net "Net-(S1002-Pad5)")
    (add_net "Net-(S1003-Pad12)")
    (add_net "Net-(S1003-Pad3)")
    (add_net "Net-(S1003-Pad5)")
    (add_net "Net-(S1004-Pad17)")
    (add_net "Net-(S1004-Pad26)")
    (add_net "Net-(S1004-Pad27)")
    (add_net "Net-(S1004-Pad4)")
    (add_net "Net-(U1101-PadA1)")
    (add_net "Net-(U1101-PadA5)")
    (add_net "Net-(U1101-PadA6)")
    (add_net "Net-(U1101-PadB1)")
    (add_net "Net-(U1101-PadC1)")
    (add_net "Net-(U1101-PadC10)")
    (add_net "Net-(U1101-PadC11)")
    (add_net "Net-(U1101-PadD1)")
    (add_net "Net-(U1101-PadE1)")
    (add_net "Net-(U1101-PadE10)")
    (add_net "Net-(U1101-PadF1)")
    (add_net "Net-(U1101-PadG10)")
    (add_net "Net-(U1101-PadG11)")
    (add_net "Net-(U1101-PadH1)")
    (add_net "Net-(U1101-PadH11)")
    (add_net "Net-(U1101-PadJ1)")
    (add_net "Net-(U1101-PadK8)")
    (add_net "Net-(U1101-PadL1)")
    (add_net "Net-(U1101-PadL11)")
    (add_net "Net-(U1101-PadL2)")
    (add_net "Net-(U1101-PadL3)")
    (add_net "Net-(U1101-PadL4)")
    (add_net "Net-(U1101-PadL5)")
    (add_net "Net-(U1101-PadL7)")
    (add_net "Net-(U1101-PadL8)")
    (add_net "Net-(U1301-Pad4)")
    (add_net "Net-(U1701-Pad20)")
    (add_net "Net-(U1701-Pad21)")
    (add_net "Net-(U1901-Pad4)")
    (add_net "Net-(U1901-Pad5)")
    (add_net "Net-(U1901-Pad6)")
    (add_net "Net-(U1901-Pad7)")
    (add_net "Net-(U1901-Pad8)")
    (add_net "Net-(U1902G$1-Pad1)")
    (add_net "Net-(U1902G$1-Pad2)")
    (add_net "Net-(U1902G$1-Pad4)")
    (add_net "Net-(U1902G$1-Pad5)")
    (add_net "Net-(U1902G$1-Pad6)")
    (add_net "Net-(U201-Pad5)")
    (add_net "Net-(U2102-Pad1)")
    (add_net "Net-(U2301-Pad4)")
    (add_net "Net-(U2402-Pad12)")
    (add_net "Net-(U2402-Pad13)")
    (add_net "Net-(U2402-Pad16)")
    (add_net "Net-(U2402-Pad18)")
    (add_net "Net-(U2402-Pad19)")
    (add_net "Net-(U2402-Pad20)")
    (add_net "Net-(U2402-Pad22)")
    (add_net "Net-(U2402-Pad28)")
    (add_net "Net-(U2402-Pad29)")
    (add_net "Net-(U2402-Pad3)")
    (add_net "Net-(U2402-Pad30)")
    (add_net "Net-(U2402-Pad31)")
    (add_net "Net-(U2402-Pad32)")
    (add_net "Net-(U2502-PadA23)")
    (add_net "Net-(U2502-PadA24)")
    (add_net "Net-(U2502-PadA25)")
    (add_net "Net-(U2502-PadAA27)")
    (add_net "Net-(U2502-PadAA28)")
    (add_net "Net-(U2502-PadAE14)")
    (add_net "Net-(U2502-PadAE2)")
    (add_net "Net-(U2502-PadAE21)")
    (add_net "Net-(U2502-PadAF18)")
    (add_net "Net-(U2502-PadAF19)")
    (add_net "Net-(U2502-PadAF21)")
    (add_net "Net-(U2502-PadAF26)")
    (add_net "Net-(U2502-PadAF4)")
    (add_net "Net-(U2502-PadAG17)")
    (add_net "Net-(U2502-PadAG23)")
    (add_net "Net-(U2502-PadAG24)")
    (add_net "Net-(U2502-PadAG26)")
    (add_net "Net-(U2502-PadAG4)")
    (add_net "Net-(U2502-PadAG5)")
    (add_net "Net-(U2502-PadAH17)")
    (add_net "Net-(U2502-PadAH22)")
    (add_net "Net-(U2502-PadAH23)")
    (add_net "Net-(U2502-PadAH24)")
    (add_net "Net-(U2502-PadAH25)")
    (add_net "Net-(U2502-PadAH26)")
    (add_net "Net-(U2502-PadAH4)")
    (add_net "Net-(U2502-PadAH5)")
    (add_net "Net-(U2502-PadB24)")
    (add_net "Net-(U2502-PadB25)")
    (add_net "Net-(U2502-PadB26)")
    (add_net "Net-(U2502-PadC23)")
    (add_net "Net-(U2502-PadC26)")
    (add_net "Net-(U2502-PadD24)")
    (add_net "Net-(U2502-PadD26)")
    (add_net "Net-(U2502-PadD27)")
    (add_net "Net-(U2502-PadD28)")
    (add_net "Net-(U2502-PadE26)")
    (add_net "Net-(U2502-PadE27)")
    (add_net "Net-(U2502-PadF27)")
    (add_net "Net-(U2502-PadF28)")
    (add_net "Net-(U2502-PadG25)")
    (add_net "Net-(U2502-PadG26)")
    (add_net "Net-(U2502-PadH26)")
    (add_net "Net-(U2502-PadH27)")
    (add_net "Net-(U2502-PadJ26)")
    (add_net "Net-(U2502-PadM27)")
    (add_net "Net-(U2502-PadN25)")
    (add_net "Net-(U2502-PadN26)")
    (add_net "Net-(U2502-PadN27)")
    (add_net "Net-(U2502-PadN28)")
    (add_net "Net-(U2502-PadP26)")
    (add_net "Net-(U2502-PadP27)")
    (add_net "Net-(U2502-PadP28)")
    (add_net "Net-(U2502-PadR25)")
    (add_net "Net-(U2502-PadR27)")
    (add_net "Net-(U2701-PadH3)")
    (add_net "Net-(U2701-PadH4)")
    (add_net "Net-(U2701-PadH5)")
    (add_net "Net-(U2701-PadJ2)")
    (add_net "Net-(U2701-PadJ3)")
    (add_net "Net-(U2701-PadJ4)")
    (add_net "Net-(U2701-PadJ5)")
    (add_net "Net-(U2701-PadJ6)")
    (add_net "Net-(U2701-PadK2)")
    (add_net "Net-(U2701-PadW5)")
    (add_net "Net-(U2701-PadW6)")
    (add_net "Net-(U2802-PadA1)")
    (add_net "Net-(U2802-PadA2)")
    (add_net "Net-(U2802-PadA3)")
    (add_net "Net-(U2802-PadA4)")
    (add_net "Net-(U2802-PadA5)")
    (add_net "Net-(U2802-PadB1)")
    (add_net "Net-(U2802-PadB2)")
    (add_net "Net-(U2802-PadB3)")
    (add_net "Net-(U2802-PadB4)")
    (add_net "Net-(U2802-PadB5)")
    (add_net "Net-(U2802-PadC1)")
    (add_net "Net-(U2802-PadC3)")
    (add_net "Net-(U2802-PadC4)")
    (add_net "Net-(U2802-PadC5)")
    (add_net "Net-(U2802-PadD2)")
    (add_net "Net-(U2802-PadD3)")
    (add_net "Net-(U2802-PadD4)")
    (add_net "Net-(U2802-PadD5)")
    (add_net "Net-(U2802-PadE2)")
    (add_net "Net-(U2802-PadE3)")
    (add_net "Net-(U2802-PadE4)")
    (add_net "Net-(U2802-PadE5)")
    (add_net "Net-(U2803-PadA14)")
    (add_net "Net-(U2803-PadA2)")
    (add_net "Net-(U2803-PadB14)")
    (add_net "Net-(U2803-PadC6)")
    (add_net "Net-(U2803-PadC8)")
    (add_net "Net-(U2803-PadD13)")
    (add_net "Net-(U2803-PadD7)")
    (add_net "Net-(U2803-PadF13)")
    (add_net "Net-(U2803-PadF14)")
    (add_net "Net-(U2803-PadF15)")
    (add_net "Net-(U2803-PadF16)")
    (add_net "Net-(U2803-PadG10)")
    (add_net "Net-(U2803-PadG11)")
    (add_net "Net-(U2803-PadG13)")
    (add_net "Net-(U2803-PadG14)")
    (add_net "Net-(U2803-PadG15)")
    (add_net "Net-(U2803-PadG3)")
    (add_net "Net-(U2803-PadH4)")
    (add_net "Net-(U2803-PadH8)")
    (add_net "Net-(U2803-PadJ13)")
    (add_net "Net-(U2803-PadJ14)")
    (add_net "Net-(U2803-PadJ3)")
    (add_net "Net-(U2803-PadJ9)")
    (add_net "Net-(U2803-PadK13)")
    (add_net "Net-(U2803-PadK14)")
    (add_net "Net-(U2803-PadL13)")
    (add_net "Net-(U2803-PadL14)")
    (add_net "Net-(U2803-PadL15)")
    (add_net "Net-(U2803-PadM13)")
    (add_net "Net-(U2803-PadN1)")
    (add_net "Net-(U2803-PadN10)")
    (add_net "Net-(U2803-PadN15)")
    (add_net "Net-(U2803-PadN16)")
    (add_net "Net-(U2803-PadN2)")
    (add_net "Net-(U2803-PadN4)")
    (add_net "Net-(U2803-PadN5)")
    (add_net "Net-(U2803-PadN6)")
    (add_net "Net-(U2803-PadN7)")
    (add_net "Net-(U2803-PadP1)")
    (add_net "Net-(U2803-PadP15)")
    (add_net "Net-(U2803-PadP16)")
    (add_net "Net-(U2803-PadP2)")
    (add_net "Net-(U2803-PadP4)")
    (add_net "Net-(U2803-PadP5)")
    (add_net "Net-(U2803-PadP6)")
    (add_net "Net-(U2803-PadR12)")
    (add_net "Net-(U2803-PadR5)")
    (add_net "Net-(U2901-Pad4)")
    (add_net "Net-(U2902-Pad4)")
    (add_net "Net-(U301-Pad12)")
    (add_net "Net-(U301-Pad7)")
    (add_net "Net-(U301-Pad8)")
    (add_net "Net-(U301-Pad9)")
    (add_net "Net-(U3201-PadB4)")
    (add_net "Net-(U3201-PadD2)")
    (add_net "Net-(U3201-PadD4)")
    (add_net "Net-(U3201-PadF2)")
    (add_net "Net-(U3202-PadB4)")
    (add_net "Net-(U3202-PadD2)")
    (add_net "Net-(U3202-PadD4)")
    (add_net "Net-(U3202-PadF2)")
    (add_net "Net-(U502-PadA1)")
    (add_net "Net-(U702-Pad6)")
    (add_net "Net-(U702-Pad7)")
    (add_net "Net-(U702-Pad8)")
    (add_net "Net-(U702-Pad9)")
    (add_net "Net-(U803-Pad2)")
    (add_net "Net-(U803-Pad6)")
    (add_net "Net-(U804-Pad5)")
    (add_net "Net-(U805-Pad5)")
    (add_net "Net-(U902-Pad18)")
    (add_net "Net-(U902-Pad19)")
    (add_net OMAP_NFC_INT)
    (add_net OMAP_NFC_nRESET)
    (add_net OTG-CPU-D+)
    (add_net OTG-CPU-D-)
    (add_net OTG-CPU-ID)
    (add_net OTG-D+)
    (add_net OTG-D-)
    (add_net OTG-ID)
    (add_net PENIRQ_UPPER)
    (add_net POWERON)
    (add_net PWM_UPPER)
    (add_net PWR_IND)
    (add_net RESET_UPPER)
    (add_net RING)
    (add_net SD-CD)
    (add_net SD-CLK)
    (add_net SD-CMD)
    (add_net SD-DAT0)
    (add_net SD-DAT1)
    (add_net SD-DAT2)
    (add_net SD-DAT3)
    (add_net SD-VDD)
    (add_net SIM-CLK)
    (add_net SIM-DATA)
    (add_net SIM-RST)
    (add_net STATUS)
    (add_net SWIO-1)
    (add_net SWIO-2)
    (add_net SWP_nRESET)
    (add_net UART3-CTS_RCTX)
    (add_net UART3-RX_IRRX)
    (add_net UART3-TX_IRTX)
    (add_net UART?-CTS)
    (add_net UART?-RTS)
    (add_net UART?-RX)
    (add_net UART?-TX)
    (add_net USB-WWAN-D+)
    (add_net USB-WWAN-D-)
    (add_net VAUX3)
    (add_net VAUX4)
    (add_net VAUX??)
    (add_net "VBAT(->TPS65950)_UPPER")
    (add_net VBATT)
    (add_net VBATT_UPPER)
    (add_net VBUS)
    (add_net VBUS-CPU)
    (add_net VBUS-MODEM)
    (add_net VBUS-MODEM-CPU)
    (add_net VCSI=VAUX2???)
    (add_net VDDA)
    (add_net VGNSS)
    (add_net VIB+)
    (add_net VIB-)
    (add_net VMMC2)
    (add_net VMMC2-CPU)
    (add_net VMODEM1)
    (add_net VMODEM2)
    (add_net VMODEM3)
    (add_net VSYS)
    (add_net VSYS_UPPER)
    (add_net WLAN-EN)
    (add_net WLAN-IRQ)
  )
  (net_class bla ""
    (clearance 0.5)
    (trace_width 0.8)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "/BB-XM Adapter (CPU)/BB-130")
    (add_net "/BB-XM Adapter (CPU)/BB-132")
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B1/CTL3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(B1/CTL3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(B1/CTL3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B2/CTL2301 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(B12/FN3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(B2/CTL2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B3/\3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(B13/SPC2301-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B10/OK3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B4/A3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(B14/SPC2301-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B10/OK3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B5/Q3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(B15/M3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B10/OK3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B6/2301 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(B16/,3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B10/OK3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B7/3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(B17/PGDN3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B10/OK3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B8/3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(B18/END3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B10/OK3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B9/SPC2301 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(B19/LEFT3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B10/OK3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B10/OK3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(B10/OK3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B10/OK3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B11/ALT3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(B1/CTL3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(B11/ALT3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B12/FN3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(B12/FN3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(B12/FN3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B13/SPC2301 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(B13/SPC2301-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B13/SPC2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B14/SPC2301 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(B14/SPC2301-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B13/SPC2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B15/M3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(B15/M3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B13/SPC2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B16/,3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(B16/,3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B13/SPC2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B17/PGDN3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(B17/PGDN3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B13/SPC2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B18/END3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(B18/END3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B13/SPC2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B19/LEFT3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(B19/LEFT3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B13/SPC2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B20/RGHT3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(B10/OK3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B13/SPC2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B21/DEL3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(B1/CTL3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(B21/DEL3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B22/3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(B12/FN3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(B22/3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B23/TAB3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(B13/SPC2301-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B23/TAB3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B24/BSP3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(B14/SPC2301-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B23/TAB3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B25/RET3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(B15/M3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B23/TAB3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B26/PIPE3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(B16/,3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B23/TAB3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B27/PGUP3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(B17/PGDN3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B23/TAB3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B28/HOME3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(B18/END3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B23/TAB3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B29/UP3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(B19/LEFT3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B23/TAB3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B30/DN3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(B10/OK3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B23/TAB3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B31/ALT2301 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(B1/CTL3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(B31/ALT2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B32/SHLCK3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(B12/FN3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(B32/SHLCK3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B33/ESC3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTONMAEANDER (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(B13/SPC2301-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(B33/ESC3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B60/^2301 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTON-N900 (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(B19/LEFT3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(B60/^2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B60/^3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTON-N900 (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(B10/OK3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(B60/^2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B69/O3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTON-N900 (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(B19/LEFT3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(B69/O3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B70/P3709 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTON-N900 (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(B10/OK3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(B69/O3709-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B79/2301 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTON-N900 (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(B19/LEFT3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(B79/2301-PadP$2)"))
  )
  (module neo900-legacy:N900-BUTTON (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (tags "N900 DOME SHEET COMPATIBLE PRINTED BUTTON CONTACT")
    (attr smd)
    (fp_text reference B80/2301 (at 2.91338 -3.00482) (layer B.SilkS))
    (fp_text value BUTTON-N900 (at 1.1684 3.00482) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 13.13434 -0.3048) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0 60) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(B10/OK3709-PadP$1)"))
    (pad P$2 smd oval (at -2.70002 0 90) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(B79/2301-PadP$2)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference BATT+3709 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(BATT+3709-PadP)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference BATT-GND3709 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 27 "/Fuel Gauge/BGND"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference BATT-ID3709 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(BATT-ID3709-PadP)"))
  )
  (module neo900-legacy:1PIN-HOLE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr virtual)
    (fp_text reference BGND3709 (at 0 0) (layer F.SilkS))
    (fp_text value - (at 0 0) (layer F.SilkS))
    (pad P$1 thru_hole oval (at 0 0 90) (size 2.99974 5.99948) (drill 1.99898) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 27 "/Fuel Gauge/BGND"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C201 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2.2u;10V (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 29 VBUS))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C301 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 47n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C301-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C301-Pad2)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C302 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 4u7;10V (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 29 VBUS))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C303 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 8.2u;10V (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C303-Pad2)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C304 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 10u (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C305 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 4u7 (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C305-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C401 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C401-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C402 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C402-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C403 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C403-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C404 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C404-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C405 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C405-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C406 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C406-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C501 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 10u (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 42 BATT))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C502 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C502-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C503 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C503-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C504 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C504-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C505 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C505-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C506 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C506-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C508 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 1µ (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C508-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C510 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 10u (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(BATT+3709-PadP)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0805 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0805 BASED ON VISHAY PACKAGE")
    (tags "SMD 0805 BASED ON VISHAY PACKAGE")
    (attr smd)
    (fp_text reference C601 (at -0.28194 -0.37592) (layer F.SilkS))
    (fp_text value 47u (at -0.07874 0.16002) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 0) (size 0.79756 1.29794) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C601-Pad1)"))
    (pad 2 smd rect (at 0.99822 0) (size 0.79756 1.29794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C602 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 50 VMODEM3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C603 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 39p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 50 VMODEM3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0805 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0805 BASED ON VISHAY PACKAGE")
    (tags "SMD 0805 BASED ON VISHAY PACKAGE")
    (attr smd)
    (fp_text reference C604 (at -0.28194 -0.37592) (layer F.SilkS))
    (fp_text value 47u (at -0.07874 0.16002) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 0) (size 0.79756 1.29794) (layers F.Cu F.Paste F.Mask)
      (net 50 VMODEM3))
    (pad 2 smd rect (at 0.99822 0) (size 0.79756 1.29794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C605 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 51 VMODEM1))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C606 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 39p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 51 VMODEM1))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0805 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0805 BASED ON VISHAY PACKAGE")
    (tags "SMD 0805 BASED ON VISHAY PACKAGE")
    (attr smd)
    (fp_text reference C607 (at -0.28194 -0.37592) (layer F.SilkS))
    (fp_text value 47u (at -0.07874 0.16002) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 0) (size 0.79756 1.29794) (layers F.Cu F.Paste F.Mask)
      (net 51 VMODEM1))
    (pad 2 smd rect (at 0.99822 0) (size 0.79756 1.29794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C608 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 52 VMODEM2))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C609 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 39p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 52 VMODEM2))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0805 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0805 BASED ON VISHAY PACKAGE")
    (tags "SMD 0805 BASED ON VISHAY PACKAGE")
    (attr smd)
    (fp_text reference C610 (at -0.28194 -0.37592) (layer F.SilkS))
    (fp_text value 47u (at -0.07874 0.16002) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 0) (size 0.79756 1.29794) (layers F.Cu F.Paste F.Mask)
      (net 52 VMODEM2))
    (pad 2 smd rect (at 0.99822 0) (size 0.79756 1.29794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C611 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 220n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C611-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C612 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 54 SIM-RST))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C801 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 55 VGNSS))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C802 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value DNP (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C802-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C802-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C803 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 33p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C803-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C803-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C804 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 60 ADC1))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C805 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 15p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 61 2V7))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C806 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 61 2V7))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C807 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 62 ADC2))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C808 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 60 ADC1))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C808-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C809 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 62 ADC2))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C809-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C810 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 15p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 61 2V7))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C811 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C812 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C901 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 66 FM-RX))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C901-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C902 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C903 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1001 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1002 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C1003 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 10u (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1004 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1005 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C1006 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 10u (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1007 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1008 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1009 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 6n8 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1010 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 120n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1011 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(C1011-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1012 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1101 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 3n3 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C1101-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C1101-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1102 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C1102-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1103 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C1102-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1104 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C1104-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1105 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C1104-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1106 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 3n3 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 74 HSL+))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 75 HSL-))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1107 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C1107-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1108 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C1107-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1109 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 3n3 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 77 HSR+))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 78 HSR-))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1110 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 3n3 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 79 HFL+))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 80 HFL-))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1111 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 3n3 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 81 HFR+))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 82 HFR-))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1201 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1u (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(C1201-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1202 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1u (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(C1201-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1203 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1u (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(C1203-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(C1203-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1204 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 470n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 74 HSL+))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(C1204-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1205 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 22p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C1205-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 66 FM-RX))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1206 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 470n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 75 HSL-))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(C1206-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1207 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 470n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 77 HSR+))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C1207-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1208 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 22p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(C1208-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 66 FM-RX))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1209 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 470n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 78 HSR-))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(C1209-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1210 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1u (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(C1210-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1211 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 94 VMMC2))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1212 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(C1212-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1213 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 33n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 96 MIC+))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(C1213-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1214 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 33n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 98 MIC-))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(C1214-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1215 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(C1213-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1216 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(C1214-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1217 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(C1217-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C1401 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 10u (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1402 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1403 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 27p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1404 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(C1404-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1405 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(C1405-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1406 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 79 HFL+))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(C1406-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1407 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 80 HFL-))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(C1407-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1408 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 81 HFR+))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(C1408-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1409 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 82 HFR-))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(C1409-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1410 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(C1410-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1411 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 108 "/Audio Handsfree/SPKRR+"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1601 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1602 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1603 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(C1603-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1604 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(C1603-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1605 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C1605-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(C1605-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1606 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 47p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(C1605-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 112 NFC-ANT))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1607 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n5 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(C1607-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(C1607-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1608 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(C1605-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 112 NFC-ANT))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1609 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n5 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(C1607-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(C1607-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1610 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(C1610-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1611 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C1605-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(C1611-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1612 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 680p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C1605-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1613 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value DNP (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C1605-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1614 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 220p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(C1605-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(C1614-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1615 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(C1605-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1616 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 27p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(C1605-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1617 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value DNP (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 112 NFC-ANT))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1618 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(C1610-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1619 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1620 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(C1611-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1621 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 680p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(C1614-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1622 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1623 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(C1623-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1624 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(C1623-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1625 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 27p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(C1625-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1626 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 27p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(C1626-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1627 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(C1627-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1628 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(C1627-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1701 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value "(47pF)" (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(C1701-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1702 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1703 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1u (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1901 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 123 AUDIOIN))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(C1901-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1902 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(C1902-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1903 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 126 UART3-TX_IRTX))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(C1903-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C1904 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 128 UART3-CTS_RCTX))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(C1904-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C2101 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1u (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 130 "/uSD Breakout Board/USD-3V3"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C2102 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 47n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 130 "/uSD Breakout Board/USD-3V3"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C2103 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(C2103-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C2104 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value "4u7; 12V" (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(C2104-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C2105 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 10u (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(C2105-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C2301 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 100nF (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C2401 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 4u7 (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C2402 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(C2402-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C2403 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 27p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 138 DMIC_CLOCK))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C2404 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(C2404-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C2405 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 27p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 138 DMIC_CLOCK))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C2406 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 1n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(C2406-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C2407 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 1n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(C2407-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C2408 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 1n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C2408-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C2409 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 1n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(C2409-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C2410 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C2410-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C2411 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100nF (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C2410-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:MK325 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TAIYO YUDEN *MK325 (1210)")
    (tags "TAIYO YUDEN *MK325 (1210)")
    (attr smd)
    (fp_text reference C2501 (at -0.78232 -1.17602) (layer F.SilkS))
    (fp_text value 4u7 (at -0.57912 -0.63754) (layer F.SilkS))
    (pad 1 smd rect (at -1.4986 0) (size 0.99822 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
    (pad 2 smd rect (at 1.4986 0) (size 0.99822 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:MK325 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TAIYO YUDEN *MK325 (1210)")
    (tags "TAIYO YUDEN *MK325 (1210)")
    (attr smd)
    (fp_text reference C2502 (at -0.78232 -1.17602) (layer F.SilkS))
    (fp_text value 4.7u;50V;TMK325B7475MG (at -0.57912 -0.63754) (layer F.SilkS))
    (pad 1 smd rect (at -1.4986 0) (size 0.99822 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C2502-Pad1)"))
    (pad 2 smd rect (at 1.4986 0) (size 0.99822 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-1206 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "BASED ON VISHAY DIMENSIONS")
    (tags "BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C2801 (at -0.68326 -0.47752) (layer F.SilkS))
    (fp_text value tbd (at -0.48006 -0.00254) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.25mm" (at 7.88924 -1.63322) (layer F.SilkS))
    (pad 1 smd rect (at -1.4478 0) (size 0.89916 1.59766) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(C2801-Pad1)"))
    (pad 2 smd rect (at 1.4478 0) (size 0.89916 1.59766) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-1210 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "BASED ON VISHAY DIMENSIONS")
    (tags "BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C2802 (at -0.68326 -0.9779) (layer F.SilkS))
    (fp_text value PAS3225P3R3113 (at -0.48006 -0.40132) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.25mm" (at 6.98754 -1.93294) (layer F.SilkS))
    (pad 1 smd rect (at -1.4478 0) (size 0.89916 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(C2802-Pad1)"))
    (pad 2 smd rect (at 1.4478 0) (size 0.89916 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3001 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 27p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(C3001-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3002 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(C3001-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3003 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 27p (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3004 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3005 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3006 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 150 VCSI=VAUX2???))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3007 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 151 VDDA))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3101 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 470n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(C3101-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(C3101-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3102 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 470n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(C3102-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(C3102-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3103 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1u (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(C3103-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3201 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3202 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3203 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2u2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3204 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3205 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1u (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(C3205-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3206 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1u (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(C3206-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3207 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(C3207-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference C3208 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(C3208-Pad2)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C3401 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 1u (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 162 BB-5V))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference C3402 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 1u (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 164 "/BB-XM Adapter (CPU)/BB-VSYS"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference CD3709 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(CD3709-PadP)"))
  )
  (module neo900-legacy:TP-0.75 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT")
    (tags "TEST POINT")
    (attr smd)
    (fp_text reference CTS3709 (at 0 0) (layer F.SilkS))
    (fp_text value CTS (at 1.33096 0) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 9.32434 -1.13284) (layer B.SilkS))
    (pad P smd circle (at 0 0) (size 0.7493 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 166 UART?-RTS))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference D+3709 (at 0 0) (layer F.SilkS))
    (fp_text value WUSB+ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 167 USB-WWAN-D+))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference D-3709 (at 0 0) (layer F.SilkS))
    (fp_text value WUSB- (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 168 USB-WWAN-D-))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D201 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 169 LOCK-GPIO))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D202 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 170 GPIO-VOL+))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D203 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 171 GPIO-VOL-))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D204 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 172 POWERON))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D205 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 173 CAM1-GPIO))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D206 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 174 CAM2-GPIO))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D501 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(BATT+3709-PadP)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D502 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(BATT-ID3709-PadP)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D901 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 175 "/WLAN, Bluetooth, FM/LOOP"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D1201 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(D1201-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D1202 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(C1217-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D1203 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(D1203-Pad2)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D1204 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(D1204-Pad2)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D1205 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(D1205-Pad2)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D1401 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(C1405-Pad2)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D1402 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(C1404-Pad2)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D1403 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(C1410-Pad1)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D1404 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 108 "/Audio Handsfree/SPKRR+"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference D1701 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value LTST-C190KRKT (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 180 "/RFID/NFC Controller/NFC_LED"))
  )
  (module neo900-legacy:VSMB2948SL (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "VISHAY IR LED")
    (tags "VISHAY IR LED")
    (attr smd)
    (fp_text reference D1901 (at 0.1143 -1.00076) (layer F.SilkS))
    (fp_text value VEMD10940F (at -0.23622 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 2.3mm" (at 6.35254 -2.43332) (layer B.SilkS))
    (pad A smd rect (at 1.64846 0) (size 0.89916 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(C1901-Pad2)"))
    (pad K smd rect (at -1.64846 0) (size 0.89916 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
  )
  (module neo900-legacy:VSMB2948SL (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "VISHAY IR LED")
    (tags "VISHAY IR LED")
    (attr smd)
    (fp_text reference D1902 (at 0.1143 -1.00076) (layer F.SilkS))
    (fp_text value VSMB2948SL (at -0.23622 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 2.3mm" (at 6.35254 -2.43332) (layer B.SilkS))
    (pad A smd rect (at 1.64846 0) (size 0.89916 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(D1902-PadA)"))
    (pad K smd rect (at -1.64846 0) (size 0.89916 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(D1902-PadK)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference D2101 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value V5.5MLA0603N (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(CD3709-PadP)"))
  )
  (module neo900-legacy:CRS02 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PACKAGE FOR TOSHIBA CRS02")
    (tags "PACKAGE FOR TOSHIBA CRS02")
    (attr smd)
    (fp_text reference D2102 (at -0.18288 -0.50292) (layer F.SilkS))
    (fp_text value RSX101M-30 (at 0 0.51562) (layer F.SilkS))
    (pad A smd rect (at -1.39954 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(D2102-PadA)"))
    (pad K smd rect (at 1.39954 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(C2104-Pad1)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference D2301 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value D0603 (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(B33/ESC3709-PadP$2)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(B32/SHLCK3709-PadP$2)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference D2302 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value D0603 (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(B33/ESC3709-PadP$2)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(B31/ALT2301-PadP$2)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference D2303 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value D0603 (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B23/TAB3709-PadP$2)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(B22/3709-PadP$2)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference D2304 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value D0603 (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B23/TAB3709-PadP$2)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(B21/DEL3709-PadP$2)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference D2305 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value D0603 (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B13/SPC2301-PadP$2)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(B12/FN3709-PadP$2)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference D2306 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value D0603 (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B13/SPC2301-PadP$2)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(B11/ALT3709-PadP$2)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference D2307 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value D0603 (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B10/OK3709-PadP$2)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(B2/CTL2301-PadP$2)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference D2308 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value D0603 (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B10/OK3709-PadP$2)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(B1/CTL3709-PadP$2)"))
  )
  (module neo900-legacy:CRS02 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PACKAGE FOR TOSHIBA CRS02")
    (tags "PACKAGE FOR TOSHIBA CRS02")
    (attr smd)
    (fp_text reference D2501 (at -0.18288 -0.50292) (layer F.SilkS))
    (fp_text value RSX101M-30 (at 0 0.51562) (layer F.SilkS))
    (pad A smd rect (at -1.39954 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(D2501-PadA)"))
    (pad K smd rect (at 1.39954 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C2502-Pad1)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference D2502 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 22V,200mW,MM5Z22V (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(D2502-PadA)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C2502-Pad1)"))
  )
  (module neo900-legacy:CRS02 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PACKAGE FOR TOSHIBA CRS02")
    (tags "PACKAGE FOR TOSHIBA CRS02")
    (attr smd)
    (fp_text reference D3201 (at -0.18288 -0.50292) (layer F.SilkS))
    (fp_text value RSX101M-30 (at 0 0.51562) (layer F.SilkS))
    (pad A smd rect (at -1.39954 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(D3201-PadA)"))
    (pad K smd rect (at 1.39954 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(D3201-PadK)"))
  )
  (module neo900-legacy:CRS02 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PACKAGE FOR TOSHIBA CRS02")
    (tags "PACKAGE FOR TOSHIBA CRS02")
    (attr smd)
    (fp_text reference D3202 (at -0.18288 -0.50292) (layer F.SilkS))
    (fp_text value RSX101M-30 (at 0 0.51562) (layer F.SilkS))
    (pad A smd rect (at -1.39954 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(D3202-PadA)"))
    (pad K smd rect (at 1.39954 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(D3202-PadK)"))
  )
  (module neo900-legacy:TP-0.75 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT")
    (tags "TEST POINT")
    (attr smd)
    (fp_text reference DCD3709 (at 0 0) (layer F.SilkS))
    (fp_text value DCD (at 1.33096 0) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 9.32434 -1.13284) (layer B.SilkS))
    (pad P smd circle (at 0 0) (size 0.7493 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(DCD3709-PadP)"))
  )
  (module neo900-legacy:TP-0.75 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT")
    (tags "TEST POINT")
    (attr smd)
    (fp_text reference DSR3709 (at 0 0) (layer F.SilkS))
    (fp_text value DSR (at 1.33096 0) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 9.32434 -1.13284) (layer B.SilkS))
    (pad P smd circle (at 0 0) (size 0.7493 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(DSR3709-PadP)"))
  )
  (module neo900-legacy:TP-0.75 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT")
    (tags "TEST POINT")
    (attr smd)
    (fp_text reference DTR3709 (at 0 0) (layer F.SilkS))
    (fp_text value DTR (at 1.33096 0) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 9.32434 -1.13284) (layer B.SilkS))
    (pad P smd circle (at 0 0) (size 0.7493 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(DTR3709-PadP)"))
  )
  (module neo900-legacy:PAD-3.5X2.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference G1501 (at 0 0) (layer F.SilkS))
    (fp_text value SHIELDPAD-3.5X2.5 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:PAD-3.5X2.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference G1502 (at 0 0) (layer F.SilkS))
    (fp_text value SHIELDPAD-3.5X2.5 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:PAD-3.5X2.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference G1503 (at 0 0) (layer F.SilkS))
    (fp_text value SHIELDPAD-3.5X2.5 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:N900-SPRING-A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference G2201 (at 0 0) (layer F.SilkS))
    (fp_text value SHIELDN900 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:N900-SPRING-A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference G2202 (at 0 0) (layer F.SilkS))
    (fp_text value SHIELDN900 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:PAD-3.5X2.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference G2203 (at 0 0) (layer F.SilkS))
    (fp_text value SHIELDPAD-3.5X2.5 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:N900-SPRING-A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference G2204 (at 0 0) (layer F.SilkS))
    (fp_text value SHIELDN900 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:N900-SPRING-A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference G2205 (at 0 0) (layer F.SilkS))
    (fp_text value SHIELDN900 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:PAD-3.5X2.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference G2206 (at 0 0) (layer F.SilkS))
    (fp_text value SHIELDPAD-3.5X2.5 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:N900-SPRING-A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference G2207 (at 0 0) (layer F.SilkS))
    (fp_text value SHIELDN900 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:PAD-3.5X2.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference G2208 (at 0 0) (layer F.SilkS))
    (fp_text value SHIELDPAD-3.5X2.5 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:N900-SPRING-A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference G2209 (at 0 0) (layer F.SilkS))
    (fp_text value SHIELDN900 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference GPIO601 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 193 GPIO-MODEM_IGT))
  )
  (module neo900-legacy:N900-SPRING-A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference GPS-ANT3709 (at 0 0) (layer F.SilkS))
    (fp_text value CONNECT-POINTN900-A (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(GPS-ANT3709-Pad1)"))
  )
  (module neo900-legacy:N900-SPRING-A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference GPS-GND3709 (at 0 0) (layer F.SilkS))
    (fp_text value CONNECT-POINTN900-A (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference HS-1201 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(HS-1201-PadP)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference HS-1202 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(HS-1201-PadP)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference HS-1203 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(C1208-Pad1)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference HS-1204 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(HS-1204-PadP)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference HS-1205 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C1205-Pad1)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference HS-1206 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(HS-1206-PadP)"))
  )
  (module neo900-legacy:SMD-1212 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "1212 PACKAGE FOR INDUCTORS ETC.")
    (tags "1212 PACKAGE FOR INDUCTORS ETC.")
    (attr smd)
    (fp_text reference L301 (at -0.4826 -1.47574) (layer F.SilkS))
    (fp_text value 1u (at -0.2794 -0.9017) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.5mm" (at 6.25348 -2.33426) (layer F.SilkS))
    (pad 1 smd rect (at -1.19888 0) (size 1.09982 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 2 smd rect (at 1.19888 0) (size 1.09982 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C301-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L801 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 8n2;LQW15AN8N2G00D (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(L801-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(L801-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L802 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value DNP (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(GPS-ANT3709-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L803 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value DNP (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C802-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L804 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value DNP (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C802-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference L901 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value MLZ1608M100W (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(L901-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(L901-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L902 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 120n (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(L901-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:MPZ1608 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TDK MPZ1608 PACKAGE")
    (tags "TDK MPZ1608 PACKAGE")
    (attr smd)
    (fp_text reference L1101 (at 0.01524 -0.11684) (layer F.SilkS))
    (fp_text value tdb. (at -0.23622 0.2667) (layer F.SilkS))
    (pad 1 smd rect (at -0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C1102-Pad1)"))
    (pad 2 smd rect (at 0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 94 VMMC2))
  )
  (module neo900-legacy:MPZ1608 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TDK MPZ1608 PACKAGE")
    (tags "TDK MPZ1608 PACKAGE")
    (attr smd)
    (fp_text reference L1102 (at 0.01524 -0.11684) (layer F.SilkS))
    (fp_text value tbd. (at -0.23622 0.2667) (layer F.SilkS))
    (pad 1 smd rect (at -0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C1104-Pad1)"))
    (pad 2 smd rect (at 0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 94 VMMC2))
  )
  (module neo900-legacy:MPZ1608 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TDK MPZ1608 PACKAGE")
    (tags "TDK MPZ1608 PACKAGE")
    (attr smd)
    (fp_text reference L1103 (at 0.01524 -0.11684) (layer F.SilkS))
    (fp_text value tbd. (at -0.23622 0.2667) (layer F.SilkS))
    (pad 1 smd rect (at -0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C1107-Pad1)"))
    (pad 2 smd rect (at 0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
  )
  (module neo900-legacy:MPZ1608 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TDK MPZ1608 PACKAGE")
    (tags "TDK MPZ1608 PACKAGE")
    (attr smd)
    (fp_text reference L1201 (at 0.01524 -0.11684) (layer F.SilkS))
    (fp_text value MPZ1608S221A (at -0.23622 0.2667) (layer F.SilkS))
    (pad 1 smd rect (at -0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(C1201-Pad2)"))
    (pad 2 smd rect (at 0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 94 VMMC2))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L1202 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value tbd (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(HS-1201-PadP)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(D1203-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L1203 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value tbd (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(C1208-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(D1201-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L1204 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value tbd (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(HS-1204-PadP)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(C1217-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L1205 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value tbd (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C1205-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(D1204-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L1206 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value tbd (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(HS-1206-PadP)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(D1205-Pad2)"))
  )
  (module neo900-legacy:MPZ1608 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TDK MPZ1608 PACKAGE")
    (tags "TDK MPZ1608 PACKAGE")
    (attr smd)
    (fp_text reference L1207 (at 0.01524 -0.11684) (layer F.SilkS))
    (fp_text value MPZ1608S221A (at -0.23622 0.2667) (layer F.SilkS))
    (pad 1 smd rect (at -0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 2 smd rect (at 0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L1401 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value ~ (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(C1405-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(L1401-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L1402 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value ~ (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(C1404-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(L1402-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L1403 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value ~ (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 108 "/Audio Handsfree/SPKRR+"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(L1403-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L1404 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value ~ (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(C1410-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(L1404-Pad2)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference L1601 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 150n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C1605-Pad1)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(C1607-Pad2)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference L1602 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 330n (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(C1605-Pad2)"))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C1605-Pad1)"))
  )
  (module neo900-legacy:SMD-0805 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0805 BASED ON VISHAY PACKAGE")
    (tags "SMD 0805 BASED ON VISHAY PACKAGE")
    (attr smd)
    (fp_text reference L2101 (at -0.28194 -0.37592) (layer F.SilkS))
    (fp_text value ferrite (at -0.07874 0.16002) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 0) (size 0.79756 1.29794) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(C2105-Pad1)"))
    (pad 2 smd rect (at 0.99822 0) (size 0.79756 1.29794) (layers F.Cu F.Paste F.Mask)
      (net 206 "/uSD Breakout Board/USD-VBATT"))
  )
  (module neo900-legacy:SMD-0805 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0805 BASED ON VISHAY PACKAGE")
    (tags "SMD 0805 BASED ON VISHAY PACKAGE")
    (attr smd)
    (fp_text reference L2102 (at -0.28194 -0.37592) (layer F.SilkS))
    (fp_text value 2u2 (at -0.07874 0.16002) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 0) (size 0.79756 1.29794) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(D2102-PadA)"))
    (pad 2 smd rect (at 0.99822 0) (size 0.79756 1.29794) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(C2105-Pad1)"))
  )
  (module neo900-legacy:MPZ1608 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TDK MPZ1608 PACKAGE")
    (tags "TDK MPZ1608 PACKAGE")
    (attr smd)
    (fp_text reference L2401 (at 0.01524 -0.11684) (layer F.SilkS))
    (fp_text value tbd (at -0.23622 0.2667) (layer F.SilkS))
    (pad 1 smd rect (at -0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(C2402-Pad1)"))
    (pad 2 smd rect (at 0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 207 DMIC_BIAS))
  )
  (module neo900-legacy:MPZ1608 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TDK MPZ1608 PACKAGE")
    (tags "TDK MPZ1608 PACKAGE")
    (attr smd)
    (fp_text reference L2402 (at 0.01524 -0.11684) (layer F.SilkS))
    (fp_text value tbd (at -0.23622 0.2667) (layer F.SilkS))
    (pad 1 smd rect (at -0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(C2404-Pad1)"))
    (pad 2 smd rect (at 0.6985 0) (size 0.59944 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 207 DMIC_BIAS))
  )
  (module neo900-legacy:LB2016 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PACKAGE FOR INDUCTOR TAYO YUDEN BRC2016T100K")
    (tags "PACKAGE FOR INDUCTOR TAYO YUDEN BRC2016T100K")
    (attr smd)
    (fp_text reference L2501 (at -0.08382 -0.60198) (layer F.SilkS))
    (fp_text value 10uH,450mA,BRC2016T100K (at -0.18542 -0.0508) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 0) (size 0.6985 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(D2501-PadA)"))
    (pad 2 smd rect (at 0.7493 0) (size 0.6985 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
  )
  (module neo900-legacy:ACM2012H (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TDK COMMON MODE FILTER")
    (tags "TDK COMMON MODE FILTER")
    (attr smd)
    (fp_text reference L2502 (at 0.06096 -0.94996) (layer F.SilkS))
    (fp_text value ACM2012H (at 0.21336 0.84582) (layer F.SilkS))
    (pad 1 smd rect (at -0.92456 -0.39878 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 208 /Display-Panel&Power/CDP-D0+_UPPER))
    (pad 2 smd rect (at -0.92456 0.39878 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 209 /Display-Panel&Power/CDP-D0-_UPPER))
    (pad 3 smd rect (at 0.92456 0.39878 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(L2502-Pad3)"))
    (pad 4 smd rect (at 0.92456 -0.39878 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(L2502-Pad4)"))
  )
  (module neo900-legacy:ACM2012H (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TDK COMMON MODE FILTER")
    (tags "TDK COMMON MODE FILTER")
    (attr smd)
    (fp_text reference L2503 (at 0.06096 -0.94996) (layer F.SilkS))
    (fp_text value ACM2012H (at 0.21336 0.84582) (layer F.SilkS))
    (pad 1 smd rect (at -0.92456 -0.39878 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 212 /Display-Panel&Power/CDP-D1+_UPPER))
    (pad 2 smd rect (at -0.92456 0.39878 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 213 /Display-Panel&Power/CDP-D1-_UPPER))
    (pad 3 smd rect (at 0.92456 0.39878 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(L2503-Pad3)"))
    (pad 4 smd rect (at 0.92456 -0.39878 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(L2503-Pad4)"))
  )
  (module neo900-legacy:ACM2012H (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TDK COMMON MODE FILTER")
    (tags "TDK COMMON MODE FILTER")
    (attr smd)
    (fp_text reference L2504 (at 0.06096 -0.94996) (layer F.SilkS))
    (fp_text value ACM2012H (at 0.21336 0.84582) (layer F.SilkS))
    (pad 1 smd rect (at -0.92456 -0.39878 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 216 /Display-Panel&Power/CDP-CLK+_UPPER))
    (pad 2 smd rect (at -0.92456 0.39878 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 217 /Display-Panel&Power/CDP-CLK-_UPPER))
    (pad 3 smd rect (at 0.92456 0.39878 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(L2504-Pad3)"))
    (pad 4 smd rect (at 0.92456 -0.39878 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(L2504-Pad4)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference L3001 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value ~ (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 220 VAUX??))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(C3001-Pad1)"))
  )
  (module neo900-legacy:SMD-0806 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0806")
    (tags "SMD 0806")
    (attr smd)
    (fp_text reference L3201 (at -0.28194 -0.37592) (layer F.SilkS))
    (fp_text value 4u7 (at -0.07874 0.16002) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 0) (size 0.79756 1.59766) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(D3201-PadA)"))
    (pad 2 smd rect (at 0.99822 0) (size 0.79756 1.59766) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
  )
  (module neo900-legacy:SMD-0806 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0806")
    (tags "SMD 0806")
    (attr smd)
    (fp_text reference L3202 (at -0.28194 -0.37592) (layer F.SilkS))
    (fp_text value 4u7 (at -0.07874 0.16002) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 0) (size 0.79756 1.59766) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(D3202-PadA)"))
    (pad 2 smd rect (at 0.99822 0) (size 0.79756 1.59766) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference LC_IND3709 (at 0 0) (layer F.SilkS))
    (fp_text value LC (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 221 LC_IND))
  )
  (module neo900-legacy:CLN6A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "CREE WHITE LEDS")
    (tags "CREE WHITE LEDS")
    (attr smd)
    (fp_text reference LED2101 (at 0.50292 0.71374 270) (layer F.SilkS))
    (fp_text value CLN6A-MKW-CJ0K0233 (at -0.47244 0.96012 270) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.3mm" (at 3.75412 -5.13334) (layer B.SilkS))
    (pad 1 smd rect (at -2.99974 -1.59766) (size 1.09982 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(LED2101-Pad1)"))
    (pad 2 smd rect (at -2.99974 0) (size 1.09982 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(LED2101-Pad1)"))
    (pad 3 smd rect (at -2.99974 1.59766) (size 1.09982 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(LED2101-Pad1)"))
    (pad 4 smd rect (at 2.99974 1.59766) (size 1.09982 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(C2104-Pad1)"))
    (pad 5 smd rect (at 2.99974 0) (size 1.09982 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(C2104-Pad1)"))
    (pad 6 smd rect (at 2.99974 -1.59766) (size 1.09982 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(C2104-Pad1)"))
    (pad HS smd rect (at 0 0) (size 2.49936 3.49758) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(LED2101-Pad1)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference LED2102 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value LED-0603 (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(C2105-Pad1)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(LED2102-PadK)"))
  )
  (module neo900-legacy:CLN6A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "CREE WHITE LEDS")
    (tags "CREE WHITE LEDS")
    (attr smd)
    (fp_text reference LED2103 (at 0.50292 0.71374 270) (layer F.SilkS))
    (fp_text value CLN6A-MKW-CJ0K0233 (at -0.47244 0.96012 270) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.3mm" (at 3.75412 -5.13334) (layer B.SilkS))
    (pad 1 smd rect (at -2.99974 -1.59766) (size 1.09982 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(LED2103-Pad1)"))
    (pad 2 smd rect (at -2.99974 0) (size 1.09982 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(LED2103-Pad1)"))
    (pad 3 smd rect (at -2.99974 1.59766) (size 1.09982 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(LED2103-Pad1)"))
    (pad 4 smd rect (at 2.99974 1.59766) (size 1.09982 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(LED2101-Pad1)"))
    (pad 5 smd rect (at 2.99974 0) (size 1.09982 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(LED2101-Pad1)"))
    (pad 6 smd rect (at 2.99974 -1.59766) (size 1.09982 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(LED2101-Pad1)"))
    (pad HS smd rect (at 0 0) (size 2.49936 3.49758) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(LED2103-Pad1)"))
  )
  (module neo900-legacy:SMLP36RGB2W3 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference LED3101 (at 4.37388 -0.03302) (layer F.SilkS))
    (fp_text value LED-RGB-SMLP36 (at 2.80924 2.06248) (layer F.SilkS))
    (pad 1 smd rect (at -0.6731 0.42418) (size 0.44958 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(LED3101-Pad1)"))
    (pad 2 smd rect (at 0 0.42418) (size 0.39878 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(LED3101-Pad2)"))
    (pad 3 smd rect (at 0.6731 0.42418) (size 0.44958 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(LED3101-Pad3)"))
    (pad 4 smd rect (at 0.6731 -0.42418) (size 0.44958 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 5 smd rect (at 0 -0.42418) (size 0.39878 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 6 smd rect (at -0.6731 -0.42418) (size 0.44958 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SMLP36RGB2W3 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference LED3102 (at 4.37388 -0.03302) (layer F.SilkS))
    (fp_text value LED-RGB-SMLP36 (at 2.80924 2.06248) (layer F.SilkS))
    (pad 1 smd rect (at -0.6731 0.42418) (size 0.44958 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 228 "Net-(LED3102-Pad1)"))
    (pad 2 smd rect (at 0 0.42418) (size 0.39878 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(LED3102-Pad2)"))
    (pad 3 smd rect (at 0.6731 0.42418) (size 0.44958 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(LED3102-Pad3)"))
    (pad 4 smd rect (at 0.6731 -0.42418) (size 0.44958 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 5 smd rect (at 0 -0.42418) (size 0.39878 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 6 smd rect (at -0.6731 -0.42418) (size 0.44958 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:MSL0201RGB (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "ROHM MSL0201RGB (SIDE VIEW)")
    (tags "ROHM MSL0201RGB (SIDE VIEW)")
    (attr smd)
    (fp_text reference LED3201 (at -0.98298 -0.40132) (layer F.SilkS))
    (fp_text value LED-RGB-COMMON-A-MSL0201RGB (at -1.23698 0.5715) (layer F.SilkS))
    (fp_text user "HEIGHT> .43mm" (at 5.25272 -2.33426) (layer B.SilkS))
    (pad 1 smd rect (at 1.34874 -0.14986) (size 0.59944 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(LED3201-Pad1)"))
    (pad 2 smd rect (at 0.39878 0) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(LED3201-Pad2)"))
    (pad 3 smd rect (at -0.39878 0) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(LED3201-Pad3)"))
    (pad 4 smd rect (at -1.34874 -0.14986) (size 0.59944 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(D3201-PadK)"))
  )
  (module neo900-legacy:MSL0201RGB (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "ROHM MSL0201RGB (SIDE VIEW)")
    (tags "ROHM MSL0201RGB (SIDE VIEW)")
    (attr smd)
    (fp_text reference LED3202 (at -0.98298 -0.40132) (layer F.SilkS))
    (fp_text value LED-RGB-COMMON-A-MSL0201RGB (at -1.23698 0.5715) (layer F.SilkS))
    (fp_text user "HEIGHT> .43mm" (at 5.25272 -2.33426) (layer B.SilkS))
    (pad 1 smd rect (at 1.34874 -0.14986) (size 0.59944 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(LED3202-Pad1)"))
    (pad 2 smd rect (at 0.39878 0) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(LED3202-Pad2)"))
    (pad 3 smd rect (at -0.39878 0) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(LED3202-Pad3)"))
    (pad 4 smd rect (at -1.34874 -0.14986) (size 0.59944 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(D3202-PadK)"))
  )
  (module neo900-legacy:MSL0201RGB (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "ROHM MSL0201RGB (SIDE VIEW)")
    (tags "ROHM MSL0201RGB (SIDE VIEW)")
    (attr smd)
    (fp_text reference LED3203 (at -0.98298 -0.40132) (layer F.SilkS))
    (fp_text value LED-RGB-COMMON-A-MSL0201RGB (at -1.23698 0.5715) (layer F.SilkS))
    (fp_text user "HEIGHT> .43mm" (at 5.25272 -2.33426) (layer B.SilkS))
    (pad 1 smd rect (at 1.34874 -0.14986) (size 0.59944 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(LED3203-Pad1)"))
    (pad 2 smd rect (at 0.39878 0) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(LED3203-Pad2)"))
    (pad 3 smd rect (at -0.39878 0) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(LED3203-Pad3)"))
    (pad 4 smd rect (at -1.34874 -0.14986) (size 0.59944 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(D3201-PadK)"))
  )
  (module neo900-legacy:MSL0201RGB (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "ROHM MSL0201RGB (SIDE VIEW)")
    (tags "ROHM MSL0201RGB (SIDE VIEW)")
    (attr smd)
    (fp_text reference LED3204 (at -0.98298 -0.40132) (layer F.SilkS))
    (fp_text value LED-RGB-COMMON-A-MSL0201RGB (at -1.23698 0.5715) (layer F.SilkS))
    (fp_text user "HEIGHT> .43mm" (at 5.25272 -2.33426) (layer B.SilkS))
    (pad 1 smd rect (at 1.34874 -0.14986) (size 0.59944 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 240 "Net-(LED3204-Pad1)"))
    (pad 2 smd rect (at 0.39878 0) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(LED3204-Pad2)"))
    (pad 3 smd rect (at -0.39878 0) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(LED3204-Pad3)"))
    (pad 4 smd rect (at -1.34874 -0.14986) (size 0.59944 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(D3202-PadK)"))
  )
  (module neo900-legacy:MSL0201RGB (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "ROHM MSL0201RGB (SIDE VIEW)")
    (tags "ROHM MSL0201RGB (SIDE VIEW)")
    (attr smd)
    (fp_text reference LED3205 (at -0.98298 -0.40132) (layer F.SilkS))
    (fp_text value LED-RGB-COMMON-A-MSL0201RGB (at -1.23698 0.5715) (layer F.SilkS))
    (fp_text user "HEIGHT> .43mm" (at 5.25272 -2.33426) (layer B.SilkS))
    (pad 1 smd rect (at 1.34874 -0.14986) (size 0.59944 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 243 "Net-(LED3205-Pad1)"))
    (pad 2 smd rect (at 0.39878 0) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(LED3205-Pad2)"))
    (pad 3 smd rect (at -0.39878 0) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(LED3205-Pad3)"))
    (pad 4 smd rect (at -1.34874 -0.14986) (size 0.59944 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(D3201-PadK)"))
  )
  (module neo900-legacy:SMLP36RGB2W3 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference LED3206 (at 4.37388 -0.03302) (layer F.SilkS))
    (fp_text value LED-RGB-SMLP36 (at 2.80924 2.06248) (layer F.SilkS))
    (pad 1 smd rect (at -0.6731 0.42418) (size 0.44958 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(D3202-PadK)"))
    (pad 2 smd rect (at 0 0.42418) (size 0.39878 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(D3202-PadK)"))
    (pad 3 smd rect (at 0.6731 0.42418) (size 0.44958 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(D3202-PadK)"))
    (pad 4 smd rect (at 0.6731 -0.42418) (size 0.44958 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(LED3206-Pad4)"))
    (pad 5 smd rect (at 0 -0.42418) (size 0.39878 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(LED3206-Pad5)"))
    (pad 6 smd rect (at -0.6731 -0.42418) (size 0.44958 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(LED3206-Pad6)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference LED3207 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value LTST-C190KRKT (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(D3202-PadK)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 249 "Net-(LED3207-PadK)"))
  )
  (module neo900-legacy:MSL0201RGB (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "ROHM MSL0201RGB (SIDE VIEW)")
    (tags "ROHM MSL0201RGB (SIDE VIEW)")
    (attr smd)
    (fp_text reference LED3208 (at -0.98298 -0.40132) (layer F.SilkS))
    (fp_text value LED-RGB-COMMON-A-MSL0201RGB (at -1.23698 0.5715) (layer F.SilkS))
    (fp_text user "HEIGHT> .43mm" (at 5.25272 -2.33426) (layer B.SilkS))
    (pad 1 smd rect (at 1.34874 -0.14986) (size 0.59944 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(LED3208-Pad1)"))
    (pad 2 smd rect (at 0.39878 0) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(LED3208-Pad2)"))
    (pad 3 smd rect (at -0.39878 0) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 252 "Net-(LED3208-Pad3)"))
    (pad 4 smd rect (at -1.34874 -0.14986) (size 0.59944 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(D3201-PadK)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference LED3209 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value LTST-C190KFKT (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(D3202-PadK)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(LED3209-PadK)"))
  )
  (module neo900-legacy:SMD-0603D (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference LED3210 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value LTST-C190TBKT (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 1mm" (at 5.78358 -1.3335) (layer B.SilkS))
    (pad A smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(D3202-PadK)"))
    (pad K smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 254 CHG_IND))
  )
  (module neo900-legacy:P*S8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "CINTERION P*S8 LGA MODULES")
    (tags "CINTERION P*S8 LGA MODULES")
    (attr smd)
    (fp_text reference M601 (at 0 0) (layer F.SilkS))
    (fp_text value PHS8 (at 0 0) (layer F.SilkS))
    (fp_text user 1 (at 13.6017 13.79474) (layer F.SilkS))
    (fp_text user 16 (at -13.49248 13.89634) (layer F.SilkS))
    (fp_text user "HEIGHT> 2.0mm" (at -3.94462 -16.13408) (layer B.SilkS))
    (pad A4 smd rect (at 8.09752 11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 52 VMODEM2))
    (pad A5 smd rect (at 6.2992 11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad A6 smd rect (at 4.49834 11.69924) (size 1.4986 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad A7 smd rect (at 2.69748 11.69924) (size 0.79756 1.24968) (layers F.Cu F.Paste F.Mask))
    (pad A8 smd rect (at 0.89916 11.69924) (size 1.4986 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad A9 smd rect (at -0.89916 11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad A10 smd rect (at -2.70002 11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad A11 smd rect (at -4.49834 11.69924) (size 1.4986 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad A12 smd rect (at -6.2992 11.69924) (size 0.79756 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 255 GSM-ANT-DRX))
    (pad A13 smd rect (at -8.10006 11.69924) (size 1.4986 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad B3 smd rect (at 9.89838 9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 52 VMODEM2))
    (pad B4 smd rect (at 8.09752 9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad B5 smd rect (at 6.2992 9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad B6 smd rect (at 4.49834 9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad B7 smd rect (at 2.69748 9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad B8 smd rect (at 0.89916 9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad B9 smd rect (at -0.89916 9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad B10 smd rect (at -2.70002 9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad B11 smd rect (at -4.49834 9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad B12 smd rect (at -6.2992 9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad B13 smd rect (at -8.10006 9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad B14 smd rect (at -9.89838 9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 256 STATUS))
    (pad C2 smd rect (at 11.69924 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C3 smd rect (at 9.89838 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C4 smd rect (at 8.09752 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C5 smd rect (at 6.2992 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C6 smd rect (at 4.49834 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C7 smd rect (at 2.69748 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C8 smd rect (at 0.89916 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C9 smd rect (at -0.89916 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C10 smd rect (at -2.70002 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C11 smd rect (at -4.49834 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C12 smd rect (at -6.2992 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad C13 smd rect (at -8.10006 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad C14 smd rect (at -9.89838 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 257 "Net-(M601-PadC14)"))
    (pad C15 smd rect (at -11.69924 8.10006) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D1 smd rect (at 13.49756 6.2992) (size 0.99822 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D2 smd rect (at 11.69924 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D3 smd rect (at 9.89838 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D4 smd rect (at 8.09752 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D5 smd rect (at 6.2992 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 258 ANT-GNSS-DC))
    (pad D6 smd rect (at 4.49834 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D7 smd rect (at 2.69748 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D8 smd rect (at 0.89916 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D9 smd rect (at -0.89916 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D10 smd rect (at -2.70002 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D11 smd rect (at -4.49834 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D12 smd rect (at -6.2992 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad D13 smd rect (at -8.10006 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad D14 smd rect (at -9.89838 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad D15 smd rect (at -11.69924 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 259 "Net-(M601-PadD15)"))
    (pad D16 smd rect (at -13.49756 6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(M601-PadD16)"))
    (pad E1 smd rect (at 13.49756 4.49834) (size 1.24968 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 261 GNSS-IN))
    (pad E2 smd rect (at 11.69924 4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad E3 smd rect (at 9.89838 4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad E4 smd rect (at 8.09752 4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad E5 smd rect (at 6.2992 4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad E12 smd rect (at -6.2992 4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad E13 smd rect (at -8.10006 4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad E14 smd rect (at -9.89838 4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad E15 smd rect (at -11.69924 4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 262 "Net-(M601-PadE15)"))
    (pad E16 smd rect (at -13.49756 4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 263 "Net-(M601-PadE16)"))
    (pad F1 smd rect (at 13.49756 2.70002) (size 0.99822 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad F2 smd rect (at 11.69924 2.70002) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad F3 smd rect (at 9.89838 2.70002) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad F4 smd rect (at 8.09752 2.70002) (size 0.99822 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad F13 smd rect (at -8.10006 2.70002) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad F14 smd rect (at -9.89838 2.70002) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad F15 smd rect (at -11.69924 2.70002) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad F16 smd rect (at -13.49756 2.70002) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad G1 smd rect (at 13.49756 0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G2 smd rect (at 11.69924 0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G3 smd rect (at 9.89838 0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G4 smd rect (at 8.09752 0.89916) (size 1.24968 0.79756) (layers F.Cu F.Paste F.Mask))
    (pad G13 smd rect (at -8.10006 0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad G14 smd rect (at -9.89838 0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad G15 smd rect (at -11.69924 0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad G16 smd rect (at -13.49756 0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad H1 smd rect (at 13.49756 -0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad H2 smd rect (at 11.69924 -0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad H3 smd rect (at 9.89838 -0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad H4 smd rect (at 8.09752 -0.89916) (size 0.99822 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad H13 smd rect (at -8.10006 -0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad H14 smd rect (at -9.89838 -0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 264 3G-WOE))
    (pad H15 smd rect (at -11.69924 -0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad H16 smd rect (at -13.49756 -0.89916) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 221 LC_IND))
    (pad J1 smd rect (at 13.49756 -2.69748) (size 0.99822 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad J2 smd rect (at 11.69924 -2.69748) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad J3 smd rect (at 9.89838 -2.69748) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad J4 smd rect (at 8.09752 -2.69748) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad J13 smd rect (at -8.10006 -2.69748) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad J14 smd rect (at -9.89838 -2.69748) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad J15 smd rect (at -11.69924 -2.69748) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad J16 smd rect (at -13.49756 -2.69748) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad K1 smd rect (at 13.49756 -4.49834) (size 1.24968 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 265 GSM-ANT-TRX))
    (pad K2 smd rect (at 11.69924 -4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad K3 smd rect (at 9.89838 -4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad K4 smd rect (at 8.09752 -4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad K5 smd rect (at 6.2992 -4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad K12 smd rect (at -6.2992 -4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad K13 smd rect (at -8.10006 -4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad K14 smd rect (at -9.89838 -4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 266 MODEM_DATA_A))
    (pad K15 smd rect (at -11.69924 -4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C611-Pad1)"))
    (pad K16 smd rect (at -13.49756 -4.49834) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 55 VGNSS))
    (pad L1 smd rect (at 13.49756 -6.2992) (size 0.99822 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad L2 smd rect (at 11.69924 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad L3 smd rect (at 9.89838 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad L4 smd rect (at 8.09752 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad L5 smd rect (at 6.2992 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad L6 smd rect (at 4.49834 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad L7 smd rect (at 2.69748 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad L8 smd rect (at 0.89916 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad L9 smd rect (at -0.89916 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad L10 smd rect (at -2.70002 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad L11 smd rect (at -4.49834 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad L12 smd rect (at -6.2992 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad L13 smd rect (at -8.10006 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad L14 smd rect (at -9.89838 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 267 MODEM_RST_A))
    (pad L15 smd rect (at -11.69924 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 268 MODEM_CLK_A))
    (pad L16 smd rect (at -13.49756 -6.2992) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 269 "/3G/4G Modem + SIM/ON_KEY"))
    (pad M2 smd rect (at 11.69924 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad M3 smd rect (at 9.89838 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad M4 smd rect (at 8.09752 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 270 PWR_IND))
    (pad M5 smd rect (at 6.2992 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 271 "Net-(M601-PadM5)"))
    (pad M6 smd rect (at 4.49834 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad M7 smd rect (at 2.69748 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 272 MCBSP4-DX))
    (pad M8 smd rect (at 0.89916 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 273 MCBSP4-CLKX))
    (pad M9 smd rect (at -0.89916 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 274 MCBSP4-FSX))
    (pad M10 smd rect (at -2.70002 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 275 MCBSP4-DR))
    (pad M11 smd rect (at -4.49834 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad M12 smd rect (at -6.2992 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad M13 smd rect (at -8.10006 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad M14 smd rect (at -9.89838 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 276 MODEM-CD_A))
    (pad M15 smd rect (at -11.69924 -8.09752) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C601-Pad1)"))
    (pad N3 smd rect (at 9.89838 -9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 51 VMODEM1))
    (pad N4 smd rect (at 8.09752 -9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 51 VMODEM1))
    (pad N5 smd rect (at 6.2992 -9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 277 VBUS-MODEM))
    (pad N6 smd rect (at 4.49834 -9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 278 "Net-(M601-PadN6)"))
    (pad N7 smd rect (at 2.69748 -9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 279 "Net-(M601-PadN7)"))
    (pad N8 smd rect (at 0.89916 -9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 166 UART?-RTS))
    (pad N9 smd rect (at -0.89916 -9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(DCD3709-PadP)"))
    (pad N10 smd rect (at -2.70002 -9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 280 UART?-CTS))
    (pad N11 smd rect (at -4.49834 -9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad N12 smd rect (at -6.2992 -9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad N13 smd rect (at -8.10006 -9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 50 VMODEM3))
    (pad N14 smd rect (at -9.89838 -9.89838) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 281 EMERG_OFF))
    (pad P4 smd rect (at 8.09752 -11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 167 USB-WWAN-D+))
    (pad P5 smd rect (at 6.2992 -11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 168 USB-WWAN-D-))
    (pad P6 smd rect (at 4.49834 -11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 282 "Net-(M601-PadP6)"))
    (pad P7 smd rect (at 2.69748 -11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 283 "Net-(M601-PadP7)"))
    (pad P8 smd rect (at 0.89916 -11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(DTR3709-PadP)"))
    (pad P9 smd rect (at -0.89916 -11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(DSR3709-PadP)"))
    (pad P10 smd rect (at -2.70002 -11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 284 RING))
    (pad P11 smd rect (at -4.49834 -11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 285 UART?-TX))
    (pad P12 smd rect (at -6.2992 -11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 286 UART?-RX))
    (pad P13 smd rect (at -8.10006 -11.69924) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 50 VMODEM3))
  )
  (module neo900-legacy:WL18XXMOD (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "LGA FOR TI WL18XXMOD WILINK 8 MODULES")
    (tags "LGA FOR TI WL18XXMOD WILINK 8 MODULES")
    (attr smd)
    (fp_text reference M901 (at -3.47472 -4.90474) (layer F.SilkS))
    (fp_text value WL1837MODGIMOC (at -2.36982 4.99364) (layer F.SilkS))
    (fp_text user ">HEIGHT: 2mm" (at 0.05588 -0.00254) (layer B.SilkS))
    (pad 1 smd rect (at -6.02488 5.97408) (size 0.7493 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at -4.89966 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 287 "Net-(M901-Pad2)"))
    (pad 3 smd rect (at -4.19862 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 288 "Net-(M901-Pad3)"))
    (pad 4 smd rect (at -3.49758 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 289 "Net-(M901-Pad4)"))
    (pad 5 smd rect (at -2.79908 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 290 "Net-(M901-Pad5)"))
    (pad 6 smd rect (at -2.09804 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 291 "/WLAN, Bluetooth, FM/N$82"))
    (pad 7 smd rect (at -1.39954 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 8 smd rect (at -0.6985 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 292 "/WLAN, Bluetooth, FM/N$97"))
    (pad 9 smd rect (at 0 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 10 smd rect (at 0.6985 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 293 "/WLAN, Bluetooth, FM/N$63"))
    (pad 11 smd rect (at 1.39954 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 294 "/WLAN, Bluetooth, FM/N$62"))
    (pad 12 smd rect (at 2.09804 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 295 "/WLAN, Bluetooth, FM/N$59"))
    (pad 13 smd rect (at 2.79908 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 296 "/WLAN, Bluetooth, FM/N$61"))
    (pad 14 smd rect (at 3.49758 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 297 WLAN-IRQ))
    (pad 15 smd rect (at 4.19862 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 16 smd rect (at 4.89966 5.97408) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 17 smd rect (at 6.02488 5.97408) (size 0.7493 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 18 smd rect (at 6.02488 4.89966 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 298 "/WLAN, Bluetooth, FM/ANT2"))
    (pad 19 smd rect (at 6.02488 4.19862 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 20 smd rect (at 6.02488 3.49758 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 21 smd rect (at 6.02488 2.79908 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 6.02488 2.09804 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 6.02488 1.39954 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 24 smd rect (at 6.02488 0.6985 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 25 smd rect (at 6.02488 0 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 299 "Net-(M901-Pad25)"))
    (pad 26 smd rect (at 6.02488 -0.6985 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 300 "Net-(M901-Pad26)"))
    (pad 27 smd rect (at 6.02488 -1.39954 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 301 "Net-(M901-Pad27)"))
    (pad 28 smd rect (at 6.02488 -2.09804 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 29 smd rect (at 6.02488 -2.79908 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 30 smd rect (at 6.02488 -3.49758 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 31 smd rect (at 6.02488 -4.19862 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 32 smd rect (at 6.02488 -4.89966 90) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 302 "/WLAN, Bluetooth, FM/N$9"))
    (pad 33 smd rect (at 6.02488 -5.97408) (size 0.7493 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 34 smd rect (at 4.89966 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 35 smd rect (at 4.19862 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 36 smd rect (at 3.49758 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 303 32KHZ))
    (pad 37 smd rect (at 2.79908 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 38 smd rect (at 2.09804 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 39 smd rect (at 1.39954 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 40 smd rect (at 0.6985 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 304 WLAN-EN))
    (pad 41 smd rect (at 0 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 305 BT-EN))
    (pad 42 smd rect (at -0.6985 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 306 "Net-(M901-Pad42)"))
    (pad 43 smd rect (at -1.39954 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 307 "Net-(M901-Pad43)"))
    (pad 44 smd rect (at -2.09804 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 45 smd rect (at -2.79908 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 46 smd rect (at -3.49758 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 308 VBATT))
    (pad 47 smd rect (at -4.19862 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 308 VBATT))
    (pad 48 smd rect (at -4.89966 -5.97408 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 49 smd rect (at -6.02488 -5.97408) (size 0.7493 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 50 smd rect (at -6.02488 -4.89966 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 309 "/WLAN, Bluetooth, FM/N$57"))
    (pad 51 smd rect (at -6.02488 -4.19862 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 310 "/WLAN, Bluetooth, FM/N$15"))
    (pad 52 smd rect (at -6.02488 -3.49758 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 311 "/WLAN, Bluetooth, FM/N$36"))
    (pad 53 smd rect (at -6.02488 -2.79908 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 312 "/WLAN, Bluetooth, FM/N$13"))
    (pad 54 smd rect (at -6.02488 -2.09804 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 55 smd rect (at -6.02488 -1.39954 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 56 smd rect (at -6.02488 -0.6985 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 313 "/WLAN, Bluetooth, FM/BT-PCM-DX"))
    (pad 57 smd rect (at -6.02488 0 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 314 "/WLAN, Bluetooth, FM/BT-PCM-DR"))
    (pad 58 smd rect (at -6.02488 0.6985 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 315 "/WLAN, Bluetooth, FM/N$319"))
    (pad 59 smd rect (at -6.02488 1.39954 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 60 smd rect (at -6.02488 2.09804 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 316 "/WLAN, Bluetooth, FM/N$312"))
    (pad 61 smd rect (at -6.02488 2.79908 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 62 smd rect (at -6.02488 3.49758 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask))
    (pad 63 smd rect (at -6.02488 4.19862 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 64 smd rect (at -6.02488 4.89966 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G1 smd rect (at -3.8481 3.8481) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G2 smd rect (at -2.44856 3.8481) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G3 smd rect (at -1.04902 3.8481) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G4 smd rect (at 1.04902 3.8481) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G5 smd rect (at 2.44856 3.8481) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G6 smd rect (at 3.8481 3.8481) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G7 smd rect (at -3.8481 2.44856) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G8 smd rect (at -2.44856 2.44856) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G9 smd rect (at -1.04902 2.44856) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G10 smd rect (at 1.04902 2.44856) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G11 smd rect (at 2.44856 2.44856) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G12 smd rect (at 3.8481 2.44856) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G13 smd rect (at -3.8481 1.04902) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G14 smd rect (at -2.44856 1.04902) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G15 smd rect (at -1.04902 1.04902) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G16 smd rect (at 1.04902 1.04902) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G17 smd rect (at 2.44856 1.04902) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G18 smd rect (at 3.8481 1.04902) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G19 smd rect (at -3.8481 -1.04902) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G20 smd rect (at -2.44856 -1.04902) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G21 smd rect (at -1.04902 -1.04902) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G22 smd rect (at 1.04902 -1.04902) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G23 smd rect (at 2.44856 -1.04902) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G24 smd rect (at 3.8481 -1.04902) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G25 smd rect (at -3.8481 -2.44856) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G26 smd rect (at -2.44856 -2.44856) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G27 smd rect (at -1.04902 -2.44856) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G28 smd rect (at 1.04902 -2.44856) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G29 smd rect (at 2.44856 -2.44856) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G30 smd rect (at 3.8481 -2.44856) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G31 smd rect (at -3.8481 -3.8481) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G32 smd rect (at -2.44856 -3.8481) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G33 smd rect (at -1.04902 -3.8481) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G34 smd rect (at 1.04902 -3.8481) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G35 smd rect (at 2.44856 -3.8481) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G36 smd rect (at 3.8481 -3.8481) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SPK0415HM4H-B (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "KNOWLES SPK0415HM4H-B DIGITAL MICROPHONE")
    (tags "KNOWLES SPK0415HM4H-B DIGITAL MICROPHONE")
    (attr smd)
    (fp_text reference M2401 (at -3.81508 -0.99568 180) (layer F.SilkS))
    (fp_text value SPK0415HM4H (at -3.61188 -0.34544 180) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.06mm" (at 3.9878 -3.93446) (layer B.SilkS))
    (pad 1 smd rect (at 0.42418 0.6731 270) (size 0.94996 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(C2402-Pad1)"))
    (pad 2 smd rect (at 0.42418 -0.6731 270) (size 0.94996 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 3 smd rect (at -0.42418 -0.6731 270) (size 0.94996 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 138 DMIC_CLOCK))
    (pad 4 smd rect (at -0.42418 0.6731 270) (size 0.94996 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 317 DMIC_DATA))
    (pad 5 smd rect (at 0 1.77292) (size 1.29794 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 6 smd rect (at 1.27254 0 90) (size 2.2987 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 7 smd rect (at 0 -1.77292 180) (size 1.29794 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 8 smd rect (at -1.27254 0 270) (size 2.2987 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SPK0415HM4H-B (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "KNOWLES SPK0415HM4H-B DIGITAL MICROPHONE")
    (tags "KNOWLES SPK0415HM4H-B DIGITAL MICROPHONE")
    (attr smd)
    (fp_text reference M2402 (at -3.81508 -0.99568 180) (layer F.SilkS))
    (fp_text value SPK0415HM4H (at -3.61188 -0.34544 180) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.06mm" (at 3.9878 -3.93446) (layer B.SilkS))
    (pad 1 smd rect (at 0.42418 0.6731 270) (size 0.94996 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(C2404-Pad1)"))
    (pad 2 smd rect (at 0.42418 -0.6731 270) (size 0.94996 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(C2404-Pad1)"))
    (pad 3 smd rect (at -0.42418 -0.6731 270) (size 0.94996 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 138 DMIC_CLOCK))
    (pad 4 smd rect (at -0.42418 0.6731 270) (size 0.94996 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 317 DMIC_DATA))
    (pad 5 smd rect (at 0 1.77292) (size 1.29794 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 6 smd rect (at 1.27254 0 90) (size 2.2987 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 7 smd rect (at 0 -1.77292 180) (size 1.29794 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 8 smd rect (at -1.27254 0 270) (size 2.2987 0.44958) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference MCBSP4-CLK3709 (at 0 0) (layer F.SilkS))
    (fp_text value PCB-CLK (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 273 MCBSP4-CLKX))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference MCBSP4-DR3709 (at 0 0) (layer F.SilkS))
    (fp_text value PCM-OUT (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 275 MCBSP4-DR))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference MCBSP4-DX3709 (at 0 0) (layer F.SilkS))
    (fp_text value PCM-IN (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 272 MCBSP4-DX))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference MCBSP4-FSX3709 (at 0 0) (layer F.SilkS))
    (fp_text value PCM-SYNC (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 274 MCBSP4-FSX))
  )
  (module neo900-legacy:0R (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference N2901 (at 0 0) (layer F.SilkS))
    (fp_text value 0R (at 0 0) (layer F.SilkS))
    (pad P$1 smd rect (at -0.14986 0) (size 0.19812 0.19812) (layers F.Cu F.Paste F.Mask)
      (net 318 3V3-CPU))
    (pad P$2 smd rect (at 0.14986 0) (size 0.19812 0.19812) (layers F.Cu F.Paste F.Mask)
      (net 319 VMMC2-CPU))
  )
  (module neo900-legacy:N97-CAMERA (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HOLE FOR A N97 CAMERA MODULE")
    (tags "HOLE FOR A N97 CAMERA MODULE")
    (attr virtual)
    (fp_text reference N3001 (at 0 0) (layer F.SilkS))
    (fp_text value N97-CAMERA (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:NONE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (tags "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (attr virtual)
    (fp_text reference N3701 (at 0 0) (layer F.SilkS))
    (fp_text value 15015-0439 (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:NONE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (tags "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (attr virtual)
    (fp_text reference N3702 (at 0 0) (layer F.SilkS))
    (fp_text value 15015-0439 (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:NONE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (tags "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (attr virtual)
    (fp_text reference N3703 (at 0 0) (layer F.SilkS))
    (fp_text value 15015-0439 (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:NONE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (tags "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (attr virtual)
    (fp_text reference N3704 (at 0 0) (layer F.SilkS))
    (fp_text value "N900 case assembly" (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:N97-CAMERA-SPACE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HOLE FOR A N97 CAMERA MODULE")
    (tags "HOLE FOR A N97 CAMERA MODULE")
    (attr virtual)
    (fp_text reference N3705 (at 0 0) (layer F.SilkS))
    (fp_text value N97-CAMERA-HOLE (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:NONE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (tags "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (attr virtual)
    (fp_text reference N3706 (at 0 0) (layer F.SilkS))
    (fp_text value "headset jack" (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:GDC-STENCIL (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr virtual)
    (fp_text reference N3707 (at 0 0) (layer F.SilkS))
    (fp_text value STENCIL-TOP (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:GDC-STENCIL (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr virtual)
    (fp_text reference N3708 (at 0 0) (layer F.SilkS))
    (fp_text value STENCIL-BOTTOM (at 0 0) (layer F.SilkS))
  )
  (module neo900:N900-BATTCONN (layer F.Cu) (tedit 5790685E)
    (at 0 0)
    (descr "N900 BATTERY CONNECTOR")
    (tags "N900 BATTERY CONNECTOR")
    (attr smd)
    (fp_text reference P-BATT3709 (at 1.83134 -4.5339) (layer F.SilkS))
    (fp_text value BATT-3PIN-N900 (at 2.23774 -2.63398) (layer F.SilkS))
    (fp_text user "HEIGHT> 4.7mm" (at 4.953 -5.77342) (layer B.SilkS))
    (pad BAT3 smd rect (at 0 -3.69824) (size 4.49834 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(BATT+3709-PadP)"))
    (pad BAT2 smd rect (at 0 0) (size 4.49834 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(BATT-ID3709-PadP)"))
    (pad BAT1 smd rect (at 0 3.69824) (size 4.49834 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 27 "/Fuel Gauge/BGND"))
  )
  (module neo900-legacy:EVQQ0 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PANASONIC MULTI-LEVEL PUSHBUTTON (CAMERA SHUTTER)")
    (tags "PANASONIC MULTI-LEVEL PUSHBUTTON (CAMERA SHUTTER)")
    (attr smd)
    (fp_text reference P-CAMERA201 (at -0.47498 -2.10312) (layer F.SilkS))
    (fp_text value EVQ-Q0G03K (at -0.07112 -1.30302) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.5mm" (at 1.25476 -6.9342) (layer B.SilkS))
    (fp_text user "SPACE> -2.15mm" (at 1.88976 -5.334) (layer B.SilkS))
    (pad 1 smd rect (at -1.39954 0.89916 180) (size 1.19888 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 173 CAM1-GPIO))
    (pad 2 smd rect (at 0 0.89916 180) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 174 CAM2-GPIO))
    (pad 3 smd rect (at 1.39954 0.89916 180) (size 1.19888 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S1 smd rect (at -3.24866 -1.37414 90) (size 2.04978 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S2 smd rect (at 3.24866 -1.37414 270) (size 2.04978 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:500024-6471 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "MOLEX SLIMSTACK 0.4MM WITH 0.95MM STACKING HEIGHT (N900)")
    (tags "MOLEX SLIMSTACK 0.4MM WITH 0.95MM STACKING HEIGHT (N900)")
    (attr smd)
    (fp_text reference P-DISP3709 (at 0 0) (layer F.SilkS))
    (fp_text value N900-DISPLAY (at 0 0) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.95mm" (at 1.88976 -5.13334) (layer F.SilkS))
    (pad 1 smd rect (at 6.1976 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 2 smd rect (at 5.79882 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 3 smd rect (at 5.3975 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 4 smd rect (at 4.99872 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 5 smd rect (at 4.5974 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 320 EAR-_UPPER))
    (pad 6 smd rect (at 4.19862 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 321 EAR+_UPPER))
    (pad 7 smd rect (at 3.79984 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 8 smd rect (at 3.39852 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 322 "Net-(P-DISP3709-Pad8)"))
    (pad 9 smd rect (at 2.99974 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 323 2V5_UPPER))
    (pad 10 smd rect (at 2.59842 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 324 "Net-(P-DISP3709-Pad10)"))
    (pad 11 smd rect (at 2.19964 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 12 smd rect (at 1.79832 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 325 I2C2-SDA-CPU))
    (pad 13 smd rect (at 1.39954 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 326 I2C2-SCL-CPU))
    (pad 14 smd rect (at 0.99822 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 15 smd rect (at 0.59944 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 327 GPIO97))
    (pad 16 smd rect (at 0.19812 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 17 smd rect (at -0.19812 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 328 N$49_UPPER))
    (pad 18 smd rect (at -0.59944 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 19 smd rect (at -0.99822 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 329 N$50_UPPER))
    (pad 20 smd rect (at -1.39954 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 21 smd rect (at -1.79832 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 22 smd rect (at -2.19964 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 330 N$41_UPPER))
    (pad 23 smd rect (at -2.59842 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 24 smd rect (at -2.99974 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad 25 smd rect (at -3.39852 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 26 smd rect (at -3.79984 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 331 2V8_UPPER))
    (pad 27 smd rect (at -4.19862 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 28 smd rect (at -4.59994 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C2502-Pad1)"))
    (pad 29 smd rect (at -4.99872 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 332 "Net-(P-DISP3709-Pad29)"))
    (pad 30 smd rect (at -5.40004 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 333 "Net-(P-DISP3709-Pad30)"))
    (pad 31 smd rect (at -5.79882 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C2502-Pad1)"))
    (pad 32 smd rect (at -6.1976 2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 33 smd rect (at -6.1976 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 34 smd rect (at -5.79882 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 334 "Net-(P-DISP3709-Pad34)"))
    (pad 35 smd rect (at -5.40004 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 335 "Net-(P-DISP3709-Pad35)"))
    (pad 36 smd rect (at -4.99872 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 336 "Net-(P-DISP3709-Pad36)"))
    (pad 37 smd rect (at -4.59994 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 337 "Net-(P-DISP3709-Pad37)"))
    (pad 38 smd rect (at -4.19862 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 338 "Net-(P-DISP3709-Pad38)"))
    (pad 39 smd rect (at -3.79984 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 40 smd rect (at -3.39852 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(C2406-Pad1)"))
    (pad 41 smd rect (at -2.99974 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(C2409-Pad1)"))
    (pad 42 smd rect (at -2.59842 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 43 smd rect (at -2.19964 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C2408-Pad1)"))
    (pad 44 smd rect (at -1.79832 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(C2407-Pad1)"))
    (pad 45 smd rect (at -1.39954 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 46 smd rect (at -0.99822 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(L2503-Pad4)"))
    (pad 47 smd rect (at -0.59944 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(L2503-Pad3)"))
    (pad 48 smd rect (at -0.19812 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(L2504-Pad4)"))
    (pad 49 smd rect (at 0.19812 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(L2504-Pad3)"))
    (pad 50 smd rect (at 0.59944 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(L2502-Pad4)"))
    (pad 51 smd rect (at 0.99822 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(L2502-Pad3)"))
    (pad 52 smd rect (at 1.39954 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 53 smd rect (at 1.79832 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 339 /Camera/CSI-B-C-_UPPER))
    (pad 54 smd rect (at 2.19964 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 340 /Camera/CSI-B-C+_UPPER))
    (pad 55 smd rect (at 2.59842 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 56 smd rect (at 2.99974 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 341 /Camera/CSI-B-D-_UPPER))
    (pad 57 smd rect (at 3.39852 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 342 /Camera/CSI-B-D+_UPPER))
    (pad 58 smd rect (at 3.79984 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 59 smd rect (at 4.19862 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 343 CAM-CLK))
    (pad 60 smd rect (at 4.5974 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 61 smd rect (at 4.99872 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 344 "Net-(P-DISP3709-Pad61)"))
    (pad 62 smd rect (at 5.3975 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 345 "Net-(P-DISP3709-Pad62)"))
    (pad 63 smd rect (at 5.79882 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 346 "Net-(P-DISP3709-Pad63)"))
    (pad 64 smd rect (at 6.1976 -2.42316 180) (size 0.2286 0.6477) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad M1 smd rect (at -7.11962 2.31902 180) (size 0.89916 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad M2 smd rect (at -7.11962 -2.31902 180) (size 0.89916 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad M3 smd rect (at 7.11962 2.31902 180) (size 0.89916 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad M4 smd rect (at 7.11962 -2.31902 180) (size 0.89916 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:U.FL-SOCKET-SMT-HIROSE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "U.FL BOARD CONNECTOR")
    (tags "U.FL BOARD CONNECTOR")
    (attr smd)
    (fp_text reference P-DRX3709 (at -0.37592 -1.70434) (layer F.SilkS))
    (fp_text value ANTENNA-PLUGU.FL (at -0.07112 -0.60452) (layer F.SilkS))
    (pad GND1 smd rect (at -1.4732 0) (size 1.04902 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad GND2 smd rect (at 1.4732 0) (size 1.04902 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad SIG smd rect (at 0 1.524) (size 0.99822 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 255 GSM-ANT-DRX))
  )
  (module neo900-legacy:U.FL-SOCKET-SMT-HIROSE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "U.FL BOARD CONNECTOR")
    (tags "U.FL BOARD CONNECTOR")
    (attr smd)
    (fp_text reference P-GNSS3709 (at -0.37592 -1.70434) (layer F.SilkS))
    (fp_text value ANTENNA-PLUGU.FL (at -0.07112 -0.60452) (layer F.SilkS))
    (pad GND1 smd rect (at -1.4732 0) (size 1.04902 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad GND2 smd rect (at 1.4732 0) (size 1.04902 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad SIG smd rect (at 0 1.524) (size 0.99822 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 261 GNSS-IN))
  )
  (module neo900-legacy:N900-HEADSET (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HEADSET SOCKET WITH SPRING CONCTACTS USED IN THE NOKIA N900")
    (tags "HEADSET SOCKET WITH SPRING CONCTACTS USED IN THE NOKIA N900")
    (attr smd)
    (fp_text reference P-HS3709 (at 0 0) (layer F.SilkS))
    (fp_text value N900-HEADSET (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at -5.99948 2.99974 90) (size 1.79832 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(C1208-Pad1)"))
    (pad 2 smd rect (at -3.99796 -2.99974 90) (size 1.79832 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(HS-1201-PadP)"))
    (pad 3 smd rect (at -1.99898 1.99898 90) (size 1.79832 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C1205-Pad1)"))
    (pad 4 smd rect (at 0 -1.99898 90) (size 1.79832 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(HS-1204-PadP)"))
    (pad 5 smd rect (at 1.99898 2.99974 90) (size 1.79832 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(HS-1206-PadP)"))
    (pad 6 smd rect (at 3.99796 1.99898 90) (size 1.79832 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(HS-1201-PadP)"))
  )
  (module neo900-legacy:U.FL-SOCKET-SMT-HIROSE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "U.FL BOARD CONNECTOR")
    (tags "U.FL BOARD CONNECTOR")
    (attr smd)
    (fp_text reference P-INT801 (at -0.37592 -1.70434) (layer F.SilkS))
    (fp_text value ANTENNA-PLUGU.FL (at -0.07112 -0.60452) (layer F.SilkS))
    (pad GND1 smd rect (at -1.4732 0) (size 1.04902 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad GND2 smd rect (at 1.4732 0) (size 1.04902 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad SIG smd rect (at 0 1.524) (size 0.99822 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 347 "Net-(P-INT801-PadSIG)"))
  )
  (module neo900-legacy:ESE-16J001 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PANASONIC SENSOR BUTTON WITH \"SHARK FIN\"")
    (tags "PANASONIC SENSOR BUTTON WITH \"SHARK FIN\"")
    (attr smd)
    (fp_text reference P-LOCK201 (at 0.12192 -0.70358) (layer F.SilkS))
    (fp_text value ESE16J001 (at 0.32766 0.69342) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.55mm" (at 1.7653 -2.30378) (layer B.SilkS))
    (pad 1 smd rect (at -0.6985 -1.39954 270) (size 0.89916 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 169 LOCK-GPIO))
    (pad 2 smd rect (at 0.6985 -1.39954 270) (size 0.89916 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at -0.6985 1.39954 270) (size 0.89916 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 4 smd rect (at 0.6985 1.39954 270) (size 0.89916 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:ST1W008S4BR1500 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "JAE ST1W008S4B MICROSD READER WITH CARD PRESENCE DETECT")
    (tags "JAE ST1W008S4B MICROSD READER WITH CARD PRESENCE DETECT")
    (attr smd)
    (fp_text reference P-MICRO-SD3709 (at 1.87452 -4.13258) (layer F.SilkS))
    (fp_text value ST1W008S4BR1500 (at 2.50952 -2.03454) (layer F.SilkS))
    (pad 1 smd rect (at -3.99796 3.8481) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 348 "Net-(P-MICRO-SD3709-Pad1)"))
    (pad 2 smd rect (at -3.99796 2.74828) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 349 "Net-(P-MICRO-SD3709-Pad2)"))
    (pad 3 smd rect (at -3.99796 1.64846) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 350 "Net-(P-MICRO-SD3709-Pad3)"))
    (pad 4 smd rect (at -3.99796 0.54864) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(C2103-Pad1)"))
    (pad 5 smd rect (at -3.99796 -0.54864) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 351 "Net-(P-MICRO-SD3709-Pad5)"))
    (pad 6 smd rect (at -3.99796 -1.64846) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad 7 smd rect (at -3.99796 -2.74828) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 352 "Net-(P-MICRO-SD3709-Pad7)"))
    (pad 8 smd rect (at -3.99796 -3.8481) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 353 "Net-(P-MICRO-SD3709-Pad8)"))
    (pad S1 smd rect (at -5.99948 -3.24866) (size 1.39954 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad S2 smd rect (at -5.99948 3.24866) (size 1.39954 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad S3 smd rect (at 6.79958 -3.99796) (size 1.19888 1.59766) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad S4 smd rect (at 6.79958 2.70002) (size 1.19888 1.59766) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad SW smd rect (at 8.74776 1.29794) (size 1.4986 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(CD3709-PadP)"))
  )
  (module neo900-legacy:EVQP40B3M (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PANASONIC PUSHBUTTON")
    (tags "PANASONIC PUSHBUTTON")
    (attr smd)
    (fp_text reference P-MINUS201 (at -0.17526 -1.10236) (layer F.SilkS))
    (fp_text value EVQP42B3M (at 0.2286 -0.10414) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.35mm" (at 1.88976 -5.63372) (layer B.SilkS))
    (fp_text user "SPACE> -2.15mm" (at 1.88976 -3.7338) (layer B.SilkS))
    (pad 1 smd rect (at -2.2733 0.92456 180) (size 1.4478 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 171 GPIO-VOL-))
    (pad 2 smd rect (at 2.2733 0.92456 180) (size 1.4478 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S1 smd rect (at -3.19786 -0.79756 90) (size 0.79756 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S2 smd rect (at 3.19786 -0.79756 270) (size 0.79756 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:105017-0001 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "MICRO-B SOCKET MOLEX 105017-0001")
    (tags "MICRO-B SOCKET MOLEX 105017-0001")
    (attr smd)
    (fp_text reference P-MODEM3709-OTG2 (at 0.43942 -3.58648) (layer F.SilkS))
    (fp_text value 105017-0001 (at -0.17018 1.51384) (layer F.SilkS))
    (fp_text user "HEIGHT> 2.47mm" (at 2.68986 -5.73278) (layer B.SilkS))
    (pad 1/VB smd rect (at 1.29794 2.70002 90) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 354 VBUS-MODEM-CPU))
    (pad 2/D- smd rect (at 0.6477 2.70002 90) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 355 MODEM-CPU-D-))
    (pad 3/D+ smd rect (at 0 2.70002 90) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 356 MODEM-CPU-D+))
    (pad 4/ID smd rect (at -0.6477 2.70002 90) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 357 "Net-(P-MODEM3709-OTG2-Pad4/ID)"))
    (pad 5/GN smd rect (at -1.29794 2.70002 90) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad MOUN smd rect (at 0 0) (size 3.49758 1.89992) (layers F.Cu F.Paste F.Mask))
    (pad SH1 thru_hole circle (at -2.49936 2.69748) (size 1.4478 1.4478) (drill 0.84836) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad SH2 thru_hole circle (at 2.49936 2.69748) (size 1.4478 1.4478) (drill 0.84836) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad SH3 thru_hole circle (at -3.49758 0) (size 1.29794 1.29794) (drill 0.99822) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad SH4 thru_hole circle (at 3.49758 0) (size 1.29794 1.29794) (drill 0.99822) (layers *.Cu F.Paste F.SilkS F.Mask))
  )
  (module neo900-legacy:EVQP40B3M (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PANASONIC PUSHBUTTON")
    (tags "PANASONIC PUSHBUTTON")
    (attr smd)
    (fp_text reference P-ON201 (at -0.17526 -1.10236) (layer F.SilkS))
    (fp_text value EVQP40B3M (at 0.2286 -0.10414) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.35mm" (at 1.88976 -5.63372) (layer B.SilkS))
    (fp_text user "SPACE> -2.15mm" (at 1.88976 -3.7338) (layer B.SilkS))
    (pad 1 smd rect (at -2.2733 0.92456 180) (size 1.4478 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 172 POWERON))
    (pad 2 smd rect (at 2.2733 0.92456 180) (size 1.4478 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S1 smd rect (at -3.19786 -0.79756 90) (size 0.79756 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S2 smd rect (at 3.19786 -0.79756 270) (size 0.79756 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SD-47590-0001 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "MICRO-USB-AB (OTG) SOCKET MOLEX")
    (tags "MICRO-USB-AB (OTG) SOCKET MOLEX")
    (attr smd)
    (fp_text reference P-OTG3709 (at 0.43942 -3.58648) (layer F.SilkS))
    (fp_text value USB-AB-47590-0001 (at -0.17018 1.51384) (layer F.SilkS))
    (fp_text user "HEIGHT> 2.47mm" (at 2.68986 -5.73278) (layer B.SilkS))
    (pad 1/VB smd rect (at 1.29794 2.67462 90) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 29 VBUS))
    (pad 2/D- smd rect (at 0.6477 2.67462 90) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 358 OTG-D-))
    (pad 3/D+ smd rect (at 0 2.67462 90) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 359 OTG-D+))
    (pad 4/ID smd rect (at -0.6477 2.67462 90) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 360 OTG-ID))
    (pad 5/GN smd rect (at -1.29794 2.67462 90) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad MOUN smd rect (at 0 0) (size 2.89814 1.89992) (layers F.Cu F.Paste F.Mask))
    (pad SH1 thru_hole circle (at -2.2225 2.99974) (size 0.79756 0.79756) (drill 0.59944) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 30 GND))
    (pad SH2 thru_hole circle (at 2.2225 2.99974) (size 0.79756 0.79756) (drill 0.59944) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 30 GND))
    (pad SH3 thru_hole circle (at -4.17322 0) (size 1.29794 1.29794) (drill 0.99822) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 30 GND))
    (pad SH4 thru_hole circle (at 4.17322 0) (size 1.29794 1.29794) (drill 0.99822) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:EVQP40B3M (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PANASONIC PUSHBUTTON")
    (tags "PANASONIC PUSHBUTTON")
    (attr smd)
    (fp_text reference P-PLUS201 (at -0.17526 -1.10236) (layer F.SilkS))
    (fp_text value EVQP42B3M (at 0.2286 -0.10414) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.35mm" (at 1.88976 -5.63372) (layer B.SilkS))
    (fp_text user "SPACE> -2.15mm" (at 1.88976 -3.7338) (layer B.SilkS))
    (pad 1 smd rect (at -2.2733 0.92456 180) (size 1.4478 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 170 GPIO-VOL+))
    (pad 2 smd rect (at 2.2733 0.92456 180) (size 1.4478 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S1 smd rect (at -3.19786 -0.79756 90) (size 0.79756 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S2 smd rect (at 3.19786 -0.79756 270) (size 0.79756 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SJ106220 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "JAE SIM READER SJ106220 WITH 6 PINS")
    (tags "JAE SIM READER SJ106220 WITH 6 PINS")
    (attr smd)
    (fp_text reference P-SIM701 (at 0.60452 -4.13258) (layer F.SilkS))
    (fp_text value SIM-SLOT-6PIN+CD-CHECK-PINS (at 1.23952 -2.03454) (layer F.SilkS))
    (pad C1 smd rect (at 12.10818 -2.53746) (size 1.69926 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 361 "Net-(P-SIM701-PadC1)"))
    (pad C2 smd rect (at 12.10818 -0.53848) (size 1.69926 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 362 "/Dual SIM switch/N$224"))
    (pad C3 smd rect (at 12.10818 1.45796) (size 1.69926 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 363 "/Dual SIM switch/N$137"))
    (pad C5 smd rect (at -13.83792 -2.23774) (size 2.19964 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C6 smd rect (at -13.83792 0) (size 2.19964 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C7 smd rect (at -13.83792 2.23774) (size 2.19964 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 364 "/Dual SIM switch/N$342"))
    (pad CD smd rect (at 12.10818 2.86004) (size 1.69926 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 365 "/Dual SIM switch/N$338"))
    (pad CD-G smd rect (at 12.10818 -4.0386) (size 1.69926 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad CD-G smd rect (at 12.10818 4.25958) (size 1.69926 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S1 smd rect (at -13.74902 -4.77774) (size 2.09804 2.09804) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S2 smd rect (at -13.74902 4.77774) (size 2.09804 2.09804) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SJ106220 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "JAE SIM READER SJ106220 WITH 6 PINS")
    (tags "JAE SIM READER SJ106220 WITH 6 PINS")
    (attr smd)
    (fp_text reference P-SIM3709 (at 0.60452 -4.13258) (layer F.SilkS))
    (fp_text value SIM-SLOT-6PIN+CD-CHECK-PINS (at 1.23952 -2.03454) (layer F.SilkS))
    (pad C1 smd rect (at 12.10818 -2.53746) (size 1.69926 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C611-Pad1)"))
    (pad C2 smd rect (at 12.10818 -0.53848) (size 1.69926 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 54 SIM-RST))
    (pad C3 smd rect (at 12.10818 1.45796) (size 1.69926 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 366 SIM-CLK))
    (pad C5 smd rect (at -13.83792 -2.23774) (size 2.19964 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C6 smd rect (at -13.83792 0) (size 2.19964 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C7 smd rect (at -13.83792 2.23774) (size 2.19964 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 367 SIM-DATA))
    (pad CD smd rect (at 12.10818 2.86004) (size 1.69926 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 276 MODEM-CD_A))
    (pad CD-G smd rect (at 12.10818 -4.0386) (size 1.69926 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad CD-G smd rect (at 12.10818 4.25958) (size 1.69926 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S1 smd rect (at -13.74902 -4.77774) (size 2.09804 2.09804) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S2 smd rect (at -13.74902 4.77774) (size 2.09804 2.09804) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SWD-SOCKETSWITCH-SMT-MURATA (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "MURATA SOCKET SWITCH (FOR GSM ANTENNA MEASUREMENT)")
    (tags "MURATA SOCKET SWITCH (FOR GSM ANTENNA MEASUREMENT)")
    (attr smd)
    (fp_text reference P-WWAN3709 (at 1.20396 0.12192 270) (layer F.SilkS))
    (fp_text value MM8430-2600RA1 (at 0 0) (layer F.SilkS))
    (pad GND1 smd rect (at -1.4986 -0.99822) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad GND2 smd rect (at -1.4986 0.99822) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad GND3 smd rect (at 1.4986 0.99822) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad GND4 smd rect (at 1.4986 -0.99822) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad IN smd rect (at 0 1.4986) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C803-Pad1)"))
    (pad OUT smd rect (at 0 -1.4986) (size 0.49784 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C802-Pad2)"))
  )
  (module neo900-legacy:FX6-20S-0.8SV (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HIROSE FX6 - 0.8MM PITCH STACKING HEIGHT 5 TO 9MM CONNECTOR")
    (tags "HIROSE FX6 - 0.8MM PITCH STACKING HEIGHT 5 TO 9MM CONNECTOR")
    (attr smd)
    (fp_text reference P1501 (at -3.4925 -0.3175) (layer F.SilkS))
    (fp_text value FX6-20-PLUG (at 1.905 -0.3175) (layer F.SilkS))
    (pad 1 smd rect (at 3.59918 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 3.59918 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 368 SD-DAT2))
    (pad 3 smd rect (at 2.79908 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 369 I2C2-SDA))
    (pad 4 smd rect (at 2.79908 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 370 SD-DAT3))
    (pad 5 smd rect (at 1.99898 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad 6 smd rect (at 1.99898 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 372 SD-CMD))
    (pad 7 smd rect (at 1.19888 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 373 GPIO-FLASH-STR))
    (pad 8 smd rect (at 1.19888 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 374 SD-VDD))
    (pad 9 smd rect (at 0.39878 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 375 GPIO-FLASH-EN))
    (pad 10 smd rect (at 0.39878 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 376 SD-CLK))
    (pad 11 smd rect (at -0.39878 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 377 GPIO-FLASH-INT))
    (pad 12 smd rect (at -0.39878 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 13 smd rect (at -1.19888 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 378 GPIO-CAM-COVER))
    (pad 14 smd rect (at -1.19888 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 379 SD-DAT1))
    (pad 15 smd rect (at -1.99898 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 16 smd rect (at -1.99898 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 380 SD-DAT0))
    (pad 17 smd rect (at -2.79908 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 381 GPIO-BATT-LID))
    (pad 18 smd rect (at -2.79908 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 19 smd rect (at -3.59918 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 20 smd rect (at -3.59918 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 382 SD-CD))
  )
  (module neo900-legacy:DF40C-60DS-0.4V (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "DF40C-60DS-0.4V (1.5 OR 2 MM STACKING HEIGHT)")
    (tags "DF40C-60DS-0.4V (1.5 OR 2 MM STACKING HEIGHT)")
    (attr smd)
    (fp_text reference P2001 (at -3.96748 -0.60452) (layer F.SilkS))
    (fp_text value DF40C-60DS-0.4V (at -3.56108 0.49276) (layer F.SilkS))
    (pad 1 smd rect (at 5.79882 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 2 smd rect (at 5.3975 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at 4.99872 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 383 "Net-(P2001-Pad3)"))
    (pad 4 smd rect (at 4.5974 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 384 "Net-(P2001-Pad4)"))
    (pad 5 smd rect (at 4.19862 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 385 "Net-(P2001-Pad5)"))
    (pad 6 smd rect (at 3.79984 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 386 "Net-(P2001-Pad6)"))
    (pad 7 smd rect (at 3.39852 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 387 "Net-(P2001-Pad7)"))
    (pad 8 smd rect (at 2.99974 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 388 "Net-(P2001-Pad8)"))
    (pad 9 smd rect (at 2.59842 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 389 "Net-(P2001-Pad9)"))
    (pad 10 smd rect (at 2.19964 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 390 "Net-(P2001-Pad10)"))
    (pad 11 smd rect (at 1.79832 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 391 "Net-(P2001-Pad11)"))
    (pad 12 smd rect (at 1.39954 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 392 "Net-(P2001-Pad12)"))
    (pad 13 smd rect (at 0.99822 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 393 "Net-(P2001-Pad13)"))
    (pad 14 smd rect (at 0.59944 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 394 "Net-(P2001-Pad14)"))
    (pad 15 smd rect (at 0.19812 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 395 "Net-(P2001-Pad15)"))
    (pad 16 smd rect (at -0.19812 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 396 "Net-(P2001-Pad16)"))
    (pad 17 smd rect (at -0.59944 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 397 "Net-(P2001-Pad17)"))
    (pad 18 smd rect (at -0.99822 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 398 "Net-(P2001-Pad18)"))
    (pad 19 smd rect (at -1.39954 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 399 "Net-(P2001-Pad19)"))
    (pad 20 smd rect (at -1.79832 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 400 "Net-(P2001-Pad20)"))
    (pad 21 smd rect (at -2.19964 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 401 "Net-(P2001-Pad21)"))
    (pad 22 smd rect (at -2.59842 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 402 "Net-(P2001-Pad22)"))
    (pad 23 smd rect (at -2.99974 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 403 "Net-(P2001-Pad23)"))
    (pad 24 smd rect (at -3.39852 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 404 "Net-(P2001-Pad24)"))
    (pad 25 smd rect (at -3.79984 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 405 "Net-(P2001-Pad25)"))
    (pad 26 smd rect (at -4.19862 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 406 "Net-(P2001-Pad26)"))
    (pad 27 smd rect (at -4.59994 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 407 "Net-(P2001-Pad27)"))
    (pad 28 smd rect (at -4.99872 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 408 "Net-(P2001-Pad28)"))
    (pad 29 smd rect (at -5.40004 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 30 smd rect (at -5.79882 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 31 smd rect (at -5.79882 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 32 smd rect (at -5.40004 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 33 smd rect (at -4.99872 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 409 "Net-(P2001-Pad33)"))
    (pad 34 smd rect (at -4.59994 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 410 "Net-(P2001-Pad34)"))
    (pad 35 smd rect (at -4.19862 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 411 "Net-(P2001-Pad35)"))
    (pad 36 smd rect (at -3.79984 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 412 "Net-(P2001-Pad36)"))
    (pad 37 smd rect (at -3.39852 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 413 "Net-(P2001-Pad37)"))
    (pad 38 smd rect (at -2.99974 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 414 "Net-(P2001-Pad38)"))
    (pad 39 smd rect (at -2.59842 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 415 "Net-(P2001-Pad39)"))
    (pad 40 smd rect (at -2.19964 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 416 "Net-(P2001-Pad40)"))
    (pad 41 smd rect (at -1.79832 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 417 "Net-(P2001-Pad41)"))
    (pad 42 smd rect (at -1.39954 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 418 "Net-(P2001-Pad42)"))
    (pad 43 smd rect (at -0.99822 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 419 "Net-(P2001-Pad43)"))
    (pad 44 smd rect (at -0.59944 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 420 "Net-(P2001-Pad44)"))
    (pad 45 smd rect (at -0.19812 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 421 "Net-(P2001-Pad45)"))
    (pad 46 smd rect (at 0.19812 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 422 "Net-(P2001-Pad46)"))
    (pad 47 smd rect (at 0.59944 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 423 "Net-(P2001-Pad47)"))
    (pad 48 smd rect (at 0.99822 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 424 "Net-(P2001-Pad48)"))
    (pad 49 smd rect (at 1.39954 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 425 "Net-(P2001-Pad49)"))
    (pad 50 smd rect (at 1.79832 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 426 "Net-(P2001-Pad50)"))
    (pad 51 smd rect (at 2.19964 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 427 "Net-(P2001-Pad51)"))
    (pad 52 smd rect (at 2.59842 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 428 "Net-(P2001-Pad52)"))
    (pad 53 smd rect (at 2.99974 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 429 "Net-(P2001-Pad53)"))
    (pad 54 smd rect (at 3.39852 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 430 "Net-(P2001-Pad54)"))
    (pad 55 smd rect (at 3.79984 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 431 "Net-(P2001-Pad55)"))
    (pad 56 smd rect (at 4.19862 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 432 "Net-(P2001-Pad56)"))
    (pad 57 smd rect (at 4.5974 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 433 "Net-(P2001-Pad57)"))
    (pad 58 smd rect (at 4.99872 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 434 "Net-(P2001-Pad58)"))
    (pad 59 smd rect (at 5.3975 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 60 smd rect (at 5.79882 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
  )
  (module neo900-legacy:DF40C-60DS-0.4V (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "DF40C-60DS-0.4V (1.5 OR 2 MM STACKING HEIGHT)")
    (tags "DF40C-60DS-0.4V (1.5 OR 2 MM STACKING HEIGHT)")
    (attr smd)
    (fp_text reference P2002 (at -3.96748 -0.60452) (layer F.SilkS))
    (fp_text value DF40C-60DS-0.4V (at -3.56108 0.49276) (layer F.SilkS))
    (pad 1 smd rect (at 5.79882 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 2 smd rect (at 5.3975 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at 4.99872 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 435 "Net-(P2002-Pad3)"))
    (pad 4 smd rect (at 4.5974 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 436 "Net-(P2002-Pad4)"))
    (pad 5 smd rect (at 4.19862 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 437 "Net-(P2002-Pad5)"))
    (pad 6 smd rect (at 3.79984 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 438 "Net-(P2002-Pad6)"))
    (pad 7 smd rect (at 3.39852 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 439 "Net-(P2002-Pad7)"))
    (pad 8 smd rect (at 2.99974 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 440 "Net-(P2002-Pad8)"))
    (pad 9 smd rect (at 2.59842 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 441 "Net-(P2002-Pad9)"))
    (pad 10 smd rect (at 2.19964 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 442 "Net-(P2002-Pad10)"))
    (pad 11 smd rect (at 1.79832 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 443 "Net-(P2002-Pad11)"))
    (pad 12 smd rect (at 1.39954 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 444 "Net-(P2002-Pad12)"))
    (pad 13 smd rect (at 0.99822 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 445 "Net-(P2002-Pad13)"))
    (pad 14 smd rect (at 0.59944 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 446 "Net-(P2002-Pad14)"))
    (pad 15 smd rect (at 0.19812 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 447 "Net-(P2002-Pad15)"))
    (pad 16 smd rect (at -0.19812 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 448 "Net-(P2002-Pad16)"))
    (pad 17 smd rect (at -0.59944 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 449 "Net-(P2002-Pad17)"))
    (pad 18 smd rect (at -0.99822 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 450 "Net-(P2002-Pad18)"))
    (pad 19 smd rect (at -1.39954 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 451 "Net-(P2002-Pad19)"))
    (pad 20 smd rect (at -1.79832 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 452 "Net-(P2002-Pad20)"))
    (pad 21 smd rect (at -2.19964 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 453 "Net-(P2002-Pad21)"))
    (pad 22 smd rect (at -2.59842 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 454 "Net-(P2002-Pad22)"))
    (pad 23 smd rect (at -2.99974 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 455 "Net-(P2002-Pad23)"))
    (pad 24 smd rect (at -3.39852 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 456 "Net-(P2002-Pad24)"))
    (pad 25 smd rect (at -3.79984 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 457 "Net-(P2002-Pad25)"))
    (pad 26 smd rect (at -4.19862 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 458 "Net-(P2002-Pad26)"))
    (pad 27 smd rect (at -4.59994 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 459 "Net-(P2002-Pad27)"))
    (pad 28 smd rect (at -4.99872 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 460 "Net-(P2002-Pad28)"))
    (pad 29 smd rect (at -5.40004 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 30 smd rect (at -5.79882 1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 31 smd rect (at -5.79882 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 32 smd rect (at -5.40004 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 33 smd rect (at -4.99872 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 461 "Net-(P2002-Pad33)"))
    (pad 34 smd rect (at -4.59994 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 462 "Net-(P2002-Pad34)"))
    (pad 35 smd rect (at -4.19862 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 463 "Net-(P2002-Pad35)"))
    (pad 36 smd rect (at -3.79984 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 464 "Net-(P2002-Pad36)"))
    (pad 37 smd rect (at -3.39852 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 465 "Net-(P2002-Pad37)"))
    (pad 38 smd rect (at -2.99974 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 466 "Net-(P2002-Pad38)"))
    (pad 39 smd rect (at -2.59842 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 467 "Net-(P2002-Pad39)"))
    (pad 40 smd rect (at -2.19964 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 468 "Net-(P2002-Pad40)"))
    (pad 41 smd rect (at -1.79832 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 469 "Net-(P2002-Pad41)"))
    (pad 42 smd rect (at -1.39954 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 470 "Net-(P2002-Pad42)"))
    (pad 43 smd rect (at -0.99822 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 471 "Net-(P2002-Pad43)"))
    (pad 44 smd rect (at -0.59944 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 472 "Net-(P2002-Pad44)"))
    (pad 45 smd rect (at -0.19812 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 473 "Net-(P2002-Pad45)"))
    (pad 46 smd rect (at 0.19812 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 474 "Net-(P2002-Pad46)"))
    (pad 47 smd rect (at 0.59944 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 475 "Net-(P2002-Pad47)"))
    (pad 48 smd rect (at 0.99822 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 476 "Net-(P2002-Pad48)"))
    (pad 49 smd rect (at 1.39954 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 477 "Net-(P2002-Pad49)"))
    (pad 50 smd rect (at 1.79832 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 478 "Net-(P2002-Pad50)"))
    (pad 51 smd rect (at 2.19964 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 479 "Net-(P2002-Pad51)"))
    (pad 52 smd rect (at 2.59842 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 480 "Net-(P2002-Pad52)"))
    (pad 53 smd rect (at 2.99974 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 481 "Net-(P2002-Pad53)"))
    (pad 54 smd rect (at 3.39852 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 482 "Net-(P2002-Pad54)"))
    (pad 55 smd rect (at 3.79984 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 483 "Net-(P2002-Pad55)"))
    (pad 56 smd rect (at 4.19862 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 484 "Net-(P2002-Pad56)"))
    (pad 57 smd rect (at 4.5974 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 485 "Net-(P2002-Pad57)"))
    (pad 58 smd rect (at 4.99872 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 486 "Net-(P2002-Pad58)"))
    (pad 59 smd rect (at 5.3975 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 60 smd rect (at 5.79882 -1.53924 180) (size 0.19812 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
  )
  (module neo900-legacy:FX6-20P-0.8SV (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "FX6 SOCKET")
    (tags "FX6 SOCKET")
    (attr smd)
    (fp_text reference P2101 (at -4.7625 -0.3175) (layer F.SilkS))
    (fp_text value FX6-20 (at 0.635 -0.3175) (layer F.SilkS))
    (pad 1 smd rect (at 3.59918 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad 2 smd rect (at 3.59918 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 348 "Net-(P-MICRO-SD3709-Pad1)"))
    (pad 3 smd rect (at 2.79908 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 487 "/uSD Breakout Board/USD-I2C2-SDA"))
    (pad 4 smd rect (at 2.79908 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 349 "Net-(P-MICRO-SD3709-Pad2)"))
    (pad 5 smd rect (at 1.99898 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 488 "/uSD Breakout Board/USD-I2C2-SCL"))
    (pad 6 smd rect (at 1.99898 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 350 "Net-(P-MICRO-SD3709-Pad3)"))
    (pad 7 smd rect (at 1.19888 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 489 "/uSD Breakout Board/USD-STR"))
    (pad 8 smd rect (at 1.19888 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(C2103-Pad1)"))
    (pad 9 smd rect (at 0.39878 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 490 "/uSD Breakout Board/USD-EN"))
    (pad 10 smd rect (at 0.39878 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 351 "Net-(P-MICRO-SD3709-Pad5)"))
    (pad 11 smd rect (at -0.39878 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 491 "/uSD Breakout Board/USD-INT"))
    (pad 12 smd rect (at -0.39878 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad 13 smd rect (at -1.19888 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 492 "Net-(P2101-Pad13)"))
    (pad 14 smd rect (at -1.19888 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 352 "Net-(P-MICRO-SD3709-Pad7)"))
    (pad 15 smd rect (at -1.99898 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 130 "/uSD Breakout Board/USD-3V3"))
    (pad 16 smd rect (at -1.99898 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 353 "Net-(P-MICRO-SD3709-Pad8)"))
    (pad 17 smd rect (at -2.79908 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 493 "/uSD Breakout Board/LID"))
    (pad 18 smd rect (at -2.79908 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 206 "/uSD Breakout Board/USD-VBATT"))
    (pad 19 smd rect (at -3.59918 -2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad 20 smd rect (at -3.59918 2.44856 90) (size 2.19964 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(CD3709-PadP)"))
  )
  (module neo900-legacy:DF40C-60DP-0.4V (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HIROSE B2B HEADER 2X30 PIN")
    (tags "HIROSE B2B HEADER 2X30 PIN")
    (attr smd)
    (fp_text reference P2201 (at 4.56692 0.4064 180) (layer F.SilkS))
    (fp_text value DF40C-60DP-0.4V (at 4.77012 -0.49276 180) (layer F.SilkS))
    (pad 1 smd rect (at 5.79882 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
    (pad 2 smd rect (at 5.3975 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 3 smd rect (at 4.99872 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 494 "Net-(P2201-Pad3)"))
    (pad 4 smd rect (at 4.5974 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 495 "Net-(P2201-Pad4)"))
    (pad 5 smd rect (at 4.19862 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 496 "Net-(P2201-Pad5)"))
    (pad 6 smd rect (at 3.79984 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 497 "Net-(P2201-Pad6)"))
    (pad 7 smd rect (at 3.39852 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 498 "Net-(P2201-Pad7)"))
    (pad 8 smd rect (at 2.99974 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 499 "Net-(P2201-Pad8)"))
    (pad 9 smd rect (at 2.59842 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 500 "Net-(P2201-Pad9)"))
    (pad 10 smd rect (at 2.19964 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 501 "Net-(P2201-Pad10)"))
    (pad 11 smd rect (at 1.79832 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 502 "Net-(P2201-Pad11)"))
    (pad 12 smd rect (at 1.39954 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 503 "Net-(P2201-Pad12)"))
    (pad 13 smd rect (at 0.99822 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 504 "Net-(P2201-Pad13)"))
    (pad 14 smd rect (at 0.59944 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 505 "Net-(P2201-Pad14)"))
    (pad 15 smd rect (at 0.19812 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 506 "Net-(P2201-Pad15)"))
    (pad 16 smd rect (at -0.19812 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 507 "Net-(P2201-Pad16)"))
    (pad 17 smd rect (at -0.59944 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 508 "Net-(P2201-Pad17)"))
    (pad 18 smd rect (at -0.99822 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 509 "Net-(P2201-Pad18)"))
    (pad 19 smd rect (at -1.39954 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 510 "Net-(P2201-Pad19)"))
    (pad 20 smd rect (at -1.79832 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 511 "Net-(P2201-Pad20)"))
    (pad 21 smd rect (at -2.19964 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 512 "Net-(P2201-Pad21)"))
    (pad 22 smd rect (at -2.59842 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 513 "Net-(P2201-Pad22)"))
    (pad 23 smd rect (at -2.99974 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 514 "Net-(P2201-Pad23)"))
    (pad 24 smd rect (at -3.39852 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 515 "Net-(P2201-Pad24)"))
    (pad 25 smd rect (at -3.79984 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 516 "Net-(P2201-Pad25)"))
    (pad 26 smd rect (at -4.19862 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 517 "Net-(P2201-Pad26)"))
    (pad 27 smd rect (at -4.59994 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 518 "Net-(P2201-Pad27)"))
    (pad 28 smd rect (at -4.99872 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 519 "Net-(P2201-Pad28)"))
    (pad 29 smd rect (at -5.40004 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 30 smd rect (at -5.79882 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
    (pad 31 smd rect (at -5.79882 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
    (pad 32 smd rect (at -5.40004 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 33 smd rect (at -4.99872 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 520 "Net-(P2201-Pad33)"))
    (pad 34 smd rect (at -4.59994 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 521 "Net-(P2201-Pad34)"))
    (pad 35 smd rect (at -4.19862 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 522 "Net-(P2201-Pad35)"))
    (pad 36 smd rect (at -3.79984 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 523 "Net-(P2201-Pad36)"))
    (pad 37 smd rect (at -3.39852 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 524 "Net-(P2201-Pad37)"))
    (pad 38 smd rect (at -2.99974 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 525 "Net-(P2201-Pad38)"))
    (pad 39 smd rect (at -2.59842 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 526 "Net-(P2201-Pad39)"))
    (pad 40 smd rect (at -2.19964 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 527 "Net-(P2201-Pad40)"))
    (pad 41 smd rect (at -1.79832 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 528 "Net-(P2201-Pad41)"))
    (pad 42 smd rect (at -1.39954 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 529 "Net-(P2201-Pad42)"))
    (pad 43 smd rect (at -0.99822 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 530 "Net-(P2201-Pad43)"))
    (pad 44 smd rect (at -0.59944 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 531 "Net-(P2201-Pad44)"))
    (pad 45 smd rect (at -0.19812 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 532 "Net-(P2201-Pad45)"))
    (pad 46 smd rect (at 0.19812 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 533 "Net-(P2201-Pad46)"))
    (pad 47 smd rect (at 0.59944 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 534 "Net-(P2201-Pad47)"))
    (pad 48 smd rect (at 0.99822 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 535 "Net-(P2201-Pad48)"))
    (pad 49 smd rect (at 1.39954 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 536 "Net-(P2201-Pad49)"))
    (pad 50 smd rect (at 1.79832 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 537 "Net-(P2201-Pad50)"))
    (pad 51 smd rect (at 2.19964 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 538 "Net-(P2201-Pad51)"))
    (pad 52 smd rect (at 2.59842 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 539 "Net-(P2201-Pad52)"))
    (pad 53 smd rect (at 2.99974 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 540 "Net-(P2201-Pad53)"))
    (pad 54 smd rect (at 3.39852 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 541 "Net-(P2201-Pad54)"))
    (pad 55 smd rect (at 3.79984 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 542 "Net-(P2201-Pad55)"))
    (pad 56 smd rect (at 4.19862 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 543 "Net-(P2201-Pad56)"))
    (pad 57 smd rect (at 4.5974 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 544 "Net-(P2201-Pad57)"))
    (pad 58 smd rect (at 4.99872 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 545 "Net-(P2201-Pad58)"))
    (pad 59 smd rect (at 5.3975 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 60 smd rect (at 5.79882 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
    (pad M1 smd rect (at 6.2738 -1.3335) (size 0.34798 0.65786) (layers F.Cu F.Paste F.Mask))
    (pad M2 smd rect (at -6.2738 -1.3335) (size 0.34798 0.65786) (layers F.Cu F.Paste F.Mask))
    (pad M3 smd rect (at -6.2738 1.3335) (size 0.34798 0.65786) (layers F.Cu F.Paste F.Mask))
    (pad M4 smd rect (at 6.2738 1.3335) (size 0.34798 0.65786) (layers F.Cu F.Paste F.Mask))
  )
  (module neo900-legacy:DF40C-60DP-0.4V (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HIROSE B2B HEADER 2X30 PIN")
    (tags "HIROSE B2B HEADER 2X30 PIN")
    (attr smd)
    (fp_text reference P2202 (at 4.56692 0.4064 180) (layer F.SilkS))
    (fp_text value DF40C-60DP-0.4V (at 4.77012 -0.49276 180) (layer F.SilkS))
    (pad 1 smd rect (at 5.79882 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
    (pad 2 smd rect (at 5.3975 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 3 smd rect (at 4.99872 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 546 "Net-(P2202-Pad3)"))
    (pad 4 smd rect (at 4.5974 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 547 "Net-(P2202-Pad4)"))
    (pad 5 smd rect (at 4.19862 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 548 "Net-(P2202-Pad5)"))
    (pad 6 smd rect (at 3.79984 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 549 "Net-(P2202-Pad6)"))
    (pad 7 smd rect (at 3.39852 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 550 "Net-(P2202-Pad7)"))
    (pad 8 smd rect (at 2.99974 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 551 "Net-(P2202-Pad8)"))
    (pad 9 smd rect (at 2.59842 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 552 "Net-(P2202-Pad9)"))
    (pad 10 smd rect (at 2.19964 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 553 "Net-(P2202-Pad10)"))
    (pad 11 smd rect (at 1.79832 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 554 "Net-(P2202-Pad11)"))
    (pad 12 smd rect (at 1.39954 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 555 "Net-(P2202-Pad12)"))
    (pad 13 smd rect (at 0.99822 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 556 "Net-(P2202-Pad13)"))
    (pad 14 smd rect (at 0.59944 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 557 "Net-(P2202-Pad14)"))
    (pad 15 smd rect (at 0.19812 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 558 "Net-(P2202-Pad15)"))
    (pad 16 smd rect (at -0.19812 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 559 "Net-(P2202-Pad16)"))
    (pad 17 smd rect (at -0.59944 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 560 "Net-(P2202-Pad17)"))
    (pad 18 smd rect (at -0.99822 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 561 "Net-(P2202-Pad18)"))
    (pad 19 smd rect (at -1.39954 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 562 "Net-(P2202-Pad19)"))
    (pad 20 smd rect (at -1.79832 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 563 "Net-(P2202-Pad20)"))
    (pad 21 smd rect (at -2.19964 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 564 "Net-(P2202-Pad21)"))
    (pad 22 smd rect (at -2.59842 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 565 "Net-(P2202-Pad22)"))
    (pad 23 smd rect (at -2.99974 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 566 "Net-(P2202-Pad23)"))
    (pad 24 smd rect (at -3.39852 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 567 "Net-(P2202-Pad24)"))
    (pad 25 smd rect (at -3.79984 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 568 "Net-(P2202-Pad25)"))
    (pad 26 smd rect (at -4.19862 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 569 "Net-(P2202-Pad26)"))
    (pad 27 smd rect (at -4.59994 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 570 "Net-(P2202-Pad27)"))
    (pad 28 smd rect (at -4.99872 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 571 "Net-(P2202-Pad28)"))
    (pad 29 smd rect (at -5.40004 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 30 smd rect (at -5.79882 -1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 572 "Net-(P2202-Pad30)"))
    (pad 31 smd rect (at -5.79882 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
    (pad 32 smd rect (at -5.40004 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 33 smd rect (at -4.99872 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 573 "Net-(P2202-Pad33)"))
    (pad 34 smd rect (at -4.59994 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 574 "Net-(P2202-Pad34)"))
    (pad 35 smd rect (at -4.19862 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 575 "Net-(P2202-Pad35)"))
    (pad 36 smd rect (at -3.79984 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 576 "Net-(P2202-Pad36)"))
    (pad 37 smd rect (at -3.39852 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 577 "Net-(P2202-Pad37)"))
    (pad 38 smd rect (at -2.99974 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 578 "Net-(P2202-Pad38)"))
    (pad 39 smd rect (at -2.59842 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 579 "Net-(P2202-Pad39)"))
    (pad 40 smd rect (at -2.19964 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 580 "Net-(P2202-Pad40)"))
    (pad 41 smd rect (at -1.79832 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 581 "Net-(P2202-Pad41)"))
    (pad 42 smd rect (at -1.39954 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 582 "Net-(P2202-Pad42)"))
    (pad 43 smd rect (at -0.99822 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 583 "Net-(P2202-Pad43)"))
    (pad 44 smd rect (at -0.59944 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 584 "Net-(P2202-Pad44)"))
    (pad 45 smd rect (at -0.19812 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 585 "Net-(P2202-Pad45)"))
    (pad 46 smd rect (at 0.19812 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 586 "Net-(P2202-Pad46)"))
    (pad 47 smd rect (at 0.59944 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 587 "Net-(P2202-Pad47)"))
    (pad 48 smd rect (at 0.99822 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 588 "Net-(P2202-Pad48)"))
    (pad 49 smd rect (at 1.39954 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 589 "Net-(P2202-Pad49)"))
    (pad 50 smd rect (at 1.79832 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 590 "Net-(P2202-Pad50)"))
    (pad 51 smd rect (at 2.19964 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 591 "Net-(P2202-Pad51)"))
    (pad 52 smd rect (at 2.59842 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 592 "Net-(P2202-Pad52)"))
    (pad 53 smd rect (at 2.99974 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 593 "Net-(P2202-Pad53)"))
    (pad 54 smd rect (at 3.39852 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 594 "Net-(P2202-Pad54)"))
    (pad 55 smd rect (at 3.79984 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 595 "Net-(P2202-Pad55)"))
    (pad 56 smd rect (at 4.19862 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 596 "Net-(P2202-Pad56)"))
    (pad 57 smd rect (at 4.5974 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 597 "Net-(P2202-Pad57)"))
    (pad 58 smd rect (at 4.99872 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 598 "Net-(P2202-Pad58)"))
    (pad 59 smd rect (at 5.3975 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 60 smd rect (at 5.79882 1.3335) (size 0.2286 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
    (pad M1 smd rect (at 6.2738 -1.3335) (size 0.34798 0.65786) (layers F.Cu F.Paste F.Mask))
    (pad M2 smd rect (at -6.2738 -1.3335) (size 0.34798 0.65786) (layers F.Cu F.Paste F.Mask))
    (pad M3 smd rect (at -6.2738 1.3335) (size 0.34798 0.65786) (layers F.Cu F.Paste F.Mask))
    (pad M4 smd rect (at 6.2738 1.3335) (size 0.34798 0.65786) (layers F.Cu F.Paste F.Mask))
  )
  (module neo900-legacy:DF37NB-20SD-0.4V (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HIROSE 0.95 MM B2B SOCKET WITH 2X10 PINS")
    (tags "HIROSE 0.95 MM B2B SOCKET WITH 2X10 PINS")
    (attr smd)
    (fp_text reference P3001 (at 0 0) (layer F.SilkS))
    (fp_text value DF37NB-20DS-0.4/N97CAM (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.79832 1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 599 "Net-(P3001-Pad1)"))
    (pad 2 smd rect (at -1.39954 1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 3 smd rect (at -0.99822 1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(C3001-Pad1)"))
    (pad 4 smd rect (at -0.59944 1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(C3001-Pad1)"))
    (pad 5 smd rect (at -0.19812 1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 6 smd rect (at 0.19812 1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 600 "Net-(P3001-Pad6)"))
    (pad 7 smd rect (at 0.59944 1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 601 "Net-(P3001-Pad7)"))
    (pad 8 smd rect (at 0.99822 1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 9 smd rect (at 1.39954 1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 602 "Net-(P3001-Pad9)"))
    (pad 10 smd rect (at 1.79832 1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 603 "Net-(P3001-Pad10)"))
    (pad 11 smd rect (at 1.79832 -1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 12 smd rect (at 1.39954 -1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad 13 smd rect (at 0.99822 -1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad 14 smd rect (at 0.59944 -1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 15 smd rect (at 0.19812 -1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
    (pad 16 smd rect (at -0.19812 -1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
    (pad 17 smd rect (at -0.59944 -1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 18 smd rect (at -0.99822 -1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 604 /Camera/GPIO102))
    (pad 19 smd rect (at -1.39954 -1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 605 I2C3-SCL-CPU))
    (pad 20 smd rect (at -1.79832 -1.32334 180) (size 0.2286 0.62992) (layers F.Cu F.Paste F.Mask)
      (net 606 I2C3-SDA-CPU))
    (pad M1 smd rect (at -3.03784 0 180) (size 0.37846 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad M2 smd rect (at 3.03784 0 180) (size 0.37846 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module "neo900-legacy:FH23-39S-0.3SHW(0.5)" (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HIROSE FH23-39S-0.3SHW(0.5) PACKAGE")
    (tags "HIROSE FH23-39S-0.3SHW(0.5) PACKAGE")
    (attr smd)
    (fp_text reference P3301 (at -2.46634 -1.00584) (layer F.SilkS))
    (fp_text value FH23-39S (at -2.05994 0.39116) (layer F.SilkS))
    (fp_text user 2 (at 6.53288 -1.83388) (layer F.SilkS))
    (fp_text user 38 (at -5.52958 -1.93294) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.25mm" (at 3.08864 -4.13258) (layer B.SilkS))
    (pad 1 smd rect (at 5.69976 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad 2 smd rect (at 5.3975 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad 3 smd rect (at 5.09778 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad 4 smd rect (at 4.79806 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad 5 smd rect (at 4.49834 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 607 "Net-(P3301-Pad5)"))
    (pad 6 smd rect (at 4.19862 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 608 "Net-(P3301-Pad6)"))
    (pad 7 smd rect (at 3.8989 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 8 smd rect (at 3.59918 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 9 smd rect (at 3.29946 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 10 smd rect (at 2.99974 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 11 smd rect (at 2.69748 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 609 "Net-(P3301-Pad11)"))
    (pad 12 smd rect (at 2.39776 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 610 "Net-(P3301-Pad12)"))
    (pad 13 smd rect (at 2.09804 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 611 "Net-(P3301-Pad13)"))
    (pad 14 smd rect (at 1.79832 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 612 "Net-(P3301-Pad14)"))
    (pad 15 smd rect (at 1.4986 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 613 "Net-(P3301-Pad15)"))
    (pad 16 smd rect (at 1.19888 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 614 "Net-(P3301-Pad16)"))
    (pad 17 smd rect (at 0.89916 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 615 "Net-(P3301-Pad17)"))
    (pad 18 smd rect (at 0.59944 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 616 "Net-(P3301-Pad18)"))
    (pad 19 smd rect (at 0.29972 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 617 "Net-(P3301-Pad19)"))
    (pad 20 smd rect (at 0 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 618 "Net-(P3301-Pad20)"))
    (pad 21 smd rect (at -0.29972 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 619 "Net-(P3301-Pad21)"))
    (pad 22 smd rect (at -0.59944 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 620 "Net-(P3301-Pad22)"))
    (pad 23 smd rect (at -0.89916 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 621 "Net-(P3301-Pad23)"))
    (pad 24 smd rect (at -1.19888 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 622 "Net-(P3301-Pad24)"))
    (pad 25 smd rect (at -1.4986 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 623 "Net-(P3301-Pad25)"))
    (pad 26 smd rect (at -1.79832 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 624 "Net-(P3301-Pad26)"))
    (pad 27 smd rect (at -2.09804 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 625 "Net-(P3301-Pad27)"))
    (pad 28 smd rect (at -2.39776 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 626 "Net-(P3301-Pad28)"))
    (pad 29 smd rect (at -2.70002 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 627 "Net-(P3301-Pad29)"))
    (pad 30 smd rect (at -2.99974 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 628 "Net-(P3301-Pad30)"))
    (pad 31 smd rect (at -3.29946 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 629 "Net-(P3301-Pad31)"))
    (pad 32 smd rect (at -3.59918 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 630 "Net-(P3301-Pad32)"))
    (pad 33 smd rect (at -3.8989 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 631 "Net-(P3301-Pad33)"))
    (pad 34 smd rect (at -4.19862 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 632 "Net-(P3301-Pad34)"))
    (pad 35 smd rect (at -4.49834 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 633 "Net-(P3301-Pad35)"))
    (pad 36 smd rect (at -4.79806 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 634 "Net-(P3301-Pad36)"))
    (pad 37 smd rect (at -5.09778 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 325 I2C2-SDA-CPU))
    (pad 38 smd rect (at -5.40004 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 326 I2C2-SCL-CPU))
    (pad 39 smd rect (at -5.69976 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 635 NRESWARM-CPU))
  )
  (module "neo900-legacy:FH23-39S-0.3SHW(0.5)" (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HIROSE FH23-39S-0.3SHW(0.5) PACKAGE")
    (tags "HIROSE FH23-39S-0.3SHW(0.5) PACKAGE")
    (attr smd)
    (fp_text reference P3302 (at -2.46634 -1.00584) (layer F.SilkS))
    (fp_text value FH23-39S (at -2.05994 0.39116) (layer F.SilkS))
    (fp_text user 2 (at 6.53288 -1.83388) (layer F.SilkS))
    (fp_text user 38 (at -5.52958 -1.93294) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.25mm" (at 3.08864 -4.13258) (layer B.SilkS))
    (pad 1 smd rect (at 5.69976 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 636 "Net-(P3302-Pad1)"))
    (pad 2 smd rect (at 5.3975 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 637 "Net-(P3302-Pad2)"))
    (pad 3 smd rect (at 5.09778 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 638 "Net-(P3302-Pad3)"))
    (pad 4 smd rect (at 4.79806 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 5 smd rect (at 4.49834 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 6 smd rect (at 4.19862 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 7 smd rect (at 3.8989 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 8 smd rect (at 3.59918 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 639 "Net-(P3302-Pad8)"))
    (pad 9 smd rect (at 3.29946 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 640 "Net-(P3302-Pad9)"))
    (pad 10 smd rect (at 2.99974 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 605 I2C3-SCL-CPU))
    (pad 11 smd rect (at 2.69748 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 606 I2C3-SDA-CPU))
    (pad 12 smd rect (at 2.39776 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 641 "Net-(P3302-Pad12)"))
    (pad 13 smd rect (at 2.09804 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 642 "Net-(P3302-Pad13)"))
    (pad 14 smd rect (at 1.79832 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 643 "Net-(P3302-Pad14)"))
    (pad 15 smd rect (at 1.4986 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 644 "Net-(P3302-Pad15)"))
    (pad 16 smd rect (at 1.19888 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 645 "Net-(P3302-Pad16)"))
    (pad 17 smd rect (at 0.89916 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 646 "Net-(P3302-Pad17)"))
    (pad 18 smd rect (at 0.59944 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 647 "Net-(P3302-Pad18)"))
    (pad 19 smd rect (at 0.29972 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 648 "Net-(P3302-Pad19)"))
    (pad 20 smd rect (at 0 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 649 "Net-(P3302-Pad20)"))
    (pad 21 smd rect (at -0.29972 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 650 "Net-(P3302-Pad21)"))
    (pad 22 smd rect (at -0.59944 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 651 "Net-(P3302-Pad22)"))
    (pad 23 smd rect (at -0.89916 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 652 "Net-(P3302-Pad23)"))
    (pad 24 smd rect (at -1.19888 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 653 "Net-(P3302-Pad24)"))
    (pad 25 smd rect (at -1.4986 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 654 "Net-(P3302-Pad25)"))
    (pad 26 smd rect (at -1.79832 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 655 "Net-(P3302-Pad26)"))
    (pad 27 smd rect (at -2.09804 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 656 "Net-(P3302-Pad27)"))
    (pad 28 smd rect (at -2.39776 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 657 "Net-(P3302-Pad28)"))
    (pad 29 smd rect (at -2.70002 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 658 "Net-(P3302-Pad29)"))
    (pad 30 smd rect (at -2.99974 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 659 "Net-(P3302-Pad30)"))
    (pad 31 smd rect (at -3.29946 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 660 "Net-(P3302-Pad31)"))
    (pad 32 smd rect (at -3.59918 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 661 "Net-(P3302-Pad32)"))
    (pad 33 smd rect (at -3.8989 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 662 "Net-(P3302-Pad33)"))
    (pad 34 smd rect (at -4.19862 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 663 "Net-(P3302-Pad34)"))
    (pad 35 smd rect (at -4.49834 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 664 "Net-(P3302-Pad35)"))
    (pad 36 smd rect (at -4.79806 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 665 "Net-(P3302-Pad36)"))
    (pad 37 smd rect (at -5.09778 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 666 "Net-(P3302-Pad37)"))
    (pad 38 smd rect (at -5.40004 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 667 "Net-(P3302-Pad38)"))
    (pad 39 smd rect (at -5.69976 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 668 "Net-(P3302-Pad39)"))
  )
  (module "neo900-legacy:FH23-39S-0.3SHW(0.5)" (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HIROSE FH23-39S-0.3SHW(0.5) PACKAGE")
    (tags "HIROSE FH23-39S-0.3SHW(0.5) PACKAGE")
    (attr smd)
    (fp_text reference P3303 (at -2.46634 -1.00584) (layer F.SilkS))
    (fp_text value FH23-39S (at -2.05994 0.39116) (layer F.SilkS))
    (fp_text user 2 (at 6.53288 -1.83388) (layer F.SilkS))
    (fp_text user 38 (at -5.52958 -1.93294) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.25mm" (at 3.08864 -4.13258) (layer B.SilkS))
    (pad 1 smd rect (at 5.69976 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 669 "Net-(P3303-Pad1)"))
    (pad 2 smd rect (at 5.3975 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 670 "Net-(P3303-Pad2)"))
    (pad 3 smd rect (at 5.09778 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 671 "Net-(P3303-Pad3)"))
    (pad 4 smd rect (at 4.79806 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 672 "Net-(P3303-Pad4)"))
    (pad 5 smd rect (at 4.49834 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 673 "Net-(P3303-Pad5)"))
    (pad 6 smd rect (at 4.19862 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 674 "Net-(P3303-Pad6)"))
    (pad 7 smd rect (at 3.8989 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 675 "Net-(P3303-Pad7)"))
    (pad 8 smd rect (at 3.59918 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 676 "Net-(P3303-Pad8)"))
    (pad 9 smd rect (at 3.29946 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 677 "Net-(P3303-Pad9)"))
    (pad 10 smd rect (at 2.99974 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 678 "Net-(P3303-Pad10)"))
    (pad 11 smd rect (at 2.69748 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 679 "Net-(P3303-Pad11)"))
    (pad 12 smd rect (at 2.39776 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 680 "Net-(P3303-Pad12)"))
    (pad 13 smd rect (at 2.09804 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 681 "Net-(P3303-Pad13)"))
    (pad 14 smd rect (at 1.79832 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 682 "Net-(P3303-Pad14)"))
    (pad 15 smd rect (at 1.4986 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 683 "Net-(P3303-Pad15)"))
    (pad 16 smd rect (at 1.19888 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 684 "Net-(P3303-Pad16)"))
    (pad 17 smd rect (at 0.89916 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 685 "Net-(P3303-Pad17)"))
    (pad 18 smd rect (at 0.59944 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 686 "Net-(P3303-Pad18)"))
    (pad 19 smd rect (at 0.29972 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 687 "Net-(P3303-Pad19)"))
    (pad 20 smd rect (at 0 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 688 "Net-(P3303-Pad20)"))
    (pad 21 smd rect (at -0.29972 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 689 "Net-(P3303-Pad21)"))
    (pad 22 smd rect (at -0.59944 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 23 smd rect (at -0.89916 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 690 "Net-(P3303-Pad23)"))
    (pad 24 smd rect (at -1.19888 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 691 "Net-(P3303-Pad24)"))
    (pad 25 smd rect (at -1.4986 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 692 "Net-(P3303-Pad25)"))
    (pad 26 smd rect (at -1.79832 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 693 "Net-(P3303-Pad26)"))
    (pad 27 smd rect (at -2.09804 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 694 "Net-(P3303-Pad27)"))
    (pad 28 smd rect (at -2.39776 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 695 "Net-(P3303-Pad28)"))
    (pad 29 smd rect (at -2.70002 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 696 "Net-(P3303-Pad29)"))
    (pad 30 smd rect (at -2.99974 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 697 "Net-(P3303-Pad30)"))
    (pad 31 smd rect (at -3.29946 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 698 "Net-(P3303-Pad31)"))
    (pad 32 smd rect (at -3.59918 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 699 "Net-(P3303-Pad32)"))
    (pad 33 smd rect (at -3.8989 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 700 "Net-(P3303-Pad33)"))
    (pad 34 smd rect (at -4.19862 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 701 "Net-(P3303-Pad34)"))
    (pad 35 smd rect (at -4.49834 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 702 "Net-(P3303-Pad35)"))
    (pad 36 smd rect (at -4.79806 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 703 VAUX4))
    (pad 37 smd rect (at -5.09778 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 704 VAUX3))
    (pad 38 smd rect (at -5.40004 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 39 smd rect (at -5.69976 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:BEAGLEBOARD (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "J3,J4,J5 OF BEAGLEBOARD (TOP VIEW)")
    (tags "J3,J4,J5 OF BEAGLEBOARD (TOP VIEW)")
    (attr virtual)
    (fp_text reference P3401 (at 0 0) (layer F.SilkS))
    (fp_text value BEAGLEBOARD (at 0 0) (layer F.SilkS))
    (fp_text user J3 (at 2.86766 40.86352) (layer F.SilkS))
    (fp_text user 1 (at 8.4328 0.96266) (layer F.SilkS))
    (fp_text user 1 (at 3.23342 0.8636) (layer F.SilkS))
    (fp_text user 1 (at -0.16256 39.36492) (layer F.SilkS))
    (pad J3$1 thru_hole circle (at 1.4478 37.84854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$2 thru_hole circle (at 3.9878 37.84854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$3 thru_hole circle (at 1.4478 35.30854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$4 thru_hole circle (at 3.9878 35.30854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$5 thru_hole circle (at 1.4478 32.76854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$6 thru_hole circle (at 3.9878 32.76854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$7 thru_hole circle (at 1.4478 30.22854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$8 thru_hole circle (at 3.9878 30.22854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$9 thru_hole circle (at 1.4478 27.68854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$1 thru_hole circle (at 3.9878 27.68854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$1 thru_hole circle (at 1.4478 25.14854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$1 thru_hole circle (at 3.9878 25.14854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$1 thru_hole circle (at 1.4478 22.60854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$1 thru_hole circle (at 3.9878 22.60854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$1 thru_hole circle (at 1.4478 20.06854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$1 thru_hole circle (at 3.9878 20.06854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$1 thru_hole circle (at 1.4478 17.52854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$1 thru_hole circle (at 3.9878 17.52854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$1 thru_hole circle (at 1.4478 14.98854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$2 thru_hole circle (at 3.9878 14.98854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$2 thru_hole circle (at 1.4478 12.44854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$2 thru_hole circle (at 3.9878 12.44854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$2 thru_hole circle (at 1.4478 9.90854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$2 thru_hole circle (at 3.9878 9.90854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$2 thru_hole circle (at 1.4478 7.36854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$2 thru_hole circle (at 3.9878 7.36854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$2 thru_hole circle (at 1.4478 4.82854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J3$2 thru_hole circle (at 3.9878 4.82854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$1 thru_hole circle (at 1.27 0) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J4$2 thru_hole circle (at 0 0) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J4$3 thru_hole circle (at 1.27 -1.27) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 705 "/BB-XM Adapter (DISP)/BB-DSS1"))
    (pad J4$4 thru_hole circle (at 0 -1.27) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 706 "/BB-XM Adapter (DISP)/BB-DSS0"))
    (pad J4$5 thru_hole circle (at 1.27 -2.54) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 707 "/BB-XM Adapter (DISP)/BB-DSS3"))
    (pad J4$6 thru_hole circle (at 0 -2.54) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 708 "/BB-XM Adapter (DISP)/BB-DSS2"))
    (pad J4$7 thru_hole circle (at 1.27 -3.81) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 709 "/BB-XM Adapter (DISP)/BB-DSS5"))
    (pad J4$8 thru_hole circle (at 0 -3.81) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 710 "/BB-XM Adapter (DISP)/BB-DSS4"))
    (pad J4$9 thru_hole circle (at 1.27 -5.08) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 711 "/BB-XM Adapter (DISP)/BB-DSS12"))
    (pad J4$1 thru_hole circle (at 0 -5.08) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J4$1 thru_hole circle (at 1.27 -6.35) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J4$1 thru_hole circle (at 0 -6.35) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J4$1 thru_hole circle (at 1.27 -7.62) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J4$1 thru_hole circle (at 0 -7.62) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J4$1 thru_hole circle (at 1.27 -8.89) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J4$1 thru_hole circle (at 0 -8.89) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J4$1 thru_hole circle (at 1.27 -10.16) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J4$1 thru_hole circle (at 0 -10.16) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J4$1 thru_hole circle (at 1.27 -11.43) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J4$2 thru_hole circle (at 0 -11.43) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J5$1 thru_hole circle (at 5.79882 0) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL"))
    (pad J5$2 thru_hole circle (at 4.52882 0) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad J5$3 thru_hole circle (at 5.79882 -1.27) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 713 "/BB-XM Adapter (DISP)/BB-DSS20"))
    (pad J5$4 thru_hole circle (at 4.52882 -1.27) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 714 "/BB-XM Adapter (DISP)/BB-DSS21"))
    (pad J5$5 thru_hole circle (at 5.79882 -2.54) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 715 "/BB-XM Adapter (DISP)/BB-DSS17"))
    (pad J5$6 thru_hole circle (at 4.52882 -2.54) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 716 "/BB-XM Adapter (DISP)/BB-DSS18"))
    (pad J5$7 thru_hole circle (at 5.79882 -3.81) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 717 "/BB-XM Adapter (DISP)/BB-DSS15"))
    (pad J5$8 thru_hole circle (at 4.52882 -3.81) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 718 "/BB-XM Adapter (DISP)/BB-DSS16"))
    (pad J5$9 thru_hole circle (at 5.79882 -5.08) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 719 "/BB-XM Adapter (DISP)/BB-DSS7"))
    (pad J5$1 thru_hole circle (at 4.52882 -5.08) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL"))
    (pad J5$1 thru_hole circle (at 5.79882 -6.35) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL"))
    (pad J5$1 thru_hole circle (at 4.52882 -6.35) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL"))
    (pad J5$1 thru_hole circle (at 5.79882 -7.62) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL"))
    (pad J5$1 thru_hole circle (at 4.52882 -7.62) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL"))
    (pad J5$1 thru_hole circle (at 5.79882 -8.89) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL"))
    (pad J5$1 thru_hole circle (at 4.52882 -8.89) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL"))
    (pad J5$1 thru_hole circle (at 5.79882 -10.16) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL"))
    (pad J5$1 thru_hole circle (at 4.52882 -10.16) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL"))
    (pad J5$1 thru_hole circle (at 5.79882 -11.43) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL"))
    (pad J5$2 thru_hole circle (at 4.52882 -11.43) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
  )
  (module neo900-legacy:BEAGLEBOARD (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "J3,J4,J5 OF BEAGLEBOARD (TOP VIEW)")
    (tags "J3,J4,J5 OF BEAGLEBOARD (TOP VIEW)")
    (attr virtual)
    (fp_text reference P3401J3 (at 0 0) (layer F.SilkS))
    (fp_text value BEAGLEBOARD (at 0 0) (layer F.SilkS))
    (fp_text user J3 (at 2.86766 40.86352) (layer F.SilkS))
    (fp_text user 1 (at 8.4328 0.96266) (layer F.SilkS))
    (fp_text user 1 (at 3.23342 0.8636) (layer F.SilkS))
    (fp_text user 1 (at -0.16256 39.36492) (layer F.SilkS))
    (pad J3$1 thru_hole circle (at 1.4478 37.84854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 720 "/BB-XM Adapter (CPU)/BB-159"))
    (pad J3$2 thru_hole circle (at 3.9878 37.84854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 721 "/BB-XM Adapter (CPU)/BB-156"))
    (pad J3$3 thru_hole circle (at 1.4478 35.30854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 722 "/BB-XM Adapter (CPU)/BB-139"))
    (pad J3$4 thru_hole circle (at 3.9878 35.30854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 723 "/BB-XM Adapter (CPU)/BB-144"))
    (pad J3$5 thru_hole circle (at 1.4478 32.76854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 724 "/BB-XM Adapter (CPU)/BB-138"))
    (pad J3$6 thru_hole circle (at 3.9878 32.76854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 725 "/BB-XM Adapter (CPU)/BB-146"))
    (pad J3$7 thru_hole circle (at 1.4478 30.22854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 726 "/BB-XM Adapter (CPU)/BB-137"))
    (pad J3$8 thru_hole circle (at 3.9878 30.22854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 727 "/BB-XM Adapter (CPU)/BB-143"))
    (pad J3$9 thru_hole circle (at 1.4478 27.68854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 728 "/BB-XM Adapter (CPU)/BB-136"))
    (pad J3$1 thru_hole circle (at 3.9878 27.68854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 720 "/BB-XM Adapter (CPU)/BB-159"))
    (pad J3$1 thru_hole circle (at 1.4478 25.14854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 720 "/BB-XM Adapter (CPU)/BB-159"))
    (pad J3$1 thru_hole circle (at 3.9878 25.14854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 720 "/BB-XM Adapter (CPU)/BB-159"))
    (pad J3$1 thru_hole circle (at 1.4478 22.60854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 720 "/BB-XM Adapter (CPU)/BB-159"))
    (pad J3$1 thru_hole circle (at 3.9878 22.60854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 720 "/BB-XM Adapter (CPU)/BB-159"))
    (pad J3$1 thru_hole circle (at 1.4478 20.06854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 720 "/BB-XM Adapter (CPU)/BB-159"))
    (pad J3$1 thru_hole circle (at 3.9878 20.06854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 720 "/BB-XM Adapter (CPU)/BB-159"))
    (pad J3$1 thru_hole circle (at 1.4478 17.52854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 720 "/BB-XM Adapter (CPU)/BB-159"))
    (pad J3$1 thru_hole circle (at 3.9878 17.52854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 720 "/BB-XM Adapter (CPU)/BB-159"))
    (pad J3$1 thru_hole circle (at 1.4478 14.98854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 720 "/BB-XM Adapter (CPU)/BB-159"))
    (pad J3$2 thru_hole circle (at 3.9878 14.98854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 721 "/BB-XM Adapter (CPU)/BB-156"))
    (pad J3$2 thru_hole circle (at 1.4478 12.44854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 721 "/BB-XM Adapter (CPU)/BB-156"))
    (pad J3$2 thru_hole circle (at 3.9878 12.44854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 721 "/BB-XM Adapter (CPU)/BB-156"))
    (pad J3$2 thru_hole circle (at 1.4478 9.90854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 721 "/BB-XM Adapter (CPU)/BB-156"))
    (pad J3$2 thru_hole circle (at 3.9878 9.90854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 721 "/BB-XM Adapter (CPU)/BB-156"))
    (pad J3$2 thru_hole circle (at 1.4478 7.36854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 721 "/BB-XM Adapter (CPU)/BB-156"))
    (pad J3$2 thru_hole circle (at 3.9878 7.36854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 721 "/BB-XM Adapter (CPU)/BB-156"))
    (pad J3$2 thru_hole circle (at 1.4478 4.82854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 721 "/BB-XM Adapter (CPU)/BB-156"))
    (pad J3$2 thru_hole circle (at 3.9878 4.82854) (size 1.52908 1.52908) (drill 1.01854) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 721 "/BB-XM Adapter (CPU)/BB-156"))
    (pad J4$1 thru_hole circle (at 1.27 0) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$2 thru_hole circle (at 0 0) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$3 thru_hole circle (at 1.27 -1.27) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$4 thru_hole circle (at 0 -1.27) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$5 thru_hole circle (at 1.27 -2.54) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$6 thru_hole circle (at 0 -2.54) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$7 thru_hole circle (at 1.27 -3.81) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$8 thru_hole circle (at 0 -3.81) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$9 thru_hole circle (at 1.27 -5.08) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$1 thru_hole circle (at 0 -5.08) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$1 thru_hole circle (at 1.27 -6.35) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$1 thru_hole circle (at 0 -6.35) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$1 thru_hole circle (at 1.27 -7.62) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$1 thru_hole circle (at 0 -7.62) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$1 thru_hole circle (at 1.27 -8.89) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$1 thru_hole circle (at 0 -8.89) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$1 thru_hole circle (at 1.27 -10.16) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$1 thru_hole circle (at 0 -10.16) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$1 thru_hole circle (at 1.27 -11.43) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J4$2 thru_hole circle (at 0 -11.43) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$1 thru_hole circle (at 5.79882 0) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$2 thru_hole circle (at 4.52882 0) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$3 thru_hole circle (at 5.79882 -1.27) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$4 thru_hole circle (at 4.52882 -1.27) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$5 thru_hole circle (at 5.79882 -2.54) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$6 thru_hole circle (at 4.52882 -2.54) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$7 thru_hole circle (at 5.79882 -3.81) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$8 thru_hole circle (at 4.52882 -3.81) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$9 thru_hole circle (at 5.79882 -5.08) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$1 thru_hole circle (at 4.52882 -5.08) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$1 thru_hole circle (at 5.79882 -6.35) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$1 thru_hole circle (at 4.52882 -6.35) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$1 thru_hole circle (at 5.79882 -7.62) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$1 thru_hole circle (at 4.52882 -7.62) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$1 thru_hole circle (at 5.79882 -8.89) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$1 thru_hole circle (at 4.52882 -8.89) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$1 thru_hole circle (at 5.79882 -10.16) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$1 thru_hole circle (at 4.52882 -10.16) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$1 thru_hole circle (at 5.79882 -11.43) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
    (pad J5$2 thru_hole circle (at 4.52882 -11.43) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask))
  )
  (module "neo900-legacy:FH23-39S-0.3SHW(0.5)" (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HIROSE FH23-39S-0.3SHW(0.5) PACKAGE")
    (tags "HIROSE FH23-39S-0.3SHW(0.5) PACKAGE")
    (attr smd)
    (fp_text reference P3402 (at -2.46634 -1.00584) (layer F.SilkS))
    (fp_text value FH23-39S (at -2.05994 0.39116) (layer F.SilkS))
    (fp_text user 2 (at 6.53288 -1.83388) (layer F.SilkS))
    (fp_text user 38 (at -5.52958 -1.93294) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.25mm" (at 3.08864 -4.13258) (layer B.SilkS))
    (pad 1 smd rect (at 5.69976 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 729 "/BB-XM Adapter (CPU)/BB-NRESWARM"))
    (pad 2 smd rect (at 5.3975 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 730 "/BB-XM Adapter (CPU)/BB-I2C2SCL"))
    (pad 3 smd rect (at 5.09778 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 731 "/BB-XM Adapter (CPU)/BB-I2C2SDA"))
    (pad 4 smd rect (at 4.79806 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 732 "Net-(P3402-Pad4)"))
    (pad 5 smd rect (at 4.49834 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 733 "Net-(P3402-Pad5)"))
    (pad 6 smd rect (at 4.19862 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 734 "/BB-XM Adapter (CPU)/BB-130"))
    (pad 7 smd rect (at 3.8989 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 735 "/BB-XM Adapter (CPU)/BB-131"))
    (pad 8 smd rect (at 3.59918 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 736 "/BB-XM Adapter (CPU)/BB-132"))
    (pad 9 smd rect (at 3.29946 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 737 "/BB-XM Adapter (CPU)/BB-133"))
    (pad 10 smd rect (at 2.99974 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 738 "/BB-XM Adapter (CPU)/BB-134"))
    (pad 11 smd rect (at 2.69748 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 739 "/BB-XM Adapter (CPU)/BB-135"))
    (pad 12 smd rect (at 2.39776 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 728 "/BB-XM Adapter (CPU)/BB-136"))
    (pad 13 smd rect (at 2.09804 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 726 "/BB-XM Adapter (CPU)/BB-137"))
    (pad 14 smd rect (at 1.79832 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 724 "/BB-XM Adapter (CPU)/BB-138"))
    (pad 15 smd rect (at 1.4986 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 722 "/BB-XM Adapter (CPU)/BB-139"))
    (pad 16 smd rect (at 1.19888 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 740 "Net-(P3402-Pad16)"))
    (pad 17 smd rect (at 0.89916 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 727 "/BB-XM Adapter (CPU)/BB-143"))
    (pad 18 smd rect (at 0.59944 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 723 "/BB-XM Adapter (CPU)/BB-144"))
    (pad 19 smd rect (at 0.29972 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 741 "/BB-XM Adapter (CPU)/BB-145"))
    (pad 20 smd rect (at 0 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 725 "/BB-XM Adapter (CPU)/BB-146"))
    (pad 21 smd rect (at -0.29972 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 742 "Net-(P3402-Pad21)"))
    (pad 22 smd rect (at -0.59944 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 721 "/BB-XM Adapter (CPU)/BB-156"))
    (pad 23 smd rect (at -0.89916 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 743 "/BB-XM Adapter (CPU)/BB-157"))
    (pad 24 smd rect (at -1.19888 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 744 "/BB-XM Adapter (CPU)/BB-158"))
    (pad 25 smd rect (at -1.4986 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 720 "/BB-XM Adapter (CPU)/BB-159"))
    (pad 26 smd rect (at -1.79832 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 745 "Net-(P3402-Pad26)"))
    (pad 27 smd rect (at -2.09804 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 746 "/BB-XM Adapter (CPU)/BB-161"))
    (pad 28 smd rect (at -2.39776 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 747 "/BB-XM Adapter (CPU)/BB-162"))
    (pad 29 smd rect (at -2.70002 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 748 BB-1V8))
    (pad 30 smd rect (at -2.99974 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 31 smd rect (at -3.29946 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 32 smd rect (at -3.59918 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 33 smd rect (at -3.8989 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 34 smd rect (at -4.19862 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 162 BB-5V))
    (pad 35 smd rect (at -4.49834 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 162 BB-5V))
    (pad 36 smd rect (at -4.79806 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 164 "/BB-XM Adapter (CPU)/BB-VSYS"))
    (pad 37 smd rect (at -5.09778 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 164 "/BB-XM Adapter (CPU)/BB-VSYS"))
    (pad 38 smd rect (at -5.40004 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 164 "/BB-XM Adapter (CPU)/BB-VSYS"))
    (pad 39 smd rect (at -5.69976 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 164 "/BB-XM Adapter (CPU)/BB-VSYS"))
  )
  (module "neo900-legacy:FH23-39S-0.3SHW(0.5)" (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HIROSE FH23-39S-0.3SHW(0.5) PACKAGE")
    (tags "HIROSE FH23-39S-0.3SHW(0.5) PACKAGE")
    (attr smd)
    (fp_text reference P3501 (at -2.46634 -1.00584) (layer F.SilkS))
    (fp_text value FH23-39S (at -2.05994 0.39116) (layer F.SilkS))
    (fp_text user 2 (at 6.53288 -1.83388) (layer F.SilkS))
    (fp_text user 38 (at -5.52958 -1.93294) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.25mm" (at 3.08864 -4.13258) (layer B.SilkS))
    (pad 1 smd rect (at 5.69976 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 706 "/BB-XM Adapter (DISP)/BB-DSS0"))
    (pad 2 smd rect (at 5.3975 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 705 "/BB-XM Adapter (DISP)/BB-DSS1"))
    (pad 3 smd rect (at 5.09778 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 708 "/BB-XM Adapter (DISP)/BB-DSS2"))
    (pad 4 smd rect (at 4.79806 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 707 "/BB-XM Adapter (DISP)/BB-DSS3"))
    (pad 5 smd rect (at 4.49834 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 710 "/BB-XM Adapter (DISP)/BB-DSS4"))
    (pad 6 smd rect (at 4.19862 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 709 "/BB-XM Adapter (DISP)/BB-DSS5"))
    (pad 7 smd rect (at 3.8989 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 749 "/BB-XM Adapter (DISP)/BB-DSS6"))
    (pad 8 smd rect (at 3.59918 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 719 "/BB-XM Adapter (DISP)/BB-DSS7"))
    (pad 9 smd rect (at 3.29946 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 750 "/BB-XM Adapter (DISP)/BB-DSS8"))
    (pad 10 smd rect (at 2.99974 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 751 "/BB-XM Adapter (DISP)/BB-DSS9"))
    (pad 11 smd rect (at 2.69748 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 752 "/BB-XM Adapter (DISP)/BB-DSS10"))
    (pad 12 smd rect (at 2.39776 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 753 "/BB-XM Adapter (DISP)/BB-DSS11"))
    (pad 13 smd rect (at 2.09804 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 711 "/BB-XM Adapter (DISP)/BB-DSS12"))
    (pad 14 smd rect (at 1.79832 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 754 "/BB-XM Adapter (DISP)/BB-DSS13"))
    (pad 15 smd rect (at 1.4986 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 755 "/BB-XM Adapter (DISP)/BB-DSS14"))
    (pad 16 smd rect (at 1.19888 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 717 "/BB-XM Adapter (DISP)/BB-DSS15"))
    (pad 17 smd rect (at 0.89916 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 718 "/BB-XM Adapter (DISP)/BB-DSS16"))
    (pad 18 smd rect (at 0.59944 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 715 "/BB-XM Adapter (DISP)/BB-DSS17"))
    (pad 19 smd rect (at 0.29972 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 716 "/BB-XM Adapter (DISP)/BB-DSS18"))
    (pad 20 smd rect (at 0 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 756 "/BB-XM Adapter (DISP)/BB-DSS19"))
    (pad 21 smd rect (at -0.29972 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 713 "/BB-XM Adapter (DISP)/BB-DSS20"))
    (pad 22 smd rect (at -0.59944 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 714 "/BB-XM Adapter (DISP)/BB-DSS21"))
    (pad 23 smd rect (at -0.89916 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 757 "/BB-XM Adapter (DISP)/BB-DSS22"))
    (pad 24 smd rect (at -1.19888 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 758 "/BB-XM Adapter (DISP)/BB-DSS23"))
    (pad 25 smd rect (at -1.4986 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 759 "/BB-XM Adapter (DISP)/BB-DSSHS"))
    (pad 26 smd rect (at -1.79832 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 760 "/BB-XM Adapter (DISP)/BB-DSSVS"))
    (pad 27 smd rect (at -2.09804 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 761 "/BB-XM Adapter (DISP)/BB-DSSCK"))
    (pad 28 smd rect (at -2.39776 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 762 "/BB-XM Adapter (DISP)/BB-DSSDE"))
    (pad 29 smd rect (at -2.70002 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 763 "/BB-XM Adapter (DISP)/BB-I2C3SDA"))
    (pad 30 smd rect (at -2.99974 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 712 "/BB-XM Adapter (DISP)/BB-I2C3SCL"))
    (pad 31 smd rect (at -3.29946 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 764 BB-3V3))
    (pad 32 smd rect (at -3.59918 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 764 BB-3V3))
    (pad 33 smd rect (at -3.8989 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 34 smd rect (at -4.19862 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 35 smd rect (at -4.49834 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 36 smd rect (at -4.79806 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 37 smd rect (at -5.09778 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 162 BB-5V))
    (pad 38 smd rect (at -5.40004 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 162 BB-5V))
    (pad 39 smd rect (at -5.69976 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 162 BB-5V))
  )
  (module "neo900-legacy:FH23-39S-0.3SHW(0.5)" (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HIROSE FH23-39S-0.3SHW(0.5) PACKAGE")
    (tags "HIROSE FH23-39S-0.3SHW(0.5) PACKAGE")
    (attr smd)
    (fp_text reference P3601 (at -2.46634 -1.00584) (layer F.SilkS))
    (fp_text value FH23-39S (at -2.05994 0.39116) (layer F.SilkS))
    (fp_text user 2 (at 6.53288 -1.83388) (layer F.SilkS))
    (fp_text user 38 (at -5.52958 -1.93294) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.25mm" (at 3.08864 -4.13258) (layer B.SilkS))
    (pad 1 smd rect (at 5.69976 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 764 BB-3V3))
    (pad 2 smd rect (at 5.3975 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 765 "Net-(P3601-Pad2)"))
    (pad 3 smd rect (at 5.09778 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 766 "Net-(P3601-Pad3)"))
    (pad 4 smd rect (at 4.79806 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 767 "Net-(P3601-Pad4)"))
    (pad 5 smd rect (at 4.49834 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 768 "Net-(P3601-Pad5)"))
    (pad 6 smd rect (at 4.19862 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 769 "Net-(P3601-Pad6)"))
    (pad 7 smd rect (at 3.8989 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 770 "Net-(P3601-Pad7)"))
    (pad 8 smd rect (at 3.59918 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 771 "Net-(P3601-Pad8)"))
    (pad 9 smd rect (at 3.29946 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 772 "Net-(P3601-Pad9)"))
    (pad 10 smd rect (at 2.99974 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 773 "Net-(P3601-Pad10)"))
    (pad 11 smd rect (at 2.69748 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 774 "Net-(P3601-Pad11)"))
    (pad 12 smd rect (at 2.39776 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 775 "Net-(P3601-Pad12)"))
    (pad 13 smd rect (at 2.09804 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 776 "Net-(P3601-Pad13)"))
    (pad 14 smd rect (at 1.79832 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 777 "Net-(P3601-Pad14)"))
    (pad 15 smd rect (at 1.4986 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 778 "Net-(P3601-Pad15)"))
    (pad 16 smd rect (at 1.19888 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 779 "Net-(P3601-Pad16)"))
    (pad 17 smd rect (at 0.89916 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 780 "Net-(P3601-Pad17)"))
    (pad 18 smd rect (at 0.59944 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 781 "Net-(P3601-Pad18)"))
    (pad 19 smd rect (at 0.29972 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 782 "Net-(P3601-Pad19)"))
    (pad 20 smd rect (at 0 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 783 "Net-(P3601-Pad20)"))
    (pad 21 smd rect (at -0.29972 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 784 "Net-(P3601-Pad21)"))
    (pad 22 smd rect (at -0.59944 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 23 smd rect (at -0.89916 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 785 "Net-(P3601-Pad23)"))
    (pad 24 smd rect (at -1.19888 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 786 "Net-(P3601-Pad24)"))
    (pad 25 smd rect (at -1.4986 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 787 "Net-(P3601-Pad25)"))
    (pad 26 smd rect (at -1.79832 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 788 "Net-(P3601-Pad26)"))
    (pad 27 smd rect (at -2.09804 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 789 "Net-(P3601-Pad27)"))
    (pad 28 smd rect (at -2.39776 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 790 "Net-(P3601-Pad28)"))
    (pad 29 smd rect (at -2.70002 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 791 "Net-(P3601-Pad29)"))
    (pad 30 smd rect (at -2.99974 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 792 "Net-(P3601-Pad30)"))
    (pad 31 smd rect (at -3.29946 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 793 "Net-(P3601-Pad31)"))
    (pad 32 smd rect (at -3.59918 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 794 "Net-(P3601-Pad32)"))
    (pad 33 smd rect (at -3.8989 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 795 "Net-(P3601-Pad33)"))
    (pad 34 smd rect (at -4.19862 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 796 "Net-(P3601-Pad34)"))
    (pad 35 smd rect (at -4.49834 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 797 "Net-(P3601-Pad35)"))
    (pad 36 smd rect (at -4.79806 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 798 "Net-(P3601-Pad36)"))
    (pad 37 smd rect (at -5.09778 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 799 "Net-(P3601-Pad37)"))
    (pad 38 smd rect (at -5.40004 -2.3622) (size 0.29972 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 39 smd rect (at -5.69976 2.06248) (size 0.29972 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
  )
  (module neo900-legacy:BEAGLEBOARD-XM-CAM (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "J3,J4,J5 OF BEAGLEBOARD (TOP VIEW)")
    (tags "J3,J4,J5 OF BEAGLEBOARD (TOP VIEW)")
    (attr virtual)
    (fp_text reference P3602 (at 0 0) (layer F.SilkS))
    (fp_text value BEAGLEBOARD-XM-CAMERA (at 0 0) (layer F.SilkS))
    (pad P10$ thru_hole circle (at 9.62914 24.46782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 24.46782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 23.19782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 23.19782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 21.92782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 21.92782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 20.65782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 20.65782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 19.38782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 19.38782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 18.11782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 18.11782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 16.84782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 16.84782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 15.57782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 15.57782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 14.30782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 14.30782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 13.03782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 13.03782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 11.76782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 11.76782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 10.49782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 10.49782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 9.22782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 9.22782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 7.95782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 7.95782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 6.68782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 6.68782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 5.41782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 5.41782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 9.62914 4.14782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
    (pad P10$ thru_hole circle (at 8.39978 4.14782) (size 1.00584 1.00584) (drill 0.49784) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 163 GND4))
  )
  (module neo900-legacy:1PIN-HOLE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr virtual)
    (fp_text reference PGM3709 (at 0 0) (layer F.SilkS))
    (fp_text value - (at 0 0) (layer F.SilkS))
    (pad P$1 thru_hole oval (at 0 0 90) (size 2.99974 5.99948) (drill 1.99898) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 800 "Net-(PGM3709-PadP$1)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference PWR_IND3709 (at 0 0) (layer F.SilkS))
    (fp_text value RESET (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 270 PWR_IND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R201 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value "(0R)" (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 167 USB-WWAN-D+))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 359 OTG-D+))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R202 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value "(0R)" (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 168 USB-WWAN-D-))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 358 OTG-D-))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R203 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value "(0R)" (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 277 VBUS-MODEM))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 29 VBUS))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R301 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 317R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 801 "Net-(R301-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R302 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 5k52 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 802 BATTEMP))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C305-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R303 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 31k23 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 802 BATTEMP))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R401 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value "(0R)" (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R402 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 20mR (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 51 VMODEM1))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R403 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 20mR (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 52 VMODEM2))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R404 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 20mR (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 50 VMODEM3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R405 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C401-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R406 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C402-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 51 VMODEM1))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R407 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C403-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R408 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C404-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 52 VMODEM2))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R409 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C405-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R410 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C406-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 50 VMODEM3))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R501 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 804 HDQ))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 805 BATTID))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R502 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 805 BATTID))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(BATT-ID3709-PadP)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference R503 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value NTCG163JF103F (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 802 BATTEMP))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R504 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C502-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(BATT+3709-PadP)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R505 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C506-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(BATT+3709-PadP)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R506 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 27 "/Fuel Gauge/BGND"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C505-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R507 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 20mR (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 27 "/Fuel Gauge/BGND"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R508 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C504-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R599 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 0R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 42 BATT))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(BATT+3709-PadP)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R601 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 51R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 54 SIM-RST))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 267 MODEM_RST_A))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R602 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 51R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 367 SIM-DATA))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 266 MODEM_DATA_A))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R603 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 51R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 366 SIM-CLK))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 268 MODEM_CLK_A))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R701 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 51R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 365 "/Dual SIM switch/N$338"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R801 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 55 VGNSS))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 806 GPIO$52))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R802 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 806 GPIO$52))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R803 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 0R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 258 ANT-GNSS-DC))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R804 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value "(50R)" (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 255 GSM-ANT-DRX))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R805 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 0R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C802-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C802-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R806 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value tbd. (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 807 "Net-(R806-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 60 ADC1))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R807 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value tbd. (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 808 "Net-(R807-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 62 ADC2))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R901 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2k2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 809 "Net-(R901-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 810 "Net-(R901-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R902 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2k2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 811 "Net-(R902-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 812 "Net-(R902-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R903 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2k2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 813 "Net-(R903-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 814 "Net-(R903-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R904 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 175 "/WLAN, Bluetooth, FM/LOOP"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(L901-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R905 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 680R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 815 "Net-(R905-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 816 "Net-(R905-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R906 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2k2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 817 "Net-(R906-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 818 "Net-(R906-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1001 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value "(0R)" (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 819 "Net-(R1001-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1002 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value "(0R)" (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 820 "Net-(R1002-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 821 ACCEL-INT))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1101 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 822 DMIC-CLOCK))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 823 "Net-(R1101-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1102 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 560 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 824 "Net-(R1102-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 74 HSL+))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1103 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 560 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 825 "Net-(R1103-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 75 HSL-))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1104 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 560 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 826 "Net-(R1104-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 77 HSR+))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1105 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 560 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 827 "Net-(R1105-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 78 HSR-))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1106 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 560 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 828 "Net-(R1106-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 79 HFL+))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1107 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 560 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 829 "Net-(R1107-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 80 HFL-))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1108 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 560 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 830 "Net-(R1108-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 81 HFR+))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1109 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 560 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 831 "Net-(R1109-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 82 HFR-))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1110 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 560 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 832 "Net-(R1110-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C1101-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1111 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 560 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 833 "Net-(R1111-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C1101-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1201 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 470k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(C1217-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 94 VMMC2))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1202 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 834 GPIO177))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1203 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(C1217-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 834 GPIO177))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1204 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 220R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 835 MIC-BIAS))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(C1212-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1205 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(C1212-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 836 MIC-ECI))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1206 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2k2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(C1213-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 836 MIC-ECI))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1207 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 2k2 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(C1214-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 837 "Net-(R1207-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1208 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(D1204-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1301 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 6k8 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 838 "Net-(R1301-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 839 /ECI/2V5))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1302 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 22k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 840 "Net-(R1302-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 839 /ECI/2V5))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1303 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 32k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 841 "Net-(R1303-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 842 GPIO-ECI1))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1304 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 47k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 842 GPIO-ECI1))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1305 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 47k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 843 GPIO-ECI0))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1306 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 470R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 836 MIC-ECI))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 841 "Net-(R1303-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1307 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 836 MIC-ECI))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 844 "Net-(R1307-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1308 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 22k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 844 "Net-(R1307-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 843 GPIO-ECI0))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1309 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 22k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 838 "Net-(R1301-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1310 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 6k8 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 840 "Net-(R1302-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1311 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 836 MIC-ECI))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 845 ECI-ADC))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1601 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 112 NFC-ANT))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1701 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 150R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 846 "/RFID/NFC Controller/SWP_1_S1"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 847 SWIO-1))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1702 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 150R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 848 "/RFID/NFC Controller/SWP_2_S1"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 849 SWIO-2))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1901 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 4M7 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(C1902-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1902 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10M (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 850 "Net-(R1902-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 851 "Net-(R1902-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1903 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 50k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(C1901-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(C1902-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1904 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 33k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(C1902-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 850 "Net-(R1902-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1905 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 851 "Net-(R1902-Pad2)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 852 UART3-RX_IRRX))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1906 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1M5 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(C1902-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1907 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 1R5 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(D1902-PadA)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R1908 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 22k (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 853 "Net-(R1908-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R2101 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value tbd. (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 854 "Net-(R2101-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R2401 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 10R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C2410-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R2402 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 560R;1% (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C2408-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 855 "Net-(R2402-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R2403 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 560R;1% (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(C2409-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 856 "Net-(R2403-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R2501 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 330R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(D2502-PadA)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 333 "Net-(P-DISP3709-Pad30)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R2502 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value DNP (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 857 PWM_UPPER))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference R2503 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 62R (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 333 "Net-(P-DISP3709-Pad30)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference R2504 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value 62R (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 332 "Net-(P-DISP3709-Pad29)"))
  )
  (module neo900-legacy:SMD-0603 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (tags "SMD 0603 BASED ON VISHAY DIMENSIONS")
    (attr smd)
    (fp_text reference R2801 (at -0.08382 -0.2032) (layer F.SilkS))
    (fp_text value "(0R)" (at -0.33782 0.27178) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.75mm" (at 8.0899 -0.73406) (layer B.SilkS))
    (pad 1 smd rect (at -0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad 2 smd rect (at 0.79756 0) (size 0.59944 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 858 "VBAT(->TPS65950)_UPPER"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3001 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 47R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 859 "Net-(R3001-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 599 "Net-(P3001-Pad1)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3002 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 47R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 859 "Net-(R3001-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 343 CAM-CLK))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3003 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 860 "Net-(R3003-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 861 "Net-(R3003-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3004 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 100R (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 862 "Net-(R3004-Pad1)"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 863 "Net-(R3004-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3201 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value tbd. (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 864 "Net-(R3201-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3202 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value tbd. (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 865 "Net-(R3202-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3203 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value tbd. (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 866 "Net-(R3203-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3204 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value tbd. (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 867 "Net-(R3204-Pad2)"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3301 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value "(0R)" (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 354 VBUS-MODEM-CPU))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 868 VBUS-CPU))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3302 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value "(0R)" (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 355 MODEM-CPU-D-))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 869 OTG-CPU-D-))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3303 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value "(0R)" (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 356 MODEM-CPU-D+))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 870 OTG-CPU-D+))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3401 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 62k1 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 871 "/BB-XM Adapter (CPU)/N$68"))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 164 "/BB-XM Adapter (CPU)/BB-VSYS"))
  )
  (module neo900-legacy:SMD-0402 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (tags "0402 PACKAGE BASED ON VISHAY DIMENSIONS BUT A LITTLE LARGER")
    (attr smd)
    (fp_text reference R3402 (at 0.01016 -0.12192) (layer F.SilkS))
    (fp_text value 30k1 (at 0.06096 0.17272) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.5mm" (at 7.95274 -2.63398) (layer B.SilkS))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 871 "/BB-XM Adapter (CPU)/N$68"))
  )
  (module neo900-legacy:TP-0.75 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT")
    (tags "TEST POINT")
    (attr smd)
    (fp_text reference RING3709 (at 0 0) (layer F.SilkS))
    (fp_text value RING (at 1.33096 0) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 9.32434 -1.13284) (layer B.SilkS))
    (pad P smd circle (at 0 0) (size 0.7493 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 284 RING))
  )
  (module neo900-legacy:TP-0.75 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT")
    (tags "TEST POINT")
    (attr smd)
    (fp_text reference RTS3709 (at 0 0) (layer F.SilkS))
    (fp_text value RTS (at 1.33096 0) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 9.32434 -1.13284) (layer B.SilkS))
    (pad P smd circle (at 0 0) (size 0.7493 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 280 UART?-CTS))
  )
  (module neo900-legacy:TP-0.75 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT")
    (tags "TEST POINT")
    (attr smd)
    (fp_text reference RX3709 (at 0 0) (layer F.SilkS))
    (fp_text value RX (at 1.33096 0) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 9.32434 -1.13284) (layer B.SilkS))
    (pad P smd circle (at 0 0) (size 0.7493 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 285 UART?-TX))
  )
  (module neo900-legacy:LGA-DIL-12+2 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference S1001 (at -1.22174 -1.10744) (layer F.SilkS))
    (fp_text value LIS302DLTR (at -1.01854 -0.52578) (layer F.SilkS))
    (pad 1 smd rect (at -1.99898 0.99822) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 2 smd rect (at -1.19888 0.99822) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at -0.39878 0.99822) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 4 smd rect (at 0.39878 0.99822) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 5 smd rect (at 1.19888 0.99822) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 6 smd rect (at 1.99898 0.99822) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 7 smd rect (at 1.99898 0 90) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 8 smd rect (at 1.99898 -0.99822) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 872 GPIO$55))
    (pad 9 smd rect (at 1.19888 -0.99822) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 873 GPIO$56))
    (pad 10 smd rect (at 0.39878 -0.99822) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 11 smd rect (at -0.39878 -0.99822) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 12 smd rect (at -1.19888 -0.99822) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 13 smd rect (at -1.99898 -0.99822) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 874 I2C3-SDA))
    (pad 14 smd rect (at -1.99898 0 90) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 875 I2C3-SCL))
  )
  (module neo900-legacy:BMG160 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference S1002 (at -0.28194 -1.00076) (layer F.SilkS))
    (fp_text value BMG160 (at -0.07874 1.19634) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 1.29794 90) (size 0.79756 0.3175) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at -0.49784 1.29794 90) (size 0.79756 0.3175) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 3 smd rect (at 0 1.29794 90) (size 0.79756 0.3175) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 4 smd rect (at 0.49784 1.29794 90) (size 0.79756 0.3175) (layers F.Cu F.Paste F.Mask)
      (net 876 GPIO56))
    (pad 5 smd rect (at 0.99822 1.29794 90) (size 0.79756 0.3175) (layers F.Cu F.Paste F.Mask)
      (net 877 "Net-(S1002-Pad5)"))
    (pad 6 smd rect (at 1.29794 0) (size 0.79756 0.3175) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 7 smd rect (at 0.99822 -1.29794 90) (size 0.79756 0.3175) (layers F.Cu F.Paste F.Mask)
      (net 875 I2C3-SCL))
    (pad 8 smd rect (at 0.49784 -1.29794 90) (size 0.79756 0.3175) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 9 smd rect (at 0 -1.29794 90) (size 0.79756 0.3175) (layers F.Cu F.Paste F.Mask)
      (net 874 I2C3-SDA))
    (pad 10 smd rect (at -0.49784 -1.29794 90) (size 0.79756 0.3175) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 11 smd rect (at -0.99822 -1.29794 90) (size 0.79756 0.3175) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 12 smd rect (at -1.29794 0) (size 0.79756 0.3175) (layers F.Cu F.Paste F.Mask)
      (net 878 "Net-(S1002-Pad12)"))
  )
  (module neo900-legacy:BMC150 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "BOSCH SENSORTEC BMC150 PACKAGE")
    (tags "BOSCH SENSORTEC BMC150 PACKAGE")
    (attr smd)
    (fp_text reference S1003 (at 0.55118 0.06096 270) (layer F.SilkS))
    (fp_text value BMC150 (at -0.55118 -0.1143 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.86106 -0.59944) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at -0.86106 -0.19812) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 879 GPIN115))
    (pad 3 smd rect (at -0.86106 0.19812) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 880 "Net-(S1003-Pad3)"))
    (pad 4 smd rect (at -0.86106 0.59944) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 881 GPIO$51))
    (pad 5 smd rect (at -0.39878 0.86106 90) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 882 "Net-(S1003-Pad5)"))
    (pad 6 smd rect (at 0 0.86106 90) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 7 smd rect (at 0.39878 0.86106 90) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 8 smd rect (at 0.86106 0.59944 180) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 9 smd rect (at 0.86106 0.19812) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 10 smd rect (at 0.86106 -0.19812) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 11 smd rect (at 0.86106 -0.59944) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 875 I2C3-SCL))
    (pad 12 smd rect (at 0.39878 -0.86106 90) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 883 "Net-(S1003-Pad12)"))
    (pad 13 smd rect (at 0 -0.86106 90) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 14 smd rect (at -0.39878 -0.86106 90) (size 0.37338 0.22352) (layers F.Cu F.Paste F.Mask)
      (net 874 I2C3-SDA))
  )
  (module neo900-legacy:BNO050 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "BOSCH SENSORTEC BNO050 LGA PACKAGE")
    (tags "BOSCH SENSORTEC BNO050 LGA PACKAGE")
    (attr smd)
    (fp_text reference S1004 (at 0.4826 0.70104 180) (layer F.SilkS))
    (fp_text value BNO055 (at 0.18034 -0.69596 180) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.18mm" (at 5.08 -3.175) (layer B.SilkS))
    (pad 1 smd rect (at 2.2479 1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 2.2479 0.7493 180) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at 2.2479 0.24892 180) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 4 smd rect (at 2.2479 -0.24892) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 884 "Net-(S1004-Pad4)"))
    (pad 5 smd rect (at 2.2479 -0.7493 180) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 6 smd rect (at 2.2479 -1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 7 smd rect (at 1.74752 -1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 8 smd rect (at 1.24968 -1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 9 smd rect (at 0.7493 -1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(C1011-Pad1)"))
    (pad 10 smd rect (at 0.24892 -1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 11 smd rect (at -0.24892 -1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 819 "Net-(R1001-Pad1)"))
    (pad 12 smd rect (at -0.7493 -1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -1.24968 -1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -1.75006 -1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 820 "Net-(R1002-Pad1)"))
    (pad 15 smd rect (at -2.2479 -1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 16 smd rect (at -2.2479 -0.7493 180) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 17 smd rect (at -2.2479 -0.24892 180) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 885 "Net-(S1004-Pad17)"))
    (pad 18 smd rect (at -2.2479 0.24892 180) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 19 smd rect (at -2.2479 0.7493 180) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 875 I2C3-SCL))
    (pad 20 smd rect (at -2.2479 1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 874 I2C3-SDA))
    (pad 21 smd rect (at -1.75006 1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at -1.24968 1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at -0.7493 1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at -0.24892 1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 0.24892 1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 26 smd rect (at 0.7493 1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 886 "Net-(S1004-Pad26)"))
    (pad 27 smd rect (at 1.24968 1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 887 "Net-(S1004-Pad27)"))
    (pad 28 smd rect (at 1.74752 1.55956 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
  )
  (module neo900-legacy:BMP180 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "BOSCH BMP180 BAROMETER")
    (tags "BOSCH BMP180 BAROMETER")
    (attr smd)
    (fp_text reference S1005 (at -0.78232 -1.00076) (layer F.SilkS))
    (fp_text value BMP180 (at -0.48006 1.2954) (layer F.SilkS))
    (pad 1 smd rect (at -1.4986 1.4478 90) (size 0.79756 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 1.4478 90) (size 0.79756 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 3 smd rect (at 1.4986 1.4478 90) (size 0.79756 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 4 smd rect (at 1.4986 -1.4478 90) (size 0.79756 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 -1.4478 90) (size 0.79756 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 875 I2C3-SCL))
    (pad 6 smd rect (at -1.4986 -1.4478 90) (size 0.79756 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 874 I2C3-SDA))
    (pad 7 smd rect (at -1.4986 0 180) (size 0.79756 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:2403-260-00031 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "CONTACT PADS FOR KNOWLES 2403-260-00031 (PETRA) RECEIVER IF USING THE SPRING CONTACTS")
    (tags "CONTACT PADS FOR KNOWLES 2403-260-00031 (PETRA) RECEIVER IF USING THE SPRING CONTACTS")
    (attr smd)
    (fp_text reference SPKR-L3709 (at -0.02286 -5.43306) (layer F.SilkS))
    (fp_text value SPEAKER (at -1.56972 5.69468) (layer F.SilkS))
    (fp_text user "HEIGHT> 2.18mm (should be 2.08mm)" (at 15.3543 -9.63422) (layer B.SilkS))
    (fp_text user "SPACE> 0.0mm (should be 0.1mm)" (at 13.4493 -11.83386) (layer B.SilkS))
    (pad + smd rect (at -3.69824 -1.09982) (size 1.79832 2.59842) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(C1405-Pad2)"))
    (pad - smd rect (at 3.69824 1.09982) (size 1.79832 2.59842) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(C1404-Pad2)"))
  )
  (module neo900-legacy:2403-260-00031 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "CONTACT PADS FOR KNOWLES 2403-260-00031 (PETRA) RECEIVER IF USING THE SPRING CONTACTS")
    (tags "CONTACT PADS FOR KNOWLES 2403-260-00031 (PETRA) RECEIVER IF USING THE SPRING CONTACTS")
    (attr smd)
    (fp_text reference SPKR-R3709 (at -0.02286 -5.43306) (layer F.SilkS))
    (fp_text value SPEAKER (at -1.56972 5.69468) (layer F.SilkS))
    (fp_text user "HEIGHT> 2.18mm (should be 2.08mm)" (at 15.3543 -9.63422) (layer B.SilkS))
    (fp_text user "SPACE> 0.0mm (should be 0.1mm)" (at 13.4493 -11.83386) (layer B.SilkS))
    (pad + smd rect (at -3.69824 -1.09982) (size 1.79832 2.59842) (layers F.Cu F.Paste F.Mask)
      (net 108 "/Audio Handsfree/SPKRR+"))
    (pad - smd rect (at 3.69824 1.09982) (size 1.79832 2.59842) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(C1410-Pad1)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference SPKRL+3709 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(C1405-Pad2)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference SPKRL-3709 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(C1404-Pad2)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference SPKRR+3709 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 108 "/Audio Handsfree/SPKRR+"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference SPKRR-3709 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(C1410-Pad1)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference STATUS3709 (at 0 0) (layer F.SilkS))
    (fp_text value STATUS (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 256 STATUS))
  )
  (module neo900-legacy:SC88A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "ÄHNLICH SOT23-5 ABER KLEINER")
    (tags "ÄHNLICH SOT23-5 ABER KLEINER")
    (attr smd)
    (fp_text reference T601 (at 0.1143 -0.70104) (layer F.SilkS))
    (fp_text value UMG5N (at 0.0127 -0.25146) (layer F.SilkS))
    (pad 1 smd rect (at -0.6477 0.83566) (size 0.29972 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 193 GPIO-MODEM_IGT))
    (pad 2 smd rect (at 0 0.83566) (size 0.29972 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at 0.6477 0.83566) (size 0.29972 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 888 GPIO-MODEM_EMERG))
    (pad 4 smd rect (at 0.6477 -0.83566) (size 0.29972 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 281 EMERG_OFF))
    (pad 5 smd rect (at -0.6477 -0.83566) (size 0.29972 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 269 "/3G/4G Modem + SIM/ON_KEY"))
  )
  (module neo900-legacy:SC89-3 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference T1901 (at -0.1143 0.80264 180) (layer F.SilkS))
    (fp_text value T-PMOS-FDY100PZ (at -0.0127 0.35052 180) (layer F.SilkS))
    (pad 1 smd rect (at 0.49784 -0.56896) (size 0.49784 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 889 BQ.GPIO))
    (pad 2 smd rect (at -0.49784 -0.56896) (size 0.49784 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(C1901-Pad2)"))
    (pad 3 smd rect (at 0 0.56896) (size 0.49784 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 853 "Net-(R1908-Pad2)"))
  )
  (module neo900-legacy:SC88A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "ÄHNLICH SOT23-5 ABER KLEINER")
    (tags "ÄHNLICH SOT23-5 ABER KLEINER")
    (attr smd)
    (fp_text reference T1902 (at 0.1143 -0.70104) (layer F.SilkS))
    (fp_text value UMG5N (at 0.0127 -0.25146) (layer F.SilkS))
    (pad 1 smd rect (at -0.6477 0.83566) (size 0.29972 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(C1903-Pad2)"))
    (pad 2 smd rect (at 0 0.83566) (size 0.29972 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at 0.6477 0.83566) (size 0.29972 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(C1904-Pad2)"))
    (pad 4 smd rect (at 0.6477 -0.83566) (size 0.29972 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(D1902-PadK)"))
    (pad 5 smd rect (at -0.6477 -0.83566) (size 0.29972 0.49784) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(D1902-PadK)"))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP1 (at 0 0) (layer F.SilkS))
    (fp_text value GND (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference TP2 (at 0 0) (layer F.SilkS))
    (fp_text value EMERG (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 281 EMERG_OFF))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP3 (at 0 0) (layer F.SilkS))
    (fp_text value GND (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP4 (at 0 0) (layer F.SilkS))
    (fp_text value GND (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP5 (at 0 0) (layer F.SilkS))
    (fp_text value GND (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP6 (at 0 0) (layer F.SilkS))
    (fp_text value UART_CTS (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 890 /Hackerbus/UART3_CTS))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP7 (at 0 0) (layer F.SilkS))
    (fp_text value UART_TX (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 891 /Hackerbus/UART3_TX))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP8 (at 0 0) (layer F.SilkS))
    (fp_text value GPIO_b (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 892 /Hackerbus/N$341))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP9 (at 0 0) (layer F.SilkS))
    (fp_text value GPIO_d (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 893 /Hackerbus/N$340))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP10 (at 0 0) (layer F.SilkS))
    (fp_text value GPIO_f/3V3 (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 894 /Hackerbus/N$339))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP11 (at 0 0) (layer F.SilkS))
    (fp_text value VBUS (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 29 VBUS))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP12 (at 0 0) (layer F.SilkS))
    (fp_text value VBAT (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 42 BATT))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP13 (at 0 0) (layer F.SilkS))
    (fp_text value UART_RTS (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 895 /Hackerbus/UART3_RTS))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP14 (at 0 0) (layer F.SilkS))
    (fp_text value UART_RX (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 896 /Hackerbus/UART3_RX))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP15 (at 0 0) (layer F.SilkS))
    (fp_text value GPIO_a (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 897 /Hackerbus/N$347))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP16 (at 0 0) (layer F.SilkS))
    (fp_text value GPIO_c (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 898 /Hackerbus/N$349))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP17 (at 0 0) (layer F.SilkS))
    (fp_text value GPIO_e (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 899 /Hackerbus/N$351))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP18 (at 0 0) (layer F.SilkS))
    (fp_text value VSYS (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 34 VSYS))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP19 (at 0 0) (layer F.SilkS))
    (fp_text value VBAT (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 42 BATT))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP20 (at 0 0) (layer F.SilkS))
    (fp_text value USB_DP (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 167 USB-WWAN-D+))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP21 (at 0 0) (layer F.SilkS))
    (fp_text value USB_GND (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP22 (at 0 0) (layer F.SilkS))
    (fp_text value USB_DM (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 168 USB-WWAN-D-))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP25 (at 0 0) (layer F.SilkS))
    (fp_text value NFC_GND (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP26 (at 0 0) (layer F.SilkS))
    (fp_text value NFC_ANT (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 112 NFC-ANT))
  )
  (module neo900-legacy:1PIN-1.5-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (tags "TEST POINT TO OPTIONALY SOLDER A WIRE TO IT")
    (attr virtual)
    (fp_text reference TP1401 (at 0 0) (layer F.SilkS))
    (fp_text value LOOP+ (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 175 "/WLAN, Bluetooth, FM/LOOP"))
  )
  (module neo900-legacy:1PIN-1.5SQ-0.8 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr virtual)
    (fp_text reference TP1402 (at 0 0) (layer F.SilkS))
    (fp_text value LOOP- (at 5.08 0) (layer F.SilkS))
    (fp_text user "SPACE> -1.0mm" (at 7.75462 -2.23266) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.4986 1.4986) (drill 0.79756) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:TP-0.75 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEST POINT")
    (tags "TEST POINT")
    (attr smd)
    (fp_text reference TX3709 (at 0 0) (layer F.SilkS))
    (fp_text value TX (at 1.33096 0) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.035mm" (at 9.32434 -1.13284) (layer B.SilkS))
    (pad P smd circle (at 0 0) (size 0.7493 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 286 UART?-RX))
  )
  (module neo900-legacy:SOT457-6 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SOT457 6 LEADS = SC74 = TSOP6")
    (tags "SOT457 6 LEADS = SC74 = TSOP6")
    (attr smd)
    (fp_text reference U201 (at -0.4826 -0.60198) (layer F.SilkS))
    (fp_text value IP4220CZ6 (at -0.5842 -0.1524) (layer F.SilkS))
    (pad 1 smd rect (at -0.94996 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 360 OTG-ID))
    (pad 2 smd rect (at 0 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at 0.94742 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 359 OTG-D+))
    (pad 4 smd rect (at 0.94742 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 358 OTG-D-))
    (pad 5 smd rect (at 0 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 900 "Net-(U201-Pad5)"))
    (pad 6 smd rect (at -0.94996 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 29 VBUS))
  )
  (module neo900-legacy:S-PVQFN-N24-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "RGE (S-PVQFN-N24)")
    (tags "RGE (S-PVQFN-N24)")
    (attr smd)
    (fp_text reference U301 (at -0.38354 -1.65354) (layer F.SilkS))
    (fp_text value BQ24297RGE (at -0.68834 -0.93218) (layer F.SilkS))
    (pad 1 smd rect (at -1.24968 1.99898 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 29 VBUS))
    (pad 2 smd rect (at -0.7493 1.99898 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 359 OTG-D+))
    (pad 3 smd rect (at -0.24892 1.99898 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 358 OTG-D-))
    (pad 4 smd rect (at 0.24892 1.99898 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 254 CHG_IND))
    (pad 5 smd rect (at 0.7493 1.99898 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 875 I2C3-SCL))
    (pad 6 smd rect (at 1.24968 1.99898 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 874 I2C3-SDA))
    (pad 7 smd rect (at 1.99898 1.24968 180) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 901 "Net-(U301-Pad7)"))
    (pad 8 smd rect (at 1.99898 0.7493 180) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 902 "Net-(U301-Pad8)"))
    (pad 9 smd rect (at 1.99898 0.24892 180) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 903 "Net-(U301-Pad9)"))
    (pad 10 smd rect (at 1.99898 -0.24892 180) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 801 "Net-(R301-Pad2)"))
    (pad 11 smd rect (at 1.99898 -0.7493 180) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 802 BATTEMP))
    (pad 12 smd rect (at 1.99898 -1.24968 180) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 904 "Net-(U301-Pad12)"))
    (pad 13 smd rect (at 1.24968 -1.99898 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 42 BATT))
    (pad 14 smd rect (at 0.7493 -1.99898 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 42 BATT))
    (pad 15 smd rect (at 0.24892 -1.99898 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 16 smd rect (at -0.24892 -1.99898 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 17 smd rect (at -0.7493 -1.99898 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 18 smd rect (at -1.24968 -1.99898 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 19 smd rect (at -1.99898 -1.24968) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C301-Pad1)"))
    (pad 20 smd rect (at -1.99898 -0.7493) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C301-Pad1)"))
    (pad 21 smd rect (at -1.99898 -0.24892) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C301-Pad2)"))
    (pad 22 smd rect (at -1.99898 0.24892) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C305-Pad1)"))
    (pad 23 smd rect (at -1.99898 0.7493) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C303-Pad2)"))
    (pad 24 smd rect (at -1.99898 1.24968) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 29 VBUS))
    (pad E smd rect (at 0 0) (size 2.69748 2.69748) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:R-XBGA-N6-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TI YZP")
    (tags "TI YZP")
    (attr smd)
    (fp_text reference U401 (at -0.2413 -0.14478 90) (layer F.SilkS))
    (fp_text value TPS22963CYZP (at 0.09652 -0.04318 90) (layer F.SilkS))
    (pad A1 smd circle (at 0.24892 0.49784 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
    (pad A2 smd circle (at -0.24892 0.49784 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad B1 smd circle (at 0.24892 0 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
    (pad B2 smd circle (at -0.24892 0 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad C1 smd circle (at 0.24892 -0.49784 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C2 smd circle (at -0.24892 -0.49784 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 905 GPIO-EN-MODEM))
  )
  (module neo900-legacy:R-XBGA-N12-0.4 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TI YFF (SOME SIZE)")
    (tags "TI YFF (SOME SIZE)")
    (attr smd)
    (fp_text reference U402 (at 0.0635 -0.50292) (layer F.SilkS))
    (fp_text value INA231YFF (at -0.18796 -0.0254) (layer F.SilkS))
    (pad A1 smd circle (at -0.59944 0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad A2 smd circle (at -0.59944 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 369 I2C2-SDA))
    (pad A3 smd circle (at -0.59944 -0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 906 INA231-INT))
    (pad B1 smd circle (at -0.19812 0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
    (pad B2 smd circle (at -0.19812 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask))
    (pad B3 smd circle (at -0.19812 -0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad C1 smd circle (at 0.19812 0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C2 smd circle (at 0.19812 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask))
    (pad C3 smd circle (at 0.19812 -0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad D1 smd circle (at 0.59944 0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
    (pad D2 smd circle (at 0.59944 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C402-Pad1)"))
    (pad D3 smd circle (at 0.59944 -0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C401-Pad1)"))
  )
  (module neo900-legacy:R-XBGA-N12-0.4 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TI YFF (SOME SIZE)")
    (tags "TI YFF (SOME SIZE)")
    (attr smd)
    (fp_text reference U403 (at 0.0635 -0.50292) (layer F.SilkS))
    (fp_text value INA231YFF (at -0.18796 -0.0254) (layer F.SilkS))
    (pad A1 smd circle (at -0.59944 0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad A2 smd circle (at -0.59944 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 369 I2C2-SDA))
    (pad A3 smd circle (at -0.59944 -0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 906 INA231-INT))
    (pad B1 smd circle (at -0.19812 0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
    (pad B2 smd circle (at -0.19812 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask))
    (pad B3 smd circle (at -0.19812 -0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 369 I2C2-SDA))
    (pad C1 smd circle (at 0.19812 0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C2 smd circle (at 0.19812 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask))
    (pad C3 smd circle (at 0.19812 -0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad D1 smd circle (at 0.59944 0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
    (pad D2 smd circle (at 0.59944 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C404-Pad1)"))
    (pad D3 smd circle (at 0.59944 -0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C403-Pad1)"))
  )
  (module neo900-legacy:R-XBGA-N12-0.4 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TI YFF (SOME SIZE)")
    (tags "TI YFF (SOME SIZE)")
    (attr smd)
    (fp_text reference U404 (at 0.0635 -0.50292) (layer F.SilkS))
    (fp_text value INA231YFF (at -0.18796 -0.0254) (layer F.SilkS))
    (pad A1 smd circle (at -0.59944 0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad A2 smd circle (at -0.59944 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 369 I2C2-SDA))
    (pad A3 smd circle (at -0.59944 -0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 906 INA231-INT))
    (pad B1 smd circle (at -0.19812 0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
    (pad B2 smd circle (at -0.19812 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask))
    (pad B3 smd circle (at -0.19812 -0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
    (pad C1 smd circle (at 0.19812 0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C2 smd circle (at 0.19812 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask))
    (pad C3 smd circle (at 0.19812 -0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad D1 smd circle (at 0.59944 0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 803 "/Modem Power/VMODEM"))
    (pad D2 smd circle (at 0.59944 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C406-Pad1)"))
    (pad D3 smd circle (at 0.59944 -0.39878) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C405-Pad1)"))
  )
  (module neo900-legacy:S-PVSON-N10-4X3 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "S-PVSON-N10 FOR 4X3MM PACKAGE")
    (tags "S-PVSON-N10 FOR 4X3MM PACKAGE")
    (attr smd)
    (fp_text reference U501 (at -0.508 -2.79908) (layer F.SilkS))
    (fp_text value BQ27200DRK (at -0.20828 2.89814) (layer F.SilkS))
    (pad 1 smd oval (at -0.99822 1.97358 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C503-Pad1)"))
    (pad 2 smd oval (at -0.49784 1.97358 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C502-Pad1)"))
    (pad 3 smd oval (at 0 1.97358 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 4 smd oval (at 0.49784 1.97358 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad 5 smd oval (at 0.99822 1.97358 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 369 I2C2-SDA))
    (pad 6 smd oval (at 0.99822 -1.97358 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C506-Pad1)"))
    (pad 7 smd oval (at 0.49784 -1.97358 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C504-Pad1)"))
    (pad 8 smd oval (at 0 -1.97358 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C505-Pad1)"))
    (pad 9 smd oval (at -0.49784 -1.97358 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 889 BQ.GPIO))
    (pad 10 smd oval (at -0.99822 -1.97358 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 800 "Net-(PGM3709-PadP$1)"))
    (pad EXP smd oval (at 0 0) (size 2.99974 2.64922) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:S-XBGA-N9-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TI YZF")
    (tags "TI YZF")
    (attr smd)
    (fp_text reference U502 (at -0.2413 -0.14478 90) (layer F.SilkS))
    (fp_text value "BQ27421YZFR-G1A (4V2)" (at 0.09652 -0.04318 90) (layer F.SilkS))
    (pad A1 smd circle (at 0.49784 0.49784 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 907 "Net-(U502-PadA1)"))
    (pad A2 smd circle (at 0 0.49784 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 874 I2C3-SDA))
    (pad A3 smd circle (at -0.49784 0.49784 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 875 I2C3-SCL))
    (pad B1 smd circle (at 0.49784 0 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 805 BATTID))
    (pad B2 smd circle (at 0 0 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad B3 smd circle (at -0.49784 0 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C508-Pad1)"))
    (pad C1 smd circle (at 0.49784 -0.49784 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad C2 smd circle (at 0 -0.49784 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 42 BATT))
    (pad C3 smd circle (at -0.49784 -0.49784 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(BATT+3709-PadP)"))
  )
  (module neo900-legacy:SOT666IP (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SOT666 WITH INTERNAL PAD")
    (tags "SOT666 WITH INTERNAL PAD")
    (attr smd)
    (fp_text reference U601 (at 0.31496 -0.2032) (layer F.SilkS))
    (fp_text value ESDA6V1-5P6 (at 0.21336 0.24638) (layer F.SilkS))
    (pad 1 smd rect (at -0.49784 0.60452) (size 0.29972 0.58928) (layers F.Cu F.Paste F.Mask)
      (net 276 MODEM-CD_A))
    (pad 2 smd rect (at 0 0.39878) (size 0.29972 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at 0.49784 0.60452) (size 0.29972 0.58928) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C611-Pad1)"))
    (pad 4 smd rect (at 0.49784 -0.60452) (size 0.29972 0.58928) (layers F.Cu F.Paste F.Mask)
      (net 367 SIM-DATA))
    (pad 5 smd rect (at 0 -0.60452) (size 0.29972 0.58928) (layers F.Cu F.Paste F.Mask)
      (net 54 SIM-RST))
    (pad 6 smd rect (at -0.49784 -0.60452) (size 0.29972 0.58928) (layers F.Cu F.Paste F.Mask)
      (net 366 SIM-CLK))
  )
  (module neo900-legacy:S-PWQFN-N20-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TI RTJ (S-PWQFN-N20)")
    (tags "TI RTJ (S-PWQFN-N20)")
    (attr smd)
    (fp_text reference U701 (at -0.28448 -1.35382) (layer F.SilkS))
    (fp_text value "FSA2866UMX(CHECK0.5VS0.4PITCH)" (at -0.49022 -0.63246) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 908 "/Dual SIM switch/N$344"))
    (pad 2 smd rect (at -0.49784 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 909 "/Dual SIM switch/N$353"))
    (pad 3 smd rect (at 0 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 267 MODEM_RST_A))
    (pad 4 smd rect (at 0.49784 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 268 MODEM_CLK_A))
    (pad 5 smd rect (at 0.99822 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 266 MODEM_DATA_A))
    (pad 6 smd rect (at 1.89992 0.99822 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 910 "/Dual SIM switch/N$354"))
    (pad 7 smd rect (at 1.89992 0.49784 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 911 "/Dual SIM switch/MODEM_RST_B"))
    (pad 8 smd rect (at 1.89992 0 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 912 "/Dual SIM switch/MODEM_CLK_B"))
    (pad 9 smd rect (at 1.89992 -0.49784 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 913 "/Dual SIM switch/MODEM_DATA_B"))
    (pad 10 smd rect (at 1.89992 -0.99822 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 11 smd rect (at 0.99822 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 12 smd rect (at 0.49784 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 364 "/Dual SIM switch/N$342"))
    (pad 13 smd rect (at 0 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 363 "/Dual SIM switch/N$137"))
    (pad 14 smd rect (at -0.49784 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 362 "/Dual SIM switch/N$224"))
    (pad 15 smd rect (at -0.99822 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 365 "/Dual SIM switch/N$338"))
    (pad 16 smd rect (at -1.89992 -0.99822) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 367 SIM-DATA))
    (pad 17 smd rect (at -1.89992 -0.49784) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 366 SIM-CLK))
    (pad 18 smd rect (at -1.89992 0) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 54 SIM-RST))
    (pad 19 smd rect (at -1.89992 0.49784) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 276 MODEM-CD_A))
    (pad 20 smd rect (at -1.89992 0.99822) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 914 "/Dual SIM switch/N$343"))
    (pad E smd rect (at 0.02794 -0.0381) (size 2.14884 2.14884) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:S-PWQFN-N20-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TI RTJ (S-PWQFN-N20)")
    (tags "TI RTJ (S-PWQFN-N20)")
    (attr smd)
    (fp_text reference U702 (at -0.28448 -1.35382) (layer F.SilkS))
    (fp_text value "FSA2866UMX(CHECK0.5VS0.4PITCH)" (at -0.49022 -0.63246) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 915 "/Dual SIM switch/N$352"))
    (pad 2 smd rect (at -0.49784 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 916 "/Dual SIM switch/N$20"))
    (pad 3 smd rect (at 0 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 917 "/Dual SIM switch/N$40"))
    (pad 4 smd rect (at 0.49784 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 918 "/Dual SIM switch/N$65"))
    (pad 5 smd rect (at 0.99822 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 919 "/Dual SIM switch/N$53"))
    (pad 6 smd rect (at 1.89992 0.99822 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 920 "Net-(U702-Pad6)"))
    (pad 7 smd rect (at 1.89992 0.49784 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 921 "Net-(U702-Pad7)"))
    (pad 8 smd rect (at 1.89992 0 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 922 "Net-(U702-Pad8)"))
    (pad 9 smd rect (at 1.89992 -0.49784 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 923 "Net-(U702-Pad9)"))
    (pad 10 smd rect (at 1.89992 -0.99822 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 11 smd rect (at 0.99822 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 12 smd rect (at 0.49784 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 364 "/Dual SIM switch/N$342"))
    (pad 13 smd rect (at 0 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 363 "/Dual SIM switch/N$137"))
    (pad 14 smd rect (at -0.49784 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 362 "/Dual SIM switch/N$224"))
    (pad 15 smd rect (at -0.99822 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 365 "/Dual SIM switch/N$338"))
    (pad 16 smd rect (at -1.89992 -0.99822) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 367 SIM-DATA))
    (pad 17 smd rect (at -1.89992 -0.49784) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 366 SIM-CLK))
    (pad 18 smd rect (at -1.89992 0) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 54 SIM-RST))
    (pad 19 smd rect (at -1.89992 0.49784) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 276 MODEM-CD_A))
    (pad 20 smd rect (at -1.89992 0.99822) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 924 "/Dual SIM switch/N$346"))
    (pad E smd rect (at 0.02794 -0.0381) (size 2.14884 2.14884) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:TSNP-7-10 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "INFINEON TSNP-7-10")
    (tags "INFINEON TSNP-7-10")
    (attr smd)
    (fp_text reference U801 (at 0.2159 -0.40132) (layer F.SilkS))
    (fp_text value BGM1034N7 (at 0.4191 0.19558) (layer F.SilkS))
    (pad 1 smd oval (at -0.53848 1.08966 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 55 VGNSS))
    (pad 2 smd oval (at 0 1.08966 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 55 VGNSS))
    (pad 3 smd oval (at 0.53848 1.08966 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(GPS-ANT3709-Pad1)"))
    (pad 4 smd oval (at 0.53848 -1.08966 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(L801-Pad2)"))
    (pad 5 smd oval (at 0 -1.08966 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(L801-Pad1)"))
    (pad 6 smd oval (at -0.53848 -1.08966 270) (size 0.49784 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 925 "/Antenna connections/ANT-GNSS"))
    (pad 7 smd oval (at 0 0) (size 1.41986 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:SC70-6 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr SC70-6)
    (tags SC70-6)
    (attr smd)
    (fp_text reference U802 (at 0.1143 -0.2032) (layer F.SilkS))
    (fp_text value PE4259 (at -0.13716 0.27178) (layer F.SilkS))
    (pad 1 smd rect (at -0.6477 1.09982 90) (size 0.89916 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 0 1.09982 90) (size 0.89916 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at 0.6477 1.09982 90) (size 0.89916 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 925 "/Antenna connections/ANT-GNSS"))
    (pad 4 smd rect (at 0.6477 -1.09982 90) (size 0.89916 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 926 GPIO$70))
    (pad 5 smd rect (at 0 -1.09982 90) (size 0.89916 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 261 GNSS-IN))
    (pad 6 smd rect (at -0.6477 -1.09982 90) (size 0.89916 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
  )
  (module neo900-legacy:SOT23-6 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SOT23 WITH 6 PINS")
    (tags "SOT23 WITH 6 PINS")
    (attr smd)
    (fp_text reference U803 (at -0.4826 -0.60198) (layer F.SilkS))
    (fp_text value CPL-WBF-00D3-WRONGPACK (at -0.5842 -0.1524) (layer F.SilkS))
    (pad 1 smd rect (at -0.94996 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C803-Pad1)"))
    (pad 2 smd rect (at 0 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 927 "Net-(U803-Pad2)"))
    (pad 3 smd rect (at 0.94742 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 265 GSM-ANT-TRX))
    (pad 4 smd rect (at 0.94742 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 5 smd rect (at 0 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 6 smd rect (at -0.94996 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 928 "Net-(U803-Pad6)"))
  )
  (module neo900-legacy:SOT23-6 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SOT23 WITH 6 PINS")
    (tags "SOT23 WITH 6 PINS")
    (attr smd)
    (fp_text reference U804 (at -0.4826 -0.60198) (layer F.SilkS))
    (fp_text value LMV221SD-WRONGPACK (at -0.5842 -0.1524) (layer F.SilkS))
    (pad 1 smd rect (at -0.94996 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 61 2V7))
    (pad 2 smd rect (at 0 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 927 "Net-(U803-Pad2)"))
    (pad 3 smd rect (at 0.94742 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 4 smd rect (at 0.94742 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 929 N$229))
    (pad 5 smd rect (at 0 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 930 "Net-(U804-Pad5)"))
    (pad 6 smd rect (at -0.94996 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 807 "Net-(R806-Pad1)"))
  )
  (module neo900-legacy:SOT23-6 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SOT23 WITH 6 PINS")
    (tags "SOT23 WITH 6 PINS")
    (attr smd)
    (fp_text reference U805 (at -0.4826 -0.60198) (layer F.SilkS))
    (fp_text value LMV221SD-WRONGPACK (at -0.5842 -0.1524) (layer F.SilkS))
    (pad 1 smd rect (at -0.94996 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 61 2V7))
    (pad 2 smd rect (at 0 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 928 "Net-(U803-Pad6)"))
    (pad 3 smd rect (at 0.94742 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 4 smd rect (at 0.94742 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 931 N$19))
    (pad 5 smd rect (at 0 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 932 "Net-(U805-Pad5)"))
    (pad 6 smd rect (at -0.94996 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 808 "Net-(R807-Pad1)"))
  )
  (module neo900-legacy:SC70-6 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr SC70-6)
    (tags SC70-6)
    (attr smd)
    (fp_text reference U806 (at 0.1143 -0.2032) (layer F.SilkS))
    (fp_text value LTC5508 (at -0.13716 0.27178) (layer F.SilkS))
    (pad 1 smd rect (at -0.6477 1.09982 90) (size 0.89916 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 933 GPIO$110))
    (pad 2 smd rect (at 0 1.09982 90) (size 0.89916 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at 0.6477 1.09982 90) (size 0.89916 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 934 ADC$114))
    (pad 4 smd rect (at 0.6477 -1.09982 90) (size 0.89916 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 5 smd rect (at 0 -1.09982 90) (size 0.89916 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 6 smd rect (at -0.6477 -1.09982 90) (size 0.89916 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C803-Pad2)"))
  )
  (module neo900-legacy:NONE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (tags "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (attr virtual)
    (fp_text reference U807 (at 0 0) (layer F.SilkS))
    (fp_text value Comparator (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:QFN-16+4+E-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "QFN20 FOR SI47XX")
    (tags "QFN20 FOR SI47XX")
    (attr smd)
    (fp_text reference U902 (at 1.30302 -0.4826 270) (layer F.SilkS))
    (fp_text value SI4721BG (at 0.60198 -0.2794 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.26492 -1.26492) (size 0.33782 0.33782) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.35382 -0.7493) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C901-Pad2)"))
    (pad 3 smd rect (at -1.35382 -0.24892) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 4 smd rect (at -1.35382 0.24892) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(L901-Pad2)"))
    (pad 5 smd rect (at -1.35382 0.7493) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 935 NRESWARM))
    (pad 6 smd rect (at -1.26492 1.26492) (size 0.33782 0.33782) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 7 smd rect (at -0.7493 1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad 8 smd rect (at -0.24892 1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 369 I2C2-SDA))
    (pad 9 smd rect (at 0.24892 1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 303 32KHZ))
    (pad 10 smd rect (at 0.7493 1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 11 smd rect (at 1.26492 1.26492) (size 0.33782 0.33782) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 12 smd rect (at 1.35382 0.7493) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 13 smd rect (at 1.35382 0.24892) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 813 "Net-(R903-Pad1)"))
    (pad 14 smd rect (at 1.35382 -0.24892) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 809 "Net-(R901-Pad1)"))
    (pad 15 smd rect (at 1.35382 -0.7493) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 815 "Net-(R905-Pad1)"))
    (pad 16 smd rect (at 1.26492 -1.26492) (size 0.33782 0.33782) (layers F.Cu F.Paste F.Mask)
      (net 817 "Net-(R906-Pad1)"))
    (pad 17 smd rect (at 0.7493 -1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 811 "Net-(R902-Pad1)"))
    (pad 18 smd rect (at 0.24892 -1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 936 "Net-(U902-Pad18)"))
    (pad 19 smd rect (at -0.24892 -1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 937 "Net-(U902-Pad19)"))
    (pad 20 smd rect (at -0.7493 -1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask))
    (pad EXP smd rect (at 0 0) (size 1.69926 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:S-PBGA-N87-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "S-PBGA-N87 (ZAS) IN 0.5MM PITCH; TLV320AIC34")
    (tags "S-PBGA-N87 (ZAS) IN 0.5MM PITCH; TLV320AIC34")
    (attr smd)
    (fp_text reference U1101 (at 0 0) (layer F.SilkS))
    (fp_text value tlv320aic34 (at 0 0) (layer F.SilkS))
    (pad A1 smd circle (at -2.49936 -2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 938 "Net-(U1101-PadA1)"))
    (pad A2 smd circle (at -1.99898 -2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 833 "Net-(R1111-Pad1)"))
    (pad A3 smd circle (at -1.4986 -2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 832 "Net-(R1110-Pad1)"))
    (pad A4 smd circle (at -0.99822 -2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C1104-Pad1)"))
    (pad A5 smd circle (at -0.49784 -2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 939 "Net-(U1101-PadA5)"))
    (pad A6 smd circle (at 0 -2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 940 "Net-(U1101-PadA6)"))
    (pad A7 smd circle (at 0.49784 -2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 941 EAR-))
    (pad A8 smd circle (at 0.99822 -2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 942 EAR+))
    (pad A9 smd circle (at 1.4986 -2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C1104-Pad1)"))
    (pad A10 smd circle (at 1.99898 -2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A11 smd circle (at 2.49936 -2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B1 smd circle (at -2.49936 -1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 943 "Net-(U1101-PadB1)"))
    (pad B3 smd circle (at -1.4986 -1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C1102-Pad1)"))
    (pad B4 smd circle (at -0.99822 -1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C1104-Pad1)"))
    (pad B5 smd circle (at -0.49784 -1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 826 "Net-(R1104-Pad1)"))
    (pad B6 smd circle (at 0 -1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 827 "Net-(R1105-Pad1)"))
    (pad B7 smd circle (at 0.49784 -1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 825 "Net-(R1103-Pad1)"))
    (pad B8 smd circle (at 0.99822 -1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 824 "Net-(R1102-Pad1)"))
    (pad B9 smd circle (at 1.4986 -1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C1104-Pad1)"))
    (pad B10 smd circle (at 1.99898 -1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 944 DMIC-BIAS))
    (pad B11 smd circle (at 2.49936 -1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 945 MICBIAS))
    (pad C1 smd circle (at -2.49936 -1.4986) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 946 "Net-(U1101-PadC1)"))
    (pad C2 smd circle (at -1.99898 -1.4986) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 828 "Net-(R1106-Pad1)"))
    (pad C10 smd circle (at 1.99898 -1.4986) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 947 "Net-(U1101-PadC10)"))
    (pad C11 smd circle (at 2.49936 -1.4986) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 948 "Net-(U1101-PadC11)"))
    (pad D1 smd circle (at -2.49936 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 949 "Net-(U1101-PadD1)"))
    (pad D2 smd circle (at -1.99898 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 829 "Net-(R1107-Pad1)"))
    (pad D4 smd circle (at -0.99822 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D5 smd circle (at -0.49784 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D6 smd circle (at 0 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D7 smd circle (at 0.49784 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D8 smd circle (at 0.99822 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad D10 smd circle (at 1.99898 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D11 smd circle (at 2.49936 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E1 smd circle (at -2.49936 -0.49784) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 950 "Net-(U1101-PadE1)"))
    (pad E2 smd circle (at -1.99898 -0.49784) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 830 "Net-(R1108-Pad1)"))
    (pad E4 smd circle (at -0.99822 -0.49784) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad E8 smd circle (at 0.99822 -0.49784) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad E10 smd circle (at 1.99898 -0.49784) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 951 "Net-(U1101-PadE10)"))
    (pad E11 smd circle (at 2.49936 -0.49784) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C1101-Pad2)"))
    (pad F1 smd circle (at -2.49936 0) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 952 "Net-(U1101-PadF1)"))
    (pad F2 smd circle (at -1.99898 0) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 831 "Net-(R1109-Pad1)"))
    (pad F4 smd circle (at -0.99822 0) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad F8 smd circle (at 0.99822 0) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad F10 smd circle (at 1.99898 0) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 953 FM-R-OUT))
    (pad F11 smd circle (at 2.49936 0) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C1101-Pad1)"))
    (pad G1 smd circle (at -2.49936 0.49784) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 954 N$129))
    (pad G2 smd circle (at -1.99898 0.49784) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 954 N$129))
    (pad G4 smd circle (at -0.99822 0.49784) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G8 smd circle (at 0.99822 0.49784) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad G10 smd circle (at 1.99898 0.49784) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 955 "Net-(U1101-PadG10)"))
    (pad G11 smd circle (at 2.49936 0.49784) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 956 "Net-(U1101-PadG11)"))
    (pad H1 smd circle (at -2.49936 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 957 "Net-(U1101-PadH1)"))
    (pad H2 smd circle (at -1.99898 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 958 DMIC-DATA))
    (pad H4 smd circle (at -0.99822 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad H5 smd circle (at -0.49784 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad H6 smd circle (at 0 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad H7 smd circle (at 0.49784 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C1107-Pad1)"))
    (pad H8 smd circle (at 0.99822 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad H10 smd circle (at 1.99898 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 959 FM-L-OUT))
    (pad H11 smd circle (at 2.49936 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 960 "Net-(U1101-PadH11)"))
    (pad J1 smd circle (at -2.49936 1.4986) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 961 "Net-(U1101-PadJ1)"))
    (pad J2 smd circle (at -1.99898 1.4986) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 823 "Net-(R1101-Pad2)"))
    (pad J10 smd circle (at 1.99898 1.4986) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J11 smd circle (at 2.49936 1.4986) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K1 smd circle (at -2.49936 1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C1107-Pad1)"))
    (pad K2 smd circle (at -1.99898 1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 962 N$148))
    (pad K3 smd circle (at -1.4986 1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 963 N$153))
    (pad K4 smd circle (at -0.99822 1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 964 N$154))
    (pad K5 smd circle (at -0.49784 1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 965 N$149))
    (pad K6 smd circle (at 0 1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 966 N$150))
    (pad K7 smd circle (at 0.49784 1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C1107-Pad1)"))
    (pad K8 smd circle (at 0.99822 1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 967 "Net-(U1101-PadK8)"))
    (pad K9 smd circle (at 1.4986 1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 96 MIC+))
    (pad K10 smd circle (at 1.99898 1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K11 smd circle (at 2.49936 1.99898) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L1 smd circle (at -2.49936 2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 968 "Net-(U1101-PadL1)"))
    (pad L2 smd circle (at -1.99898 2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 969 "Net-(U1101-PadL2)"))
    (pad L3 smd circle (at -1.4986 2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 970 "Net-(U1101-PadL3)"))
    (pad L4 smd circle (at -0.99822 2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 971 "Net-(U1101-PadL4)"))
    (pad L5 smd circle (at -0.49784 2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 972 "Net-(U1101-PadL5)"))
    (pad L6 smd circle (at 0 2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 369 I2C2-SDA))
    (pad L7 smd circle (at 0.49784 2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 973 "Net-(U1101-PadL7)"))
    (pad L8 smd circle (at 0.99822 2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 974 "Net-(U1101-PadL8)"))
    (pad L9 smd circle (at 1.4986 2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad L10 smd circle (at 1.99898 2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 98 MIC-))
    (pad L11 smd circle (at 2.49936 2.49936) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 975 "Net-(U1101-PadL11)"))
  )
  (module neo900-legacy:NONE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (tags "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (attr virtual)
    (fp_text reference U1201 (at 0 0) (layer F.SilkS))
    (fp_text value TS5A22366 (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:S-PWQFN-N20-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TI RTJ (S-PWQFN-N20)")
    (tags "TI RTJ (S-PWQFN-N20)")
    (attr smd)
    (fp_text reference U1202 (at -0.28448 -1.35382) (layer F.SilkS))
    (fp_text value TPA6130A2RTJ (at -0.49022 -0.63246) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(C1206-Pad2)"))
    (pad 2 smd rect (at -0.49784 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(C1204-Pad2)"))
    (pad 3 smd rect (at 0 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 4 smd rect (at 0.49784 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C1207-Pad2)"))
    (pad 5 smd rect (at 0.99822 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(C1209-Pad2)"))
    (pad 6 smd rect (at 1.89992 0.99822 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 976 GPIO-HP-EN))
    (pad 7 smd rect (at 1.89992 0.49784 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 369 I2C2-SDA))
    (pad 8 smd rect (at 1.89992 0 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad 9 smd rect (at 1.89992 -0.49784 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 10 smd rect (at 1.89992 -0.99822 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 11 smd rect (at 0.99822 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(D1201-Pad1)"))
    (pad 12 smd rect (at 0.49784 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(C1201-Pad2)"))
    (pad 13 smd rect (at 0 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 14 smd rect (at -0.49784 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(D1204-Pad2)"))
    (pad 15 smd rect (at -0.99822 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(C1210-Pad1)"))
    (pad 16 smd rect (at -1.89992 -0.99822) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(C1210-Pad1)"))
    (pad 17 smd rect (at -1.89992 -0.49784) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(C1203-Pad2)"))
    (pad 18 smd rect (at -1.89992 0) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(C1203-Pad1)"))
    (pad 19 smd rect (at -1.89992 0.49784) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 20 smd rect (at -1.89992 0.99822) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(C1201-Pad2)"))
    (pad E smd rect (at 0.02794 -0.0381) (size 2.14884 2.14884) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
  )
  (module neo900-legacy:S-PWQFN-N16-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "S-PWQFN-N16 (TI RTE)")
    (tags "S-PWQFN-N16 (TI RTE)")
    (attr smd)
    (fp_text reference U1203 (at -0.28448 -1.35382) (layer F.SilkS))
    (fp_text value TS3A225ERTE (at -0.49022 -0.63246) (layer F.SilkS))
    (pad 1 smd rect (at -0.7493 1.4732 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 371 I2C2-SCL))
    (pad 2 smd rect (at -0.24892 1.4732 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 369 I2C2-SDA))
    (pad 3 smd rect (at 0.24892 1.4732 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 4 smd rect (at 0.7493 1.4732 90) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 5 smd rect (at 1.4732 0.7493 180) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(C1217-Pad1)"))
    (pad 6 smd rect (at 1.4732 0.24892 180) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(D1203-Pad2)"))
    (pad 7 smd rect (at 1.4732 -0.24892 180) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(D1205-Pad2)"))
    (pad 8 smd rect (at 1.4732 -0.7493 180) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 977 GPIO$60))
    (pad 9 smd rect (at 0.7493 -1.4732 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(D1204-Pad2)"))
    (pad 10 smd rect (at 0.24892 -1.4732 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
    (pad 11 smd rect (at -0.24892 -1.4732 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 836 MIC-ECI))
    (pad 12 smd rect (at -0.7493 -1.4732 270) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 837 "Net-(R1207-Pad2)"))
    (pad 13 smd rect (at -1.4732 -0.7493) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 94 VMMC2))
    (pad 14 smd rect (at -1.4732 -0.24892) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(D1205-Pad2)"))
    (pad 15 smd rect (at -1.4732 0.24892) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(D1203-Pad2)"))
    (pad 16 smd rect (at -1.4732 0.7493) (size 0.84836 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 94 VMMC2))
    (pad E smd rect (at 0.02794 -0.0381) (size 1.69926 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 83 AGND))
  )
  (module neo900-legacy:SOT23-5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SOT23 WITH 5 PINS")
    (tags "SOT23 WITH 5 PINS")
    (attr smd)
    (fp_text reference U1301 (at -0.4826 -0.60198) (layer F.SilkS))
    (fp_text value TLV702225DBV (at -0.5842 -0.1524) (layer F.SilkS))
    (pad 1 smd rect (at -0.94996 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 2 smd rect (at 0 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at 0.94742 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 4 smd rect (at 0.94742 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 978 "Net-(U1301-Pad4)"))
    (pad 5 smd rect (at -0.94996 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 839 /ECI/2V5))
  )
  (module neo900-legacy:R-PDSO-G8-0.65 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TEXAS INSTRUMENTS DGK")
    (tags "TEXAS INSTRUMENTS DGK")
    (attr smd)
    (fp_text reference U1302 (at -0.43688 -0.55118) (layer F.SilkS))
    (fp_text value TLV1702DGK (at -0.28448 0.04572) (layer F.SilkS))
    (pad 1 smd rect (at -0.97282 2.19964) (size 0.44958 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 842 GPIO-ECI1))
    (pad 2 smd rect (at -0.32258 2.19964) (size 0.44958 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 838 "Net-(R1301-Pad1)"))
    (pad 3 smd rect (at 0.32258 2.19964) (size 0.44958 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 841 "Net-(R1303-Pad1)"))
    (pad 4 smd rect (at 0.97282 2.19964) (size 0.44958 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 5 smd rect (at 0.97282 -2.19964) (size 0.44958 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 844 "Net-(R1307-Pad2)"))
    (pad 6 smd rect (at 0.32258 -2.19964) (size 0.44958 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 840 "Net-(R1302-Pad1)"))
    (pad 7 smd rect (at -0.32258 -2.19964) (size 0.44958 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 843 GPIO-ECI0))
    (pad 8 smd rect (at -0.97282 -2.19964) (size 0.44958 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 839 /ECI/2V5))
  )
  (module neo900-legacy:S-PWQFN-N20-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TI RTJ (S-PWQFN-N20)")
    (tags "TI RTJ (S-PWQFN-N20)")
    (attr smd)
    (fp_text reference U1401 (at -0.28448 -1.35382) (layer F.SilkS))
    (fp_text value TPA2012D2RTJ (at -0.49022 -0.63246) (layer F.SilkS))
    (pad 1 smd rect (at -0.99822 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at -0.49784 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(L1402-Pad2)"))
    (pad 3 smd rect (at 0 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 4 smd rect (at 0.49784 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 5 smd rect (at 0.99822 1.89992 90) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(L1401-Pad2)"))
    (pad 6 smd rect (at 1.89992 0.99822 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.89992 0.49784 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 979 GPIO-HF-EN))
    (pad 8 smd rect (at 1.89992 0 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 979 GPIO-HF-EN))
    (pad 9 smd rect (at 1.89992 -0.49784 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 10 smd rect (at 1.89992 -0.99822 180) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.99822 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(L1403-Pad2)"))
    (pad 12 smd rect (at 0.49784 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 13 smd rect (at 0 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 34 VSYS))
    (pad 14 smd rect (at -0.49784 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(L1404-Pad2)"))
    (pad 15 smd rect (at -0.99822 -1.89992 270) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 16 smd rect (at -1.89992 -0.99822) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(C1409-Pad2)"))
    (pad 17 smd rect (at -1.89992 -0.49784) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(C1408-Pad2)"))
    (pad 18 smd rect (at -1.89992 0) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 19 smd rect (at -1.89992 0.49784) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(C1406-Pad2)"))
    (pad 20 smd rect (at -1.89992 0.99822) (size 0.99822 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(C1407-Pad2)"))
    (pad E smd rect (at 0.02794 -0.0381) (size 2.14884 2.14884) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:TRF7960_61 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TRF796X HF RFID ASIC")
    (tags "TRF796X HF RFID ASIC")
    (attr smd)
    (fp_text reference U1601 (at 0 0) (layer F.SilkS))
    (fp_text value TRF7970A (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at -2.49936 -1.74752 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(C1623-Pad1)"))
    (pad 2 smd rect (at -2.49936 -1.24968 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3))
    (pad 3 smd rect (at -2.49936 -0.7493 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(C1610-Pad1)"))
    (pad 4 smd rect (at -2.49936 -0.24892 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(C1610-Pad1)"))
    (pad 5 smd rect (at -2.49936 0.24892 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(C1607-Pad1)"))
    (pad 6 smd rect (at -2.49936 0.7493 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 7 smd rect (at -2.49936 1.24968 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 8 smd rect (at -2.49936 1.75006 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(C1611-Pad2)"))
    (pad 9 smd rect (at -1.75006 2.49936 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(C1614-Pad2)"))
    (pad 10 smd rect (at -1.24968 2.49936 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 11 smd rect (at -0.7493 2.49936 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(C1603-Pad2)"))
    (pad 12 smd rect (at -0.24892 2.49936 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 980 NFC-ASKOOK))
    (pad 13 smd rect (at 0.24892 2.49936 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 981 NFC-IRQ))
    (pad 14 smd rect (at 0.7493 2.49936 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 982 NFC-TXD/MOD))
    (pad 15 smd rect (at 1.24968 2.49936 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 16 smd rect (at 1.74752 2.49936 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 17 smd rect (at 2.49936 1.75006) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 18 smd rect (at 2.49936 1.24968) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 983 NFC-IO1))
    (pad 19 smd rect (at 2.49936 0.7493) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 984 NFC-TXEN))
    (pad 20 smd rect (at 2.49936 0.24892) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 982 NFC-TXD/MOD))
    (pad 21 smd rect (at 2.49936 -0.24892) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 985 NFC-SS))
    (pad 22 smd rect (at 2.49936 -0.7493) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 986 NFC-TRXCLK))
    (pad 23 smd rect (at 2.49936 -1.24968) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 987 NFC-MISO))
    (pad 24 smd rect (at 2.49936 -1.74752) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 988 NFC-MOSI))
    (pad 25 smd rect (at 1.74752 -2.49936 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 26 smd rect (at 1.24968 -2.49936 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 989 NFC-SCLK))
    (pad 27 smd rect (at 0.7493 -2.49936 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 990 NFC-CLK))
    (pad 28 smd rect (at 0.24892 -2.49936 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 991 NFC-EN))
    (pad 29 smd rect (at -0.24892 -2.49936 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 30 smd rect (at -0.7493 -2.49936 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(C1625-Pad1)"))
    (pad 31 smd rect (at -1.24968 -2.49936 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(C1626-Pad1)"))
    (pad 32 smd rect (at -1.75006 -2.49936 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(C1627-Pad1)"))
    (pad TP smd rect (at 0 0) (size 3.44932 3.44932) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:QFN-32+E-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "QFN 32-0.5MM")
    (tags "QFN 32-0.5MM")
    (attr smd)
    (fp_text reference U1701 (at 1.55448 -0.57404 270) (layer F.SilkS))
    (fp_text value MKL16Z128VFM4 (at 0.65278 -0.32004 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.2987 -1.74752) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 987 NFC-MISO))
    (pad 2 smd rect (at -2.2987 -1.24968) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 982 NFC-TXD/MOD))
    (pad 3 smd rect (at -2.2987 -0.7493) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 985 NFC-SS))
    (pad 4 smd rect (at -2.2987 -0.24892) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 989 NFC-SCLK))
    (pad 5 smd rect (at -2.2987 0.24892) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 988 NFC-MOSI))
    (pad 6 smd rect (at -2.2987 0.7493) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 987 NFC-MISO))
    (pad 7 smd rect (at -2.2987 1.24968) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 8 smd rect (at -2.2987 1.75006) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 9 smd rect (at -1.75006 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(C1701-Pad1)"))
    (pad 10 smd rect (at -1.24968 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 984 NFC-TXEN))
    (pad 11 smd rect (at -0.7493 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 981 NFC-IRQ))
    (pad 12 smd rect (at -0.24892 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 991 NFC-EN))
    (pad 13 smd rect (at 0.24892 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 980 NFC-ASKOOK))
    (pad 14 smd rect (at 0.7493 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 180 "/RFID/NFC Controller/NFC_LED"))
    (pad 15 smd rect (at 1.24968 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 68 1V8))
    (pad 16 smd rect (at 1.74752 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 17 smd rect (at 2.2987 1.75006 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 990 NFC-CLK))
    (pad 18 smd rect (at 2.2987 1.24968 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 983 NFC-IO1))
    (pad 19 smd rect (at 2.2987 0.7493 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 992 OMAP_NFC_nRESET))
    (pad 20 smd rect (at 2.2987 0.24892 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 993 "Net-(U1701-Pad20)"))
    (pad 21 smd rect (at 2.2987 -0.24892 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 994 "Net-(U1701-Pad21)"))
    (pad 22 smd rect (at 2.2987 -0.7493 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 982 NFC-TXD/MOD))
    (pad 23 smd rect (at 2.2987 -1.24968 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 995 OMAP_NFC_INT))
    (pad 24 smd rect (at 2.2987 -1.74752 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 996 SWP_nRESET))
    (pad 25 smd rect (at 1.74752 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 997 "/RFID/NFC Controller/SELF"))
    (pad 26 smd rect (at 1.24968 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 987 NFC-MISO))
    (pad 27 smd rect (at 0.7493 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 849 SWIO-2))
    (pad 28 smd rect (at 0.24892 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 847 SWIO-1))
    (pad 29 smd rect (at -0.24892 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 997 "/RFID/NFC Controller/SELF"))
    (pad 30 smd rect (at -0.7493 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 986 NFC-TRXCLK))
    (pad 31 smd rect (at -1.24968 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 848 "/RFID/NFC Controller/SWP_2_S1"))
    (pad 32 smd rect (at -1.75006 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 846 "/RFID/NFC Controller/SWP_1_S1"))
    (pad EXP smd rect (at 0 0) (size 3.19786 3.19786) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:PW_R-PDSO-G08 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PLASTIC SMALL-OUTLINE PACKAGE, SO 8 JEDEC MO-153, PW TYPE")
    (tags "PLASTIC SMALL-OUTLINE PACKAGE, SO 8 JEDEC MO-153, PW TYPE")
    (attr smd)
    (fp_text reference U1901 (at -0.15748 -1.42748) (layer F.SilkS))
    (fp_text value TLV7256ISSOP (at 0.04318 -0.47752) (layer F.SilkS))
    (pad 1 smd rect (at -0.97282 2.89814) (size 0.39878 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 851 "Net-(R1902-Pad2)"))
    (pad 2 smd rect (at -0.32258 2.89814) (size 0.39878 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 853 "Net-(R1908-Pad2)"))
    (pad 3 smd rect (at 0.32258 2.89814) (size 0.39878 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 850 "Net-(R1902-Pad1)"))
    (pad 4 smd rect (at 0.97282 2.89814) (size 0.39878 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 998 "Net-(U1901-Pad4)"))
    (pad 5 smd rect (at 0.97282 -2.89814 180) (size 0.39878 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 999 "Net-(U1901-Pad5)"))
    (pad 6 smd rect (at 0.32258 -2.89814 180) (size 0.39878 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1000 "Net-(U1901-Pad6)"))
    (pad 7 smd rect (at -0.32258 -2.89814 180) (size 0.39878 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1001 "Net-(U1901-Pad7)"))
    (pad 8 smd rect (at -0.97282 -2.89814 180) (size 0.39878 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1002 "Net-(U1901-Pad8)"))
  )
  (module neo900-legacy:RPM973-H11E2A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "ROHM RPM973 IRDA MODULE")
    (tags "ROHM RPM973 IRDA MODULE")
    (attr smd)
    (fp_text reference U1902G$1 (at -2.27584 -0.2032) (layer F.SilkS))
    (fp_text value RPM973-H11E2A (at -1.97104 0.49276) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.5mm" (at 2.85496 -4.03352) (layer B.SilkS))
    (pad 1 smd rect (at 2.84988 0.79756) (size 0.6985 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1003 "Net-(U1902G$1-Pad1)"))
    (pad 2 smd rect (at 1.89992 0.79756) (size 0.6985 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1004 "Net-(U1902G$1-Pad2)"))
    (pad 3 smd rect (at 0.94742 0.79756) (size 0.6985 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 851 "Net-(R1902-Pad2)"))
    (pad 4 smd rect (at 0 0.79756) (size 0.6985 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1005 "Net-(U1902G$1-Pad4)"))
    (pad 5 smd rect (at -0.94996 0.79756) (size 0.6985 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1006 "Net-(U1902G$1-Pad5)"))
    (pad 6 smd rect (at -1.89992 0.79756) (size 0.6985 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1007 "Net-(U1902G$1-Pad6)"))
    (pad 7 smd rect (at -2.84988 0.79756) (size 0.6985 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad S smd rect (at 0.14986 -0.89916) (size 1.19888 0.59944) (layers F.Cu F.Paste F.Mask))
  )
  (module neo900-legacy:SOT23 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr SOT23)
    (tags SOT23)
    (attr smd)
    (fp_text reference U2101 (at -0.4826 -0.60198) (layer F.SilkS))
    (fp_text value MLX90248ESE (at -0.7366 -0.127) (layer F.SilkS))
    (pad 1 smd rect (at 0.94742 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 130 "/uSD Breakout Board/USD-3V3"))
    (pad 2 smd rect (at -0.94996 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 493 "/uSD Breakout Board/LID"))
    (pad 3 smd rect (at 0.01778 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
  )
  (module neo900-legacy:SFH7741 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "OSRAM SFH7741 PROXIMITY SENSOR")
    (tags "OSRAM SFH7741 PROXIMITY SENSOR")
    (attr smd)
    (fp_text reference U2102 (at 0.50292 0.71374 270) (layer F.SilkS))
    (fp_text value SFH7741 (at -0.47244 0.96012 270) (layer F.SilkS))
    (fp_text user "HEIGHT> 1.1mm" (at 5.8547 -3.43408) (layer B.SilkS))
    (pad 1 smd rect (at -1.62306 -1.19888) (size 1.24968 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 1008 "Net-(U2102-Pad1)"))
    (pad 2 smd rect (at -1.62306 0) (size 1.24968 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad 3 smd rect (at -1.62306 1.19888) (size 1.24968 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 492 "Net-(P2101-Pad13)"))
    (pad 4 smd rect (at 1.62306 1.19888) (size 1.24968 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad 5 smd rect (at 1.62306 0) (size 1.24968 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 130 "/uSD Breakout Board/USD-3V3"))
    (pad 6 smd rect (at 1.62306 -1.19888) (size 1.24968 0.84836) (layers F.Cu F.Paste F.Mask)
      (net 854 "Net-(R2101-Pad1)"))
  )
  (module neo900-legacy:QFN-16+E-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference U2103 (at 1.30302 -0.4826 270) (layer F.SilkS))
    (fp_text value ADP1653 (at 0.60198 -0.2794 270) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.85mm" (at 6.78942 -2.73304) (layer B.SilkS))
    (pad 1 smd rect (at -1.35382 -0.7493) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(C2105-Pad1)"))
    (pad 2 smd rect (at -1.35382 -0.24892) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(C2105-Pad1)"))
    (pad 3 smd rect (at -1.35382 0.24892) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 488 "/uSD Breakout Board/USD-I2C2-SCL"))
    (pad 4 smd rect (at -1.35382 0.7493) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 487 "/uSD Breakout Board/USD-I2C2-SDA"))
    (pad 5 smd rect (at -0.7493 1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(C2105-Pad1)"))
    (pad 6 smd rect (at -0.24892 1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(LED2102-PadK)"))
    (pad 7 smd rect (at 0.24892 1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(C2104-Pad1)"))
    (pad 8 smd rect (at 0.7493 1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad 9 smd rect (at 1.35382 0.7493) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(LED2103-Pad1)"))
    (pad 10 smd rect (at 1.35382 0.24892) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad 11 smd rect (at 1.35382 -0.24892) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 491 "/uSD Breakout Board/USD-INT"))
    (pad 12 smd rect (at 1.35382 -0.7493) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
    (pad 13 smd rect (at 0.7493 -1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(D2102-PadA)"))
    (pad 14 smd rect (at 0.24892 -1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(C2105-Pad1)"))
    (pad 15 smd rect (at -0.24892 -1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 490 "/uSD Breakout Board/USD-EN"))
    (pad 16 smd rect (at -0.7493 -1.35382 90) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 489 "/uSD Breakout Board/USD-STR"))
    (pad EXP smd rect (at 0 0) (size 1.69926 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 131 GND2))
  )
  (module neo900-legacy:LPCC-24 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PWQFN-24: 4X4MM 0.5 PITCH 24 PADS")
    (tags "PWQFN-24: 4X4MM 0.5 PITCH 24 PADS")
    (attr smd)
    (fp_text reference U2301 (at 0.45212 1.54178 180) (layer F.SilkS))
    (fp_text value TCA8418RTW (at 0.24892 0.96266 180) (layer F.SilkS))
    (pad 1 smd rect (at 1.24968 -1.84912 90) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(B79/2301-PadP$2)"))
    (pad 2 smd rect (at 0.7493 -1.84912 90) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(B69/O3709-PadP$2)"))
    (pad 3 smd rect (at 0.24892 -1.84912 90) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(B60/^2301-PadP$2)"))
    (pad 4 smd rect (at -0.24892 -1.84912 90) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 1009 "Net-(U2301-Pad4)"))
    (pad 5 smd rect (at -0.7493 -1.84912 90) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(B33/ESC3709-PadP$2)"))
    (pad 6 smd rect (at -1.24968 -1.84912 90) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B23/TAB3709-PadP$2)"))
    (pad 7 smd rect (at -1.84912 -1.24968) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B13/SPC2301-PadP$2)"))
    (pad 8 smd rect (at -1.84912 -0.7493) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B10/OK3709-PadP$2)"))
    (pad 9 smd rect (at -1.84912 -0.24892) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(B1/CTL3709-PadP$1)"))
    (pad 10 smd rect (at -1.84912 0.24892) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(B12/FN3709-PadP$1)"))
    (pad 11 smd rect (at -1.84912 0.7493) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(B13/SPC2301-PadP$1)"))
    (pad 12 smd rect (at -1.84912 1.24968) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(B14/SPC2301-PadP$1)"))
    (pad 13 smd rect (at -1.24968 1.84912 90) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(B15/M3709-PadP$1)"))
    (pad 14 smd rect (at -0.7493 1.84912 90) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(B16/,3709-PadP$1)"))
    (pad 15 smd rect (at -0.24892 1.84912 90) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(B17/PGDN3709-PadP$1)"))
    (pad 16 smd rect (at 0.24892 1.84912 90) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(B18/END3709-PadP$1)"))
    (pad 17 smd rect (at 0.7493 1.84912 90) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(B19/LEFT3709-PadP$1)"))
    (pad 18 smd rect (at 1.24968 1.84912 90) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(B10/OK3709-PadP$1)"))
    (pad 19 smd rect (at 1.84912 1.24968) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 20 smd rect (at 1.84912 0.7493) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 1010 RESET_UPPER))
    (pad 21 smd rect (at 1.84912 0.24892) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad 22 smd rect (at 1.84912 -0.24892) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 325 I2C2-SDA-CPU))
    (pad 23 smd rect (at 1.84912 -0.7493) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 326 I2C2-SCL-CPU))
    (pad 24 smd rect (at 1.84912 -1.24968) (size 0.49784 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 1011 KEYIRQ_UPPER))
    (pad P smd rect (at 0 0) (size 2.44856 2.44856) (layers F.Cu F.Paste F.Mask))
  )
  (module neo900-legacy:QFN-32+E-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "QFN 32-0.5MM")
    (tags "QFN 32-0.5MM")
    (attr smd)
    (fp_text reference U2402 (at 1.55448 -0.57404 270) (layer F.SilkS))
    (fp_text value CRTOUCH (at 0.65278 -0.32004 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.2987 -1.74752) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 855 "Net-(R2402-Pad2)"))
    (pad 2 smd rect (at -2.2987 -1.24968) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1012 PENIRQ_UPPER))
    (pad 3 smd rect (at -2.2987 -0.7493) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1013 "Net-(U2402-Pad3)"))
    (pad 4 smd rect (at -2.2987 -0.24892) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(C2406-Pad1)"))
    (pad 5 smd rect (at -2.2987 0.24892) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(C2407-Pad1)"))
    (pad 6 smd rect (at -2.2987 0.7493) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(C2408-Pad1)"))
    (pad 7 smd rect (at -2.2987 1.24968) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C2410-Pad1)"))
    (pad 8 smd rect (at -2.2987 1.75006) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 9 smd rect (at -1.75006 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -1.24968 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -0.7493 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -0.24892 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1014 "Net-(U2402-Pad12)"))
    (pad 13 smd rect (at 0.24892 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1015 "Net-(U2402-Pad13)"))
    (pad 14 smd rect (at 0.7493 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 15 smd rect (at 1.24968 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(C2409-Pad1)"))
    (pad 16 smd rect (at 1.74752 2.2987 90) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1016 "Net-(U2402-Pad16)"))
    (pad 17 smd rect (at 2.2987 1.75006 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 856 "Net-(R2403-Pad2)"))
    (pad 18 smd rect (at 2.2987 1.24968 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1017 "Net-(U2402-Pad18)"))
    (pad 19 smd rect (at 2.2987 0.7493 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1018 "Net-(U2402-Pad19)"))
    (pad 20 smd rect (at 2.2987 0.24892 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1019 "Net-(U2402-Pad20)"))
    (pad 21 smd rect (at 2.2987 -0.24892 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 2.2987 -0.7493 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1020 "Net-(U2402-Pad22)"))
    (pad 23 smd rect (at 2.2987 -1.24968 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 24 smd rect (at 2.2987 -1.74752 180) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(C2410-Pad1)"))
    (pad 25 smd rect (at 1.74752 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 26 smd rect (at 1.24968 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 326 I2C2-SCL-CPU))
    (pad 27 smd rect (at 0.7493 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 325 I2C2-SDA-CPU))
    (pad 28 smd rect (at 0.24892 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1021 "Net-(U2402-Pad28)"))
    (pad 29 smd rect (at -0.24892 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1022 "Net-(U2402-Pad29)"))
    (pad 30 smd rect (at -0.7493 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1023 "Net-(U2402-Pad30)"))
    (pad 31 smd rect (at -1.24968 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1024 "Net-(U2402-Pad31)"))
    (pad 32 smd rect (at -1.75006 -2.2987 270) (size 0.59944 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1025 "Net-(U2402-Pad32)"))
    (pad EXP smd rect (at 0 0) (size 3.19786 3.19786) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:SOT23-5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SOT23 WITH 5 PINS")
    (tags "SOT23 WITH 5 PINS")
    (attr smd)
    (fp_text reference U2501 (at -0.4826 -0.60198) (layer F.SilkS))
    (fp_text value TPS61041DBV (at -0.5842 -0.1524) (layer F.SilkS))
    (pad 1 smd rect (at -0.94996 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(D2501-PadA)"))
    (pad 2 smd rect (at 0 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 3 smd rect (at 0.94742 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(D2502-PadA)"))
    (pad 4 smd rect (at 0.94742 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 857 PWM_UPPER))
    (pad 5 smd rect (at -0.94996 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 145 VBATT_UPPER))
  )
  (module neo900-legacy:PBGA784-N515-0.4 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "CBB (S-PBGA-N515)")
    (tags "CBB (S-PBGA-N515)")
    (attr smd)
    (fp_text reference U2502 (at 5.03936 -3.8735 270) (layer F.SilkS))
    (fp_text value DM3730CBP100 (at 3.99796 -3.5687 270) (layer F.SilkS))
    (fp_text user A1 (at -5.45846 -5.67944) (layer F.SilkS))
    (fp_text user A28 (at 5.588 -5.67944) (layer F.SilkS))
    (fp_text user AH28 (at 5.56768 5.67944) (layer F.SilkS))
    (fp_text user AH1 (at -5.55752 5.65912) (layer F.SilkS))
    (fp_text user "HEIGHT> 2mm" (at 1.3843 -7.03326) (layer B.SilkS))
    (pad A1 smd circle (at -5.40004 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A2 smd circle (at -4.99872 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A3 smd circle (at -4.59994 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A4 smd circle (at -4.19862 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd circle (at -3.79984 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A6 smd circle (at -3.39852 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A7 smd circle (at -2.99974 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A8 smd circle (at -2.59842 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A9 smd circle (at -2.19964 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A10 smd circle (at -1.79832 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A11 smd circle (at -1.39954 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A12 smd circle (at -0.99822 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A13 smd circle (at -0.59944 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A14 smd circle (at -0.19812 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A15 smd circle (at 0.19812 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A16 smd circle (at 0.59944 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A17 smd circle (at 0.99822 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A18 smd circle (at 1.39954 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A19 smd circle (at 1.79832 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A20 smd circle (at 2.19964 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A21 smd circle (at 2.59842 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A22 smd circle (at 2.99974 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A23 smd circle (at 3.39852 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1026 "Net-(U2502-PadA23)"))
    (pad A24 smd circle (at 3.79984 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1027 "Net-(U2502-PadA24)"))
    (pad A25 smd circle (at 4.19862 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1028 "Net-(U2502-PadA25)"))
    (pad A26 smd circle (at 4.5974 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A27 smd circle (at 4.99872 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A28 smd circle (at 5.3975 -5.3975) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA1 smd circle (at -5.40004 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA2 smd circle (at -4.99872 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA3 smd circle (at -4.59994 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA4 smd circle (at -4.19862 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 336 "Net-(P-DISP3709-Pad36)"))
    (pad AA8 smd circle (at -2.59842 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA9 smd circle (at -2.19964 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA10 smd circle (at -1.79832 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA11 smd circle (at -1.39954 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA12 smd circle (at -0.99822 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA13 smd circle (at -0.59944 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA14 smd circle (at -0.19812 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA15 smd circle (at 0.19812 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA16 smd circle (at 0.59944 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA17 smd circle (at 0.99822 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA18 smd circle (at 1.39954 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA19 smd circle (at 1.79832 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA20 smd circle (at 2.19964 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA21 smd circle (at 2.59842 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA25 smd circle (at 4.19862 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA26 smd circle (at 4.5974 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA27 smd circle (at 4.99872 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1029 "Net-(U2502-PadAA27)"))
    (pad AA28 smd circle (at 5.3975 2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1030 "Net-(U2502-PadAA28)"))
    (pad AB1 smd circle (at -5.40004 2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AB2 smd circle (at -4.99872 2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AB3 smd circle (at -4.59994 2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 338 "Net-(P-DISP3709-Pad38)"))
    (pad AB4 smd circle (at -4.19862 2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 335 "Net-(P-DISP3709-Pad35)"))
    (pad AB25 smd circle (at 4.19862 2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AB26 smd circle (at 4.5974 2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AB27 smd circle (at 4.99872 2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 212 /Display-Panel&Power/CDP-D1+_UPPER))
    (pad AB28 smd circle (at 5.3975 2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 213 /Display-Panel&Power/CDP-D1-_UPPER))
    (pad AC1 smd circle (at -5.40004 3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AC2 smd circle (at -4.99872 3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 334 "Net-(P-DISP3709-Pad34)"))
    (pad AC3 smd circle (at -4.59994 3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AC4 smd circle (at -4.19862 3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AC25 smd circle (at 4.19862 3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AC26 smd circle (at 4.5974 3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AC27 smd circle (at 4.99872 3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 216 /Display-Panel&Power/CDP-CLK+_UPPER))
    (pad AC28 smd circle (at 5.3975 3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 217 /Display-Panel&Power/CDP-CLK-_UPPER))
    (pad AD1 smd circle (at -5.40004 3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AD2 smd circle (at -4.99872 3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AD3 smd circle (at -4.59994 3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AD4 smd circle (at -4.19862 3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AD25 smd circle (at 4.19862 3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AD26 smd circle (at 4.5974 3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AD27 smd circle (at 4.99872 3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 208 /Display-Panel&Power/CDP-D0+_UPPER))
    (pad AD28 smd circle (at 5.3975 3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 209 /Display-Panel&Power/CDP-D0-_UPPER))
    (pad AE1 smd circle (at -5.40004 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE2 smd circle (at -4.99872 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1031 "Net-(U2502-PadAE2)"))
    (pad AE3 smd circle (at -4.59994 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE4 smd circle (at -4.19862 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE5 smd circle (at -3.79984 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE6 smd circle (at -3.39852 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE7 smd circle (at -2.99974 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE8 smd circle (at -2.59842 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE9 smd circle (at -2.19964 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE10 smd circle (at -1.79832 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE11 smd circle (at -1.39954 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE12 smd circle (at -0.99822 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE13 smd circle (at -0.59944 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE14 smd circle (at -0.19812 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1032 "Net-(U2502-PadAE14)"))
    (pad AE15 smd circle (at 0.19812 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 325 I2C2-SDA-CPU))
    (pad AE16 smd circle (at 0.59944 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE17 smd circle (at 0.99822 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE18 smd circle (at 1.39954 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE19 smd circle (at 1.79832 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE20 smd circle (at 2.19964 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE21 smd circle (at 2.59842 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1033 "Net-(U2502-PadAE21)"))
    (pad AE22 smd circle (at 2.99974 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE23 smd circle (at 3.39852 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE24 smd circle (at 3.79984 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE25 smd circle (at 4.19862 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE26 smd circle (at 4.5974 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE27 smd circle (at 4.99872 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE28 smd circle (at 5.3975 4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF1 smd circle (at -5.40004 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF2 smd circle (at -4.99872 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF3 smd circle (at -4.59994 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF4 smd circle (at -4.19862 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1034 "Net-(U2502-PadAF4)"))
    (pad AF5 smd circle (at -3.79984 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF6 smd circle (at -3.39852 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF7 smd circle (at -2.99974 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF8 smd circle (at -2.59842 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF9 smd circle (at -2.19964 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF10 smd circle (at -1.79832 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF11 smd circle (at -1.39954 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF12 smd circle (at -0.99822 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF13 smd circle (at -0.59944 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF14 smd circle (at -0.19812 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 605 I2C3-SCL-CPU))
    (pad AF15 smd circle (at 0.19812 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 326 I2C2-SCL-CPU))
    (pad AF16 smd circle (at 0.59944 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF17 smd circle (at 0.99822 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF18 smd circle (at 1.39954 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1035 "Net-(U2502-PadAF18)"))
    (pad AF19 smd circle (at 1.79832 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1036 "Net-(U2502-PadAF19)"))
    (pad AF20 smd circle (at 2.19964 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF21 smd circle (at 2.59842 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1037 "Net-(U2502-PadAF21)"))
    (pad AF22 smd circle (at 2.99974 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF23 smd circle (at 3.39852 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF24 smd circle (at 3.79984 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 635 NRESWARM-CPU))
    (pad AF25 smd circle (at 4.19862 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF26 smd circle (at 4.5974 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1038 "Net-(U2502-PadAF26)"))
    (pad AF27 smd circle (at 4.99872 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AF28 smd circle (at 5.3975 4.59994) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG1 smd circle (at -5.40004 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG2 smd circle (at -4.99872 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG3 smd circle (at -4.59994 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG4 smd circle (at -4.19862 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1039 "Net-(U2502-PadAG4)"))
    (pad AG5 smd circle (at -3.79984 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1040 "Net-(U2502-PadAG5)"))
    (pad AG6 smd circle (at -3.39852 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG7 smd circle (at -2.99974 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG8 smd circle (at -2.59842 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG9 smd circle (at -2.19964 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG10 smd circle (at -1.79832 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG11 smd circle (at -1.39954 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG12 smd circle (at -0.99822 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG13 smd circle (at -0.59944 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG14 smd circle (at -0.19812 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 606 I2C3-SDA-CPU))
    (pad AG15 smd circle (at 0.19812 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG16 smd circle (at 0.59944 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG17 smd circle (at 0.99822 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1041 "Net-(U2502-PadAG17)"))
    (pad AG18 smd circle (at 1.39954 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG19 smd circle (at 1.79832 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG20 smd circle (at 2.19964 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG21 smd circle (at 2.59842 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG22 smd circle (at 2.99974 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 322 "Net-(P-DISP3709-Pad8)"))
    (pad AG23 smd circle (at 3.39852 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1042 "Net-(U2502-PadAG23)"))
    (pad AG24 smd circle (at 3.79984 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1043 "Net-(U2502-PadAG24)"))
    (pad AG25 smd circle (at 4.19862 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG26 smd circle (at 4.5974 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1044 "Net-(U2502-PadAG26)"))
    (pad AG27 smd circle (at 4.99872 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG28 smd circle (at 5.3975 4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH1 smd circle (at -5.40004 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH2 smd circle (at -4.99872 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH3 smd circle (at -4.59994 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH4 smd circle (at -4.19862 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1045 "Net-(U2502-PadAH4)"))
    (pad AH5 smd circle (at -3.79984 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1046 "Net-(U2502-PadAH5)"))
    (pad AH6 smd circle (at -3.39852 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH7 smd circle (at -2.99974 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH8 smd circle (at -2.59842 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH9 smd circle (at -2.19964 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH10 smd circle (at -1.79832 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH11 smd circle (at -1.39954 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH12 smd circle (at -0.99822 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH13 smd circle (at -0.59944 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH14 smd circle (at -0.19812 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH15 smd circle (at 0.19812 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH16 smd circle (at 0.59944 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH17 smd circle (at 0.99822 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1047 "Net-(U2502-PadAH17)"))
    (pad AH18 smd circle (at 1.39954 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH19 smd circle (at 1.79832 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH20 smd circle (at 2.19964 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH21 smd circle (at 2.59842 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH22 smd circle (at 2.99974 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1048 "Net-(U2502-PadAH22)"))
    (pad AH23 smd circle (at 3.39852 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1049 "Net-(U2502-PadAH23)"))
    (pad AH24 smd circle (at 3.79984 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1050 "Net-(U2502-PadAH24)"))
    (pad AH25 smd circle (at 4.19862 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1051 "Net-(U2502-PadAH25)"))
    (pad AH26 smd circle (at 4.5974 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1052 "Net-(U2502-PadAH26)"))
    (pad AH27 smd circle (at 4.99872 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH28 smd circle (at 5.3975 5.40004) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B1 smd circle (at -5.40004 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B2 smd circle (at -4.99872 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B3 smd circle (at -4.59994 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B4 smd circle (at -4.19862 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B5 smd circle (at -3.79984 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B6 smd circle (at -3.39852 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B7 smd circle (at -2.99974 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B8 smd circle (at -2.59842 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B9 smd circle (at -2.19964 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B10 smd circle (at -1.79832 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B11 smd circle (at -1.39954 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B12 smd circle (at -0.99822 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B13 smd circle (at -0.59944 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B14 smd circle (at -0.19812 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B15 smd circle (at 0.19812 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B16 smd circle (at 0.59944 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B17 smd circle (at 0.99822 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B18 smd circle (at 1.39954 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B19 smd circle (at 1.79832 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B20 smd circle (at 2.19964 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B21 smd circle (at 2.59842 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B22 smd circle (at 2.99974 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B23 smd circle (at 3.39852 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1053 /Camera/GPIO167))
    (pad B24 smd circle (at 3.79984 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1054 "Net-(U2502-PadB24)"))
    (pad B25 smd circle (at 4.19862 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1055 "Net-(U2502-PadB25)"))
    (pad B26 smd circle (at 4.5974 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1056 "Net-(U2502-PadB26)"))
    (pad B27 smd circle (at 4.99872 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B28 smd circle (at 5.3975 -4.99872) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C1 smd circle (at -5.40004 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C2 smd circle (at -4.99872 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C3 smd circle (at -4.59994 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C4 smd circle (at -4.19862 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C5 smd circle (at -3.79984 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C6 smd circle (at -3.39852 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C7 smd circle (at -2.99974 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C8 smd circle (at -2.59842 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C9 smd circle (at -2.19964 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C10 smd circle (at -1.79832 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C11 smd circle (at -1.39954 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C12 smd circle (at -0.99822 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C13 smd circle (at -0.59944 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C14 smd circle (at -0.19812 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C15 smd circle (at 0.19812 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C16 smd circle (at 0.59944 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C17 smd circle (at 0.99822 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C18 smd circle (at 1.39954 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C19 smd circle (at 1.79832 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C20 smd circle (at 2.19964 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C21 smd circle (at 2.59842 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C22 smd circle (at 2.99974 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C23 smd circle (at 3.39852 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1057 "Net-(U2502-PadC23)"))
    (pad C24 smd circle (at 3.79984 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 604 /Camera/GPIO102))
    (pad C25 smd circle (at 4.19862 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 859 "Net-(R3001-Pad1)"))
    (pad C26 smd circle (at 4.5974 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1058 "Net-(U2502-PadC26)"))
    (pad C27 smd circle (at 4.99872 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 327 GPIO97))
    (pad C28 smd circle (at 5.3975 -4.5974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D1 smd circle (at -5.40004 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D2 smd circle (at -4.99872 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D3 smd circle (at -4.59994 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D4 smd circle (at -4.19862 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D5 smd circle (at -3.79984 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D6 smd circle (at -3.39852 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D7 smd circle (at -2.99974 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D8 smd circle (at -2.59842 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D9 smd circle (at -2.19964 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D10 smd circle (at -1.79832 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D11 smd circle (at -1.39954 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D12 smd circle (at -0.99822 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D13 smd circle (at -0.59944 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D14 smd circle (at -0.19812 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D15 smd circle (at 0.19812 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D16 smd circle (at 0.59944 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D17 smd circle (at 0.99822 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D18 smd circle (at 1.39954 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D19 smd circle (at 1.79832 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D20 smd circle (at 2.19964 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D21 smd circle (at 2.59842 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D22 smd circle (at 2.99974 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D23 smd circle (at 3.39852 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D24 smd circle (at 3.79984 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1059 "Net-(U2502-PadD24)"))
    (pad D25 smd circle (at 4.19862 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1060 /Camera/CAM-STR))
    (pad D26 smd circle (at 4.5974 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1061 "Net-(U2502-PadD26)"))
    (pad D27 smd circle (at 4.99872 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1062 "Net-(U2502-PadD27)"))
    (pad D28 smd circle (at 5.3975 -4.19862) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1063 "Net-(U2502-PadD28)"))
    (pad E1 smd circle (at -5.40004 -3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E2 smd circle (at -4.99872 -3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E3 smd circle (at -4.59994 -3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E4 smd circle (at -4.19862 -3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E25 smd circle (at 4.19862 -3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E26 smd circle (at 4.5974 -3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1064 "Net-(U2502-PadE26)"))
    (pad E27 smd circle (at 4.99872 -3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1065 "Net-(U2502-PadE27)"))
    (pad E28 smd circle (at 5.3975 -3.79984) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 337 "Net-(P-DISP3709-Pad37)"))
    (pad F1 smd circle (at -5.40004 -3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F2 smd circle (at -4.99872 -3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F3 smd circle (at -4.59994 -3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F4 smd circle (at -4.19862 -3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F25 smd circle (at 4.19862 -3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F26 smd circle (at 4.5974 -3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F27 smd circle (at 4.99872 -3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1066 "Net-(U2502-PadF27)"))
    (pad F28 smd circle (at 5.3975 -3.39852) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1067 "Net-(U2502-PadF28)"))
    (pad G1 smd circle (at -5.40004 -2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad G2 smd circle (at -4.99872 -2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad G3 smd circle (at -4.59994 -2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad G4 smd circle (at -4.19862 -2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad G25 smd circle (at 4.19862 -2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1068 "Net-(U2502-PadG25)"))
    (pad G26 smd circle (at 4.5974 -2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1069 "Net-(U2502-PadG26)"))
    (pad G27 smd circle (at 4.99872 -2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad G28 smd circle (at 5.3975 -2.99974) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H1 smd circle (at -5.40004 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H2 smd circle (at -4.99872 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H3 smd circle (at -4.59994 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H4 smd circle (at -4.19862 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H9 smd circle (at -2.19964 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H10 smd circle (at -1.79832 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H11 smd circle (at -1.39954 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H12 smd circle (at -0.99822 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H13 smd circle (at -0.59944 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H14 smd circle (at -0.19812 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H15 smd circle (at 0.19812 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H16 smd circle (at 0.59944 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H17 smd circle (at 0.99822 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H18 smd circle (at 1.39954 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H19 smd circle (at 1.79832 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H20 smd circle (at 2.19964 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H21 smd circle (at 2.59842 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H25 smd circle (at 4.19862 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 324 "Net-(P-DISP3709-Pad10)"))
    (pad H26 smd circle (at 4.5974 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1070 "Net-(U2502-PadH26)"))
    (pad H27 smd circle (at 4.99872 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1071 "Net-(U2502-PadH27)"))
    (pad H28 smd circle (at 5.3975 -2.59842) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J1 smd circle (at -5.40004 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J2 smd circle (at -4.99872 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J3 smd circle (at -4.59994 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J4 smd circle (at -4.19862 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J8 smd circle (at -2.59842 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J9 smd circle (at -2.19964 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J10 smd circle (at -1.79832 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J11 smd circle (at -1.39954 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J12 smd circle (at -0.99822 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J13 smd circle (at -0.59944 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J14 smd circle (at -0.19812 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J15 smd circle (at 0.19812 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J16 smd circle (at 0.59944 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J17 smd circle (at 0.99822 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J18 smd circle (at 1.39954 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J19 smd circle (at 1.79832 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J20 smd circle (at 2.19964 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J21 smd circle (at 2.59842 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J25 smd circle (at 4.19862 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J26 smd circle (at 4.5974 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1072 "Net-(U2502-PadJ26)"))
    (pad J27 smd circle (at 4.99872 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J28 smd circle (at 5.3975 -2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K1 smd circle (at -5.40004 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K2 smd circle (at -4.99872 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K3 smd circle (at -4.59994 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K4 smd circle (at -4.19862 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K8 smd circle (at -2.59842 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K9 smd circle (at -2.19964 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K10 smd circle (at -1.79832 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K11 smd circle (at -1.39954 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K12 smd circle (at -0.99822 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K13 smd circle (at -0.59944 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K14 smd circle (at -0.19812 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K15 smd circle (at 0.19812 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K16 smd circle (at 0.59944 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K17 smd circle (at 0.99822 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K18 smd circle (at 1.39954 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K19 smd circle (at 1.79832 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K20 smd circle (at 2.19964 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K21 smd circle (at 2.59842 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K25 smd circle (at 4.19862 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K26 smd circle (at 4.5974 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K27 smd circle (at 4.99872 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 863 "Net-(R3004-Pad2)"))
    (pad K28 smd circle (at 5.3975 -1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 861 "Net-(R3003-Pad2)"))
    (pad L1 smd circle (at -5.40004 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L2 smd circle (at -4.99872 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L3 smd circle (at -4.59994 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L4 smd circle (at -4.19862 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L8 smd circle (at -2.59842 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L9 smd circle (at -2.19964 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L10 smd circle (at -1.79832 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L19 smd circle (at 1.79832 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L20 smd circle (at 2.19964 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L21 smd circle (at 2.59842 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L25 smd circle (at 4.19862 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L26 smd circle (at 4.5974 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L27 smd circle (at 4.99872 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 862 "Net-(R3004-Pad1)"))
    (pad L28 smd circle (at 5.3975 -1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 860 "Net-(R3003-Pad1)"))
    (pad M1 smd circle (at -5.40004 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M2 smd circle (at -4.99872 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M3 smd circle (at -4.59994 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M4 smd circle (at -4.19862 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M8 smd circle (at -2.59842 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M9 smd circle (at -2.19964 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M10 smd circle (at -1.79832 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M19 smd circle (at 1.79832 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M20 smd circle (at 2.19964 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M21 smd circle (at 2.59842 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M25 smd circle (at 4.19862 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M26 smd circle (at 4.5974 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M27 smd circle (at 4.99872 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1073 "Net-(U2502-PadM27)"))
    (pad M28 smd circle (at 5.3975 -0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N1 smd circle (at -5.40004 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N2 smd circle (at -4.99872 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N3 smd circle (at -4.59994 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N4 smd circle (at -4.19862 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N8 smd circle (at -2.59842 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N9 smd circle (at -2.19964 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N10 smd circle (at -1.79832 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N19 smd circle (at 1.79832 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N20 smd circle (at 2.19964 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N21 smd circle (at 2.59842 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N25 smd circle (at 4.19862 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1074 "Net-(U2502-PadN25)"))
    (pad N26 smd circle (at 4.5974 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1075 "Net-(U2502-PadN26)"))
    (pad N27 smd circle (at 4.99872 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1076 "Net-(U2502-PadN27)"))
    (pad N28 smd circle (at 5.3975 -0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1077 "Net-(U2502-PadN28)"))
    (pad P1 smd circle (at -5.40004 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P2 smd circle (at -4.99872 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P3 smd circle (at -4.59994 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P4 smd circle (at -4.19862 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P8 smd circle (at -2.59842 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P9 smd circle (at -2.19964 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P10 smd circle (at -1.79832 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P19 smd circle (at 1.79832 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P20 smd circle (at 2.19964 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P21 smd circle (at 2.59842 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P25 smd circle (at 4.19862 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P26 smd circle (at 4.5974 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1078 "Net-(U2502-PadP26)"))
    (pad P27 smd circle (at 4.99872 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1079 "Net-(U2502-PadP27)"))
    (pad P28 smd circle (at 5.3975 -0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1080 "Net-(U2502-PadP28)"))
    (pad R1 smd circle (at -5.40004 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R2 smd circle (at -4.99872 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R3 smd circle (at -4.59994 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R4 smd circle (at -4.19862 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R8 smd circle (at -2.59842 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R9 smd circle (at -2.19964 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R10 smd circle (at -1.79832 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R19 smd circle (at 1.79832 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R20 smd circle (at 2.19964 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R21 smd circle (at 2.59842 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R25 smd circle (at 4.19862 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1081 "Net-(U2502-PadR25)"))
    (pad R26 smd circle (at 4.5974 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R27 smd circle (at 4.99872 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1082 "Net-(U2502-PadR27)"))
    (pad R28 smd circle (at 5.3975 0.19812) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T1 smd circle (at -5.40004 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T2 smd circle (at -4.99872 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T3 smd circle (at -4.59994 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T4 smd circle (at -4.19862 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T8 smd circle (at -2.59842 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T9 smd circle (at -2.19964 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T10 smd circle (at -1.79832 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T19 smd circle (at 1.79832 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T20 smd circle (at 2.19964 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T21 smd circle (at 2.59842 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T25 smd circle (at 4.19862 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T26 smd circle (at 4.5974 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T27 smd circle (at 4.99872 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T28 smd circle (at 5.3975 0.59944) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U1 smd circle (at -5.40004 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U2 smd circle (at -4.99872 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U3 smd circle (at -4.59994 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U4 smd circle (at -4.19862 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U8 smd circle (at -2.59842 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U9 smd circle (at -2.19964 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U10 smd circle (at -1.79832 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U19 smd circle (at 1.79832 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U20 smd circle (at 2.19964 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U21 smd circle (at 2.59842 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U25 smd circle (at 4.19862 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U26 smd circle (at 4.5974 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U27 smd circle (at 4.99872 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U28 smd circle (at 5.3975 0.99822) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V1 smd circle (at -5.40004 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V2 smd circle (at -4.99872 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V3 smd circle (at -4.59994 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V4 smd circle (at -4.19862 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V8 smd circle (at -2.59842 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V9 smd circle (at -2.19964 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V10 smd circle (at -1.79832 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V19 smd circle (at 1.79832 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V20 smd circle (at 2.19964 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V21 smd circle (at 2.59842 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V25 smd circle (at 4.19862 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V26 smd circle (at 4.5974 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V27 smd circle (at 4.99872 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V28 smd circle (at 5.3975 1.39954) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W1 smd circle (at -5.40004 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W2 smd circle (at -4.99872 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W3 smd circle (at -4.59994 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W4 smd circle (at -4.19862 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W8 smd circle (at -2.59842 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W9 smd circle (at -2.19964 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W10 smd circle (at -1.79832 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W11 smd circle (at -1.39954 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W12 smd circle (at -0.99822 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W13 smd circle (at -0.59944 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W14 smd circle (at -0.19812 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W15 smd circle (at 0.19812 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W16 smd circle (at 0.59944 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W17 smd circle (at 0.99822 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W18 smd circle (at 1.39954 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W19 smd circle (at 1.79832 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W20 smd circle (at 2.19964 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W21 smd circle (at 2.59842 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W25 smd circle (at 4.19862 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W26 smd circle (at 4.5974 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W27 smd circle (at 4.99872 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W28 smd circle (at 5.3975 1.79832) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y1 smd circle (at -5.40004 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y2 smd circle (at -4.99872 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y3 smd circle (at -4.59994 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y4 smd circle (at -4.19862 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y8 smd circle (at -2.59842 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y9 smd circle (at -2.19964 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y10 smd circle (at -1.79832 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y11 smd circle (at -1.39954 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y12 smd circle (at -0.99822 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y13 smd circle (at -0.59944 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y14 smd circle (at -0.19812 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y15 smd circle (at 0.19812 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y16 smd circle (at 0.59944 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y17 smd circle (at 0.99822 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y18 smd circle (at 1.39954 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y19 smd circle (at 1.79832 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y20 smd circle (at 2.19964 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y21 smd circle (at 2.59842 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y25 smd circle (at 4.19862 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y26 smd circle (at 4.5974 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y27 smd circle (at 4.99872 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y28 smd circle (at 5.3975 2.19964) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
  )
  (module neo900-legacy:NONE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (tags "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (attr virtual)
    (fp_text reference U2601 (at 0 0) (layer F.SilkS))
    (fp_text value KCE00E00CA (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:EMMC-BGA-N169-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "169 BALL BGA FOR EMMC 12X16MM PACKAGE")
    (tags "169 BALL BGA FOR EMMC 12X16MM PACKAGE")
    (attr smd)
    (fp_text reference U2701 (at -5.24256 6.5532 90) (layer F.SilkS))
    (fp_text value EMMC-169 (at -4.70154 6.6548 90) (layer F.SilkS))
    (pad A4 smd circle (at 1.74752 6.74878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A6 smd circle (at 0.7493 6.74878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A9 smd circle (at -0.7493 6.74878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A11 smd circle (at -1.75006 6.74878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA1 smd circle (at 3.24866 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA2 smd circle (at 2.74828 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA3 smd circle (at 2.2479 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad AA4 smd circle (at 1.74752 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad AA5 smd circle (at 1.24968 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad AA6 smd circle (at 0.7493 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad AA7 smd circle (at 0.24892 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA8 smd circle (at -0.24892 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA9 smd circle (at -0.7493 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA10 smd circle (at -1.24968 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA11 smd circle (at -1.75006 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA12 smd circle (at -2.2479 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA13 smd circle (at -2.74828 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AA14 smd circle (at -3.24866 -3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE1 smd circle (at 3.24866 -5.24764 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AE14 smd circle (at -3.24866 -5.24764 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG2 smd circle (at 2.74828 -6.2484 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AG13 smd circle (at -2.74828 -6.2484 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH4 smd circle (at 1.74752 -6.74878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH6 smd circle (at 0.7493 -6.74878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH9 smd circle (at -0.7493 -6.74878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad AH11 smd circle (at -1.75006 -6.74878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B2 smd circle (at 2.74828 6.2484 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B13 smd circle (at -2.74828 6.2484 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D1 smd circle (at 3.24866 5.24764 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D14 smd circle (at -3.24866 5.24764 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H1 smd circle (at 3.24866 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H2 smd circle (at 2.74828 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H3 smd circle (at 2.2479 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1083 "Net-(U2701-PadH3)"))
    (pad H4 smd circle (at 1.74752 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1084 "Net-(U2701-PadH4)"))
    (pad H5 smd circle (at 1.24968 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1085 "Net-(U2701-PadH5)"))
    (pad H6 smd circle (at 0.7493 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H7 smd circle (at 0.24892 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H8 smd circle (at -0.24892 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H9 smd circle (at -0.7493 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H10 smd circle (at -1.24968 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H11 smd circle (at -1.75006 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H12 smd circle (at -2.2479 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H13 smd circle (at -2.74828 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H14 smd circle (at -3.24866 3.24866 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J1 smd circle (at 3.24866 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J2 smd circle (at 2.74828 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1086 "Net-(U2701-PadJ2)"))
    (pad J3 smd circle (at 2.2479 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1087 "Net-(U2701-PadJ3)"))
    (pad J4 smd circle (at 1.74752 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1088 "Net-(U2701-PadJ4)"))
    (pad J5 smd circle (at 1.24968 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1089 "Net-(U2701-PadJ5)"))
    (pad J6 smd circle (at 0.7493 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1090 "Net-(U2701-PadJ6)"))
    (pad J7 smd circle (at 0.24892 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J8 smd circle (at -0.24892 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J9 smd circle (at -0.7493 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J10 smd circle (at -1.24968 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J11 smd circle (at -1.75006 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J12 smd circle (at -2.2479 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J13 smd circle (at -2.74828 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J14 smd circle (at -3.24866 2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K1 smd circle (at 3.24866 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K2 smd circle (at 2.74828 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1091 "Net-(U2701-PadK2)"))
    (pad K3 smd circle (at 2.2479 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K4 smd circle (at 1.74752 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad K5 smd circle (at 1.24968 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K6 smd circle (at 0.7493 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad K7 smd circle (at 0.24892 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K8 smd circle (at -0.24892 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K9 smd circle (at -0.7493 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K10 smd circle (at -1.24968 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K11 smd circle (at -1.75006 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K12 smd circle (at -2.2479 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K13 smd circle (at -2.74828 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K14 smd circle (at -3.24866 2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L1 smd circle (at 3.24866 1.75006 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L2 smd circle (at 2.74828 1.75006 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L3 smd circle (at 2.2479 1.75006 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L4 smd circle (at 1.74752 1.75006 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L12 smd circle (at -2.2479 1.75006 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L13 smd circle (at -2.74828 1.75006 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L14 smd circle (at -3.24866 1.75006 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M1 smd circle (at 3.24866 1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M2 smd circle (at 2.74828 1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M3 smd circle (at 2.2479 1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M5 smd circle (at 1.24968 1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M6 smd circle (at 0.7493 1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 318 3V3-CPU))
    (pad M7 smd circle (at 0.24892 1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad M8 smd circle (at -0.24892 1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M9 smd circle (at -0.7493 1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M10 smd circle (at -1.24968 1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M12 smd circle (at -2.2479 1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M13 smd circle (at -2.74828 1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M14 smd circle (at -3.24866 1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N1 smd circle (at 3.24866 0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N2 smd circle (at 2.74828 0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N3 smd circle (at 2.2479 0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N5 smd circle (at 1.24968 0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 318 3V3-CPU))
    (pad N10 smd circle (at -1.24968 0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N12 smd circle (at -2.2479 0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N13 smd circle (at -2.74828 0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N14 smd circle (at -3.24866 0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P1 smd circle (at 3.24866 0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P2 smd circle (at 2.74828 0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P3 smd circle (at 2.2479 0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P5 smd circle (at 1.24968 0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad P10 smd circle (at -1.24968 0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P12 smd circle (at -2.2479 0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P13 smd circle (at -2.74828 0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P14 smd circle (at -3.24866 0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R1 smd circle (at 3.24866 -0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R2 smd circle (at 2.74828 -0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R3 smd circle (at 2.2479 -0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R5 smd circle (at 1.24968 -0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R10 smd circle (at -1.24968 -0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad R12 smd circle (at -2.2479 -0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R13 smd circle (at -2.74828 -0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R14 smd circle (at -3.24866 -0.24892 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T1 smd circle (at 3.24866 -0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T2 smd circle (at 2.74828 -0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T3 smd circle (at 2.2479 -0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T5 smd circle (at 1.24968 -0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T10 smd circle (at -1.24968 -0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 318 3V3-CPU))
    (pad T12 smd circle (at -2.2479 -0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T13 smd circle (at -2.74828 -0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T14 smd circle (at -3.24866 -0.7493 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U1 smd circle (at 3.24866 -1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U2 smd circle (at 2.74828 -1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U3 smd circle (at 2.2479 -1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U5 smd circle (at 1.24968 -1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 635 NRESWARM-CPU))
    (pad U6 smd circle (at 0.7493 -1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U7 smd circle (at 0.24892 -1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U8 smd circle (at -0.24892 -1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad U9 smd circle (at -0.7493 -1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 318 3V3-CPU))
    (pad U10 smd circle (at -1.24968 -1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U12 smd circle (at -2.2479 -1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U13 smd circle (at -2.74828 -1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad U14 smd circle (at -3.24866 -1.24968 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V1 smd circle (at 3.24866 -1.74752 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V2 smd circle (at 2.74828 -1.74752 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V3 smd circle (at 2.2479 -1.74752 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V12 smd circle (at -2.2479 -1.74752 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V13 smd circle (at -2.74828 -1.74752 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad V14 smd circle (at -3.24866 -1.74752 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W1 smd circle (at 3.24866 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W2 smd circle (at 2.74828 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W3 smd circle (at 2.2479 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W4 smd circle (at 1.74752 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad W5 smd circle (at 1.24968 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1092 "Net-(U2701-PadW5)"))
    (pad W6 smd circle (at 0.7493 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1093 "Net-(U2701-PadW6)"))
    (pad W7 smd circle (at 0.24892 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W8 smd circle (at -0.24892 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W9 smd circle (at -0.7493 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W10 smd circle (at -1.24968 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W11 smd circle (at -1.75006 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W12 smd circle (at -2.2479 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W13 smd circle (at -2.74828 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad W14 smd circle (at -3.24866 -2.2479 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y1 smd circle (at 3.24866 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y2 smd circle (at 2.74828 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad Y3 smd circle (at 2.2479 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y4 smd circle (at 1.74752 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad Y5 smd circle (at 1.24968 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad Y6 smd circle (at 0.7493 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y7 smd circle (at 0.24892 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y8 smd circle (at -0.24892 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y9 smd circle (at -0.7493 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y10 smd circle (at -1.24968 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y11 smd circle (at -1.75006 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y12 smd circle (at -2.2479 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y13 smd circle (at -2.74828 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad Y14 smd circle (at -3.24866 -2.74828 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
  )
  (module neo900-legacy:NONE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (tags "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (attr virtual)
    (fp_text reference U2801 (at 0 0) (layer F.SilkS))
    (fp_text value LTC3355 (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:WLCSP25-N25-0.4 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PBGA 25 PINS 0.4 PITCH")
    (tags "PBGA 25 PINS 0.4 PITCH")
    (attr smd)
    (fp_text reference U2802 (at -0.64262 -0.14478 90) (layer F.SilkS))
    (fp_text value USB3322 (at -0.20066 -0.04318 90) (layer F.SilkS))
    (pad A1 smd circle (at 0.79756 0.79756 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1094 "Net-(U2802-PadA1)"))
    (pad A2 smd circle (at 0.39878 0.79756 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1095 "Net-(U2802-PadA2)"))
    (pad A3 smd circle (at 0 0.79756 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1096 "Net-(U2802-PadA3)"))
    (pad A4 smd circle (at -0.39878 0.79756 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1097 "Net-(U2802-PadA4)"))
    (pad A5 smd circle (at -0.79756 0.79756 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1098 "Net-(U2802-PadA5)"))
    (pad B1 smd circle (at 0.79756 0.39878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1099 "Net-(U2802-PadB1)"))
    (pad B2 smd circle (at 0.39878 0.39878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1100 "Net-(U2802-PadB2)"))
    (pad B3 smd circle (at 0 0.39878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1101 "Net-(U2802-PadB3)"))
    (pad B4 smd circle (at -0.39878 0.39878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1102 "Net-(U2802-PadB4)"))
    (pad B5 smd circle (at -0.79756 0.39878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1103 "Net-(U2802-PadB5)"))
    (pad C1 smd circle (at 0.79756 0 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1104 "Net-(U2802-PadC1)"))
    (pad C2 smd circle (at 0.39878 0 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 354 VBUS-MODEM-CPU))
    (pad C3 smd circle (at 0 0 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1105 "Net-(U2802-PadC3)"))
    (pad C4 smd circle (at -0.39878 0 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1106 "Net-(U2802-PadC4)"))
    (pad C5 smd circle (at -0.79756 0 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1107 "Net-(U2802-PadC5)"))
    (pad D1 smd circle (at 0.79756 -0.39878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 355 MODEM-CPU-D-))
    (pad D2 smd circle (at 0.39878 -0.39878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1108 "Net-(U2802-PadD2)"))
    (pad D3 smd circle (at 0 -0.39878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1109 "Net-(U2802-PadD3)"))
    (pad D4 smd circle (at -0.39878 -0.39878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1110 "Net-(U2802-PadD4)"))
    (pad D5 smd circle (at -0.79756 -0.39878 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1111 "Net-(U2802-PadD5)"))
    (pad E1 smd circle (at 0.79756 -0.79756 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 356 MODEM-CPU-D+))
    (pad E2 smd circle (at 0.39878 -0.79756 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1112 "Net-(U2802-PadE2)"))
    (pad E3 smd circle (at 0 -0.79756 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1113 "Net-(U2802-PadE3)"))
    (pad E4 smd circle (at -0.39878 -0.79756 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1114 "Net-(U2802-PadE4)"))
    (pad E5 smd circle (at -0.79756 -0.79756 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1115 "Net-(U2802-PadE5)"))
  )
  (module neo900-legacy:PBGA256-N213-0.4 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "BALL GRID ARRAY PBGA 256 - 0.4 PITCH")
    (tags "BALL GRID ARRAY PBGA 256 - 0.4 PITCH")
    (attr smd)
    (fp_text reference U2803 (at -2.90322 1.37414 90) (layer F.SilkS))
    (fp_text value TPS65950 (at -2.00406 1.06934 90) (layer F.SilkS))
    (fp_text user T16 (at -3.10896 -3.21818) (layer F.SilkS))
    (fp_text user A16 (at -3.0988 3.21818) (layer F.SilkS))
    (fp_text user A1 (at 3.03784 3.21818) (layer F.SilkS))
    (fp_text user T1 (at 3.20802 -3.21818) (layer F.SilkS))
    (pad A1 smd circle (at 2.99974 2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A2 smd circle (at 2.59842 2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1116 "Net-(U2803-PadA2)"))
    (pad A3 smd circle (at 2.19964 2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A4 smd circle (at 1.79832 2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A6 smd circle (at 0.99822 2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A7 smd circle (at 0.59944 2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A10 smd circle (at -0.59944 2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A11 smd circle (at -0.99822 2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A13 smd circle (at -1.79832 2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A14 smd circle (at -2.19964 2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1117 "Net-(U2803-PadA14)"))
    (pad A15 smd circle (at -2.59842 2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad A16 smd circle (at -2.99974 2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B1 smd circle (at 2.99974 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B2 smd circle (at 2.59842 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B3 smd circle (at 2.19964 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B4 smd circle (at 1.79832 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B5 smd circle (at 1.39954 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B6 smd circle (at 0.99822 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B7 smd circle (at 0.59944 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B8 smd circle (at 0.19812 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B9 smd circle (at -0.19812 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B10 smd circle (at -0.59944 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B11 smd circle (at -0.99822 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B12 smd circle (at -1.39954 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B13 smd circle (at -1.79832 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B14 smd circle (at -2.19964 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1118 "Net-(U2803-PadB14)"))
    (pad B15 smd circle (at -2.59842 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad B16 smd circle (at -2.99974 2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C1 smd circle (at 2.99974 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C2 smd circle (at 2.59842 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C3 smd circle (at 2.19964 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C4 smd circle (at 1.79832 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C5 smd circle (at 1.39954 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C6 smd circle (at 0.99822 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1119 "Net-(U2803-PadC6)"))
    (pad C7 smd circle (at 0.59944 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C8 smd circle (at 0.19812 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1120 "Net-(U2803-PadC8)"))
    (pad C9 smd circle (at -0.19812 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C10 smd circle (at -0.59944 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C11 smd circle (at -0.99822 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C12 smd circle (at -1.39954 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C13 smd circle (at -1.79832 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C14 smd circle (at -2.19964 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C15 smd circle (at -2.59842 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad C16 smd circle (at -2.99974 2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D1 smd circle (at 2.99974 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D2 smd circle (at 2.59842 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D3 smd circle (at 2.19964 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D4 smd circle (at 1.79832 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D5 smd circle (at 1.39954 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D6 smd circle (at 0.99822 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D7 smd circle (at 0.59944 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1121 "Net-(U2803-PadD7)"))
    (pad D8 smd circle (at 0.19812 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D9 smd circle (at -0.19812 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D10 smd circle (at -0.59944 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D11 smd circle (at -0.99822 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D12 smd circle (at -1.39954 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D13 smd circle (at -1.79832 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1122 "Net-(U2803-PadD13)"))
    (pad D14 smd circle (at -2.19964 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D15 smd circle (at -2.59842 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad D16 smd circle (at -2.99974 1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E2 smd circle (at 2.59842 1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E3 smd circle (at 2.19964 1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E4 smd circle (at 1.79832 1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E5 smd circle (at 1.39954 1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E13 smd circle (at -1.79832 1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E14 smd circle (at -2.19964 1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad E15 smd circle (at -2.59842 1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F1 smd circle (at 2.99974 0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F2 smd circle (at 2.59842 0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F3 smd circle (at 2.19964 0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F4 smd circle (at 1.79832 0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F7 smd circle (at 0.59944 0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F8 smd circle (at 0.19812 0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F9 smd circle (at -0.19812 0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F10 smd circle (at -0.59944 0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad F13 smd circle (at -1.79832 0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1123 "Net-(U2803-PadF13)"))
    (pad F14 smd circle (at -2.19964 0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1124 "Net-(U2803-PadF14)"))
    (pad F15 smd circle (at -2.59842 0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1125 "Net-(U2803-PadF15)"))
    (pad F16 smd circle (at -2.99974 0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1126 "Net-(U2803-PadF16)"))
    (pad G1 smd circle (at 2.99974 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad G2 smd circle (at 2.59842 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad G3 smd circle (at 2.19964 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1127 "Net-(U2803-PadG3)"))
    (pad G4 smd circle (at 1.79832 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad G6 smd circle (at 0.99822 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad G7 smd circle (at 0.59944 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad G8 smd circle (at 0.19812 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad G9 smd circle (at -0.19812 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad G10 smd circle (at -0.59944 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1128 "Net-(U2803-PadG10)"))
    (pad G11 smd circle (at -0.99822 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1129 "Net-(U2803-PadG11)"))
    (pad G13 smd circle (at -1.79832 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1130 "Net-(U2803-PadG13)"))
    (pad G14 smd circle (at -2.19964 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1131 "Net-(U2803-PadG14)"))
    (pad G15 smd circle (at -2.59842 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1132 "Net-(U2803-PadG15)"))
    (pad G16 smd circle (at -2.99974 0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H2 smd circle (at 2.59842 0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H3 smd circle (at 2.19964 0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H4 smd circle (at 1.79832 0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1133 "Net-(U2803-PadH4)"))
    (pad H6 smd circle (at 0.99822 0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H7 smd circle (at 0.59944 0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H8 smd circle (at 0.19812 0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1134 "Net-(U2803-PadH8)"))
    (pad H9 smd circle (at -0.19812 0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H10 smd circle (at -0.59944 0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H11 smd circle (at -0.99822 0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H13 smd circle (at -1.79832 0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H14 smd circle (at -2.19964 0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad H15 smd circle (at -2.59842 0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J2 smd circle (at 2.59842 -0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J3 smd circle (at 2.19964 -0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1135 "Net-(U2803-PadJ3)"))
    (pad J4 smd circle (at 1.79832 -0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J6 smd circle (at 0.99822 -0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J7 smd circle (at 0.59944 -0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J8 smd circle (at 0.19812 -0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J9 smd circle (at -0.19812 -0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1136 "Net-(U2803-PadJ9)"))
    (pad J10 smd circle (at -0.59944 -0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J11 smd circle (at -0.99822 -0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad J13 smd circle (at -1.79832 -0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1137 "Net-(U2803-PadJ13)"))
    (pad J14 smd circle (at -2.19964 -0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1138 "Net-(U2803-PadJ14)"))
    (pad J15 smd circle (at -2.59842 -0.19812 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K1 smd circle (at 2.99974 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K2 smd circle (at 2.59842 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K3 smd circle (at 2.19964 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K4 smd circle (at 1.79832 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K6 smd circle (at 0.99822 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K7 smd circle (at 0.59944 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K8 smd circle (at 0.19812 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K9 smd circle (at -0.19812 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K10 smd circle (at -0.59944 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K11 smd circle (at -0.99822 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K13 smd circle (at -1.79832 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1139 "Net-(U2803-PadK13)"))
    (pad K14 smd circle (at -2.19964 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1140 "Net-(U2803-PadK14)"))
    (pad K15 smd circle (at -2.59842 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad K16 smd circle (at -2.99974 -0.59944 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L1 smd circle (at 2.99974 -0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L2 smd circle (at 2.59842 -0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L3 smd circle (at 2.19964 -0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L4 smd circle (at 1.79832 -0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L7 smd circle (at 0.59944 -0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L8 smd circle (at 0.19812 -0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L9 smd circle (at -0.19812 -0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L10 smd circle (at -0.59944 -0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad L13 smd circle (at -1.79832 -0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1141 "Net-(U2803-PadL13)"))
    (pad L14 smd circle (at -2.19964 -0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1142 "Net-(U2803-PadL14)"))
    (pad L15 smd circle (at -2.59842 -0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1143 "Net-(U2803-PadL15)"))
    (pad L16 smd circle (at -2.99974 -0.99822 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M2 smd circle (at 2.59842 -1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M3 smd circle (at 2.19964 -1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M4 smd circle (at 1.79832 -1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad M13 smd circle (at -1.79832 -1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1144 "Net-(U2803-PadM13)"))
    (pad M14 smd circle (at -2.19964 -1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(C2802-Pad1)"))
    (pad M15 smd circle (at -2.59842 -1.39954 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N1 smd circle (at 2.99974 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1145 "Net-(U2803-PadN1)"))
    (pad N2 smd circle (at 2.59842 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1146 "Net-(U2803-PadN2)"))
    (pad N3 smd circle (at 2.19964 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N4 smd circle (at 1.79832 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1147 "Net-(U2803-PadN4)"))
    (pad N5 smd circle (at 1.39954 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1148 "Net-(U2803-PadN5)"))
    (pad N6 smd circle (at 0.99822 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1149 "Net-(U2803-PadN6)"))
    (pad N7 smd circle (at 0.59944 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1150 "Net-(U2803-PadN7)"))
    (pad N8 smd circle (at 0.19812 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N9 smd circle (at -0.19812 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N10 smd circle (at -0.59944 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1151 "Net-(U2803-PadN10)"))
    (pad N11 smd circle (at -0.99822 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N12 smd circle (at -1.39954 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N13 smd circle (at -1.79832 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N14 smd circle (at -2.19964 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad N15 smd circle (at -2.59842 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1152 "Net-(U2803-PadN15)"))
    (pad N16 smd circle (at -2.99974 -1.79832 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1153 "Net-(U2803-PadN16)"))
    (pad P1 smd circle (at 2.99974 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1154 "Net-(U2803-PadP1)"))
    (pad P2 smd circle (at 2.59842 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1155 "Net-(U2803-PadP2)"))
    (pad P3 smd circle (at 2.19964 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P4 smd circle (at 1.79832 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1156 "Net-(U2803-PadP4)"))
    (pad P5 smd circle (at 1.39954 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1157 "Net-(U2803-PadP5)"))
    (pad P6 smd circle (at 0.99822 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1158 "Net-(U2803-PadP6)"))
    (pad P7 smd circle (at 0.59944 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P8 smd circle (at 0.19812 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P9 smd circle (at -0.19812 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P10 smd circle (at -0.59944 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P11 smd circle (at -0.99822 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P12 smd circle (at -1.39954 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P13 smd circle (at -1.79832 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P14 smd circle (at -2.19964 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad P15 smd circle (at -2.59842 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1159 "Net-(U2803-PadP15)"))
    (pad P16 smd circle (at -2.99974 -2.19964 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1160 "Net-(U2803-PadP16)"))
    (pad R1 smd circle (at 2.99974 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R2 smd circle (at 2.59842 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R3 smd circle (at 2.19964 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R4 smd circle (at 1.79832 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R5 smd circle (at 1.39954 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1161 "Net-(U2803-PadR5)"))
    (pad R6 smd circle (at 0.99822 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R7 smd circle (at 0.59944 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R8 smd circle (at 0.19812 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 868 VBUS-CPU))
    (pad R9 smd circle (at -0.19812 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R10 smd circle (at -0.59944 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R11 smd circle (at -0.99822 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1162 OTG-CPU-ID))
    (pad R12 smd circle (at -1.39954 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 1163 "Net-(U2803-PadR12)"))
    (pad R13 smd circle (at -1.79832 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R14 smd circle (at -2.19964 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R15 smd circle (at -2.59842 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad R16 smd circle (at -2.99974 -2.59842 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T1 smd circle (at 2.99974 -2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T2 smd circle (at 2.59842 -2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T3 smd circle (at 2.19964 -2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T4 smd circle (at 1.79832 -2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T6 smd circle (at 0.99822 -2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T7 smd circle (at 0.59944 -2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T10 smd circle (at -0.59944 -2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 870 OTG-CPU-D+))
    (pad T11 smd circle (at -0.99822 -2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask)
      (net 869 OTG-CPU-D-))
    (pad T13 smd circle (at -1.79832 -2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T14 smd circle (at -2.19964 -2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T15 smd circle (at -2.59842 -2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
    (pad T16 smd circle (at -2.99974 -2.99974 180) (size 0.27432 0.27432) (layers F.Cu F.Paste F.Mask))
  )
  (module neo900-legacy:SOT23-5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SOT23 WITH 5 PINS")
    (tags "SOT23 WITH 5 PINS")
    (attr smd)
    (fp_text reference U2901 (at -0.4826 -0.60198) (layer F.SilkS))
    (fp_text value TPS73633DBV (at -0.5842 -0.1524) (layer F.SilkS))
    (pad 1 smd rect (at -0.94996 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 858 "VBAT(->TPS65950)_UPPER"))
    (pad 2 smd rect (at 0 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 3 smd rect (at 0.94742 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 858 "VBAT(->TPS65950)_UPPER"))
    (pad 4 smd rect (at 0.94742 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1164 "Net-(U2901-Pad4)"))
    (pad 5 smd rect (at -0.94996 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 318 3V3-CPU))
  )
  (module neo900-legacy:SOT23-5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "SOT23 WITH 5 PINS")
    (tags "SOT23 WITH 5 PINS")
    (attr smd)
    (fp_text reference U2902 (at -0.4826 -0.60198) (layer F.SilkS))
    (fp_text value TPS73618DBV (at -0.5842 -0.1524) (layer F.SilkS))
    (pad 1 smd rect (at -0.94996 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 858 "VBAT(->TPS65950)_UPPER"))
    (pad 2 smd rect (at 0 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 3 smd rect (at 0.94742 1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 858 "VBAT(->TPS65950)_UPPER"))
    (pad 4 smd rect (at 0.94742 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1165 "Net-(U2902-Pad4)"))
    (pad 5 smd rect (at -0.94996 -1.19888) (size 0.49784 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
  )
  (module neo900-legacy:R-XBGA-N12-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TI YZG (0.5MM PITCH)")
    (tags "TI YZG (0.5MM PITCH)")
    (attr smd)
    (fp_text reference U3001 (at 0.0635 -0.50292) (layer F.SilkS))
    (fp_text value TS3DS26227 (at -0.18796 -0.0254) (layer F.SilkS))
    (pad A1 smd circle (at -0.7493 0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 327 GPIO97))
    (pad A2 smd circle (at -0.7493 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 150 VCSI=VAUX2???))
    (pad A3 smd circle (at -0.7493 -0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 327 GPIO97))
    (pad B1 smd circle (at -0.24892 0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 340 /Camera/CSI-B-C+_UPPER))
    (pad B2 smd circle (at -0.24892 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad B3 smd circle (at -0.24892 -0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 339 /Camera/CSI-B-C-_UPPER))
    (pad C1 smd circle (at 0.24892 0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 861 "Net-(R3003-Pad2)"))
    (pad C2 smd circle (at 0.24892 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad C3 smd circle (at 0.24892 -0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 860 "Net-(R3003-Pad1)"))
    (pad D1 smd circle (at 0.7493 0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 602 "Net-(P3001-Pad9)"))
    (pad D2 smd circle (at 0.7493 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 151 VDDA))
    (pad D3 smd circle (at 0.7493 -0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 603 "Net-(P3001-Pad10)"))
  )
  (module neo900-legacy:R-XBGA-N12-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "TI YZG (0.5MM PITCH)")
    (tags "TI YZG (0.5MM PITCH)")
    (attr smd)
    (fp_text reference U3002 (at 0.0635 -0.50292) (layer F.SilkS))
    (fp_text value TS3DS26227 (at -0.18796 -0.0254) (layer F.SilkS))
    (pad A1 smd circle (at -0.7493 0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 327 GPIO97))
    (pad A2 smd circle (at -0.7493 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 150 VCSI=VAUX2???))
    (pad A3 smd circle (at -0.7493 -0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 327 GPIO97))
    (pad B1 smd circle (at -0.24892 0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 342 /Camera/CSI-B-D+_UPPER))
    (pad B2 smd circle (at -0.24892 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad B3 smd circle (at -0.24892 -0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 341 /Camera/CSI-B-D-_UPPER))
    (pad C1 smd circle (at 0.24892 0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 863 "Net-(R3004-Pad2)"))
    (pad C2 smd circle (at 0.24892 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad C3 smd circle (at 0.24892 -0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 862 "Net-(R3004-Pad1)"))
    (pad D1 smd circle (at 0.7493 0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 600 "Net-(P3001-Pad6)"))
    (pad D2 smd circle (at 0.7493 0) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 151 VDDA))
    (pad D3 smd circle (at 0.7493 -0.49784) (size 0.24892 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 601 "Net-(P3001-Pad7)"))
  )
  (module neo900-legacy:NONE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (tags "COMPONENT WITH NO ELECTRICAL PACKAGE")
    (attr virtual)
    (fp_text reference U3003 (at 0 0) (layer F.SilkS))
    (fp_text value "slide magnetic sensor" (at 0 0) (layer F.SilkS))
  )
  (module neo900-legacy:QFN-24+E-0.5 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "QFN-24 + E 0.5MM")
    (tags "QFN-24 + E 0.5MM")
    (attr smd)
    (fp_text reference U3101 (at 1.45288 -0.07366 270) (layer F.SilkS))
    (fp_text value LP55231 (at 0.55372 0.1778 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.99898 -1.24968) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(C3102-Pad1)"))
    (pad 2 smd rect (at -1.99898 -0.7493) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(C3101-Pad1)"))
    (pad 3 smd rect (at -1.99898 -0.24892) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad 4 smd rect (at -1.99898 0.24892) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 5 smd rect (at -1.99898 0.7493) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1166 GPIO-LED-EN_UPPER))
    (pad 6 smd rect (at -1.99898 1.24968) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1167 32KHZ_UPPER))
    (pad 7 smd rect (at -1.24968 1.99898 90) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1168 GPIO-RGB-INT_UPPER))
    (pad 8 smd rect (at -0.7493 1.99898 90) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 606 I2C3-SDA-CPU))
    (pad 9 smd rect (at -0.24892 1.99898 90) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 605 I2C3-SCL-CPU))
    (pad 10 smd rect (at 0.24892 1.99898 90) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 11 smd rect (at 0.7493 1.99898 90) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 228 "Net-(LED3102-Pad1)"))
    (pad 12 smd rect (at 1.24968 1.99898 90) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(LED3102-Pad3)"))
    (pad 13 smd rect (at 1.99898 1.24968 180) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 344 "Net-(P-DISP3709-Pad61)"))
    (pad 14 smd rect (at 1.99898 0.7493 180) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 346 "Net-(P-DISP3709-Pad63)"))
    (pad 15 smd rect (at 1.99898 0.24892 180) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 345 "Net-(P-DISP3709-Pad62)"))
    (pad 16 smd rect (at 1.99898 -0.24892 180) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(LED3102-Pad2)"))
    (pad 17 smd rect (at 1.99898 -0.7493 180) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(LED3101-Pad1)"))
    (pad 18 smd rect (at 1.99898 -1.24968 180) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(LED3101-Pad3)"))
    (pad 19 smd rect (at 1.24968 -1.99898 270) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(LED3101-Pad2)"))
    (pad 20 smd rect (at 0.7493 -1.99898 270) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 21 smd rect (at 0.24892 -1.99898 270) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad 22 smd rect (at -0.24892 -1.99898 270) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(C3103-Pad1)"))
    (pad 23 smd rect (at -0.7493 -1.99898 270) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(C3102-Pad2)"))
    (pad 24 smd rect (at -1.24968 -1.99898 270) (size 0.6477 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(C3101-Pad2)"))
    (pad EXP smd rect (at 0 0) (size 2.69748 2.69748) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
  )
  (module neo900-legacy:YZR0036 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr BGA-YZR0036-0.5MM)
    (tags BGA-YZR0036-0.5MM)
    (attr smd)
    (fp_text reference U3201 (at -1.27254 0.4318 90) (layer F.SilkS))
    (fp_text value LP55281YZR (at -0.76454 0.58674 90) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.65mm" (at 4.18846 -3.23342) (layer B.SilkS))
    (pad A1 smd circle (at 1.24968 1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad A2 smd circle (at 0.7493 1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(LED3203-Pad3)"))
    (pad A3 smd circle (at 0.24892 1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(LED3203-Pad1)"))
    (pad A4 smd circle (at -0.24892 1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(LED3203-Pad2)"))
    (pad A5 smd circle (at -0.7493 1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad A6 smd circle (at -1.24968 1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(LED3201-Pad3)"))
    (pad B1 smd circle (at 1.24968 0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(C3205-Pad2)"))
    (pad B2 smd circle (at 0.7493 0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad B3 smd circle (at 0.24892 0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 605 I2C3-SCL-CPU))
    (pad B4 smd circle (at -0.24892 0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1169 "Net-(U3201-PadB4)"))
    (pad B5 smd circle (at -0.7493 0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 864 "Net-(R3201-Pad2)"))
    (pad B6 smd circle (at -1.24968 0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(LED3201-Pad1)"))
    (pad C1 smd circle (at 1.24968 0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(C3207-Pad2)"))
    (pad C2 smd circle (at 0.7493 0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 866 "Net-(R3203-Pad2)"))
    (pad C3 smd circle (at 0.24892 0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad C4 smd circle (at -0.24892 0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad C5 smd circle (at -0.7493 0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 606 I2C3-SDA-CPU))
    (pad C6 smd circle (at -1.24968 0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(LED3201-Pad2)"))
    (pad D1 smd circle (at 1.24968 -0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad D2 smd circle (at 0.7493 -0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1170 "Net-(U3201-PadD2)"))
    (pad D3 smd circle (at 0.24892 -0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad D4 smd circle (at -0.24892 -0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1171 "Net-(U3201-PadD4)"))
    (pad D5 smd circle (at -0.7493 -0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 243 "Net-(LED3205-Pad1)"))
    (pad D6 smd circle (at -1.24968 -0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(LED3205-Pad3)"))
    (pad E1 smd circle (at 1.24968 -0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 252 "Net-(LED3208-Pad3)"))
    (pad E2 smd circle (at 0.7493 -0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(LED3208-Pad1)"))
    (pad E3 smd circle (at 0.24892 -0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(LED3208-Pad2)"))
    (pad E4 smd circle (at -0.24892 -0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad E5 smd circle (at -0.7493 -0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(LED3205-Pad2)"))
    (pad E6 smd circle (at -1.24968 -0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(D3201-PadK)"))
    (pad F1 smd circle (at 1.24968 -1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad F2 smd circle (at 0.7493 -1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1172 "Net-(U3201-PadF2)"))
    (pad F3 smd circle (at 0.24892 -1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 635 NRESWARM-CPU))
    (pad F4 smd circle (at -0.24892 -1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad F5 smd circle (at -0.7493 -1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad F6 smd circle (at -1.24968 -1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(D3201-PadA)"))
  )
  (module neo900-legacy:YZR0036 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr BGA-YZR0036-0.5MM)
    (tags BGA-YZR0036-0.5MM)
    (attr smd)
    (fp_text reference U3202 (at -1.27254 0.4318 90) (layer F.SilkS))
    (fp_text value LP55281YZR (at -0.76454 0.58674 90) (layer F.SilkS))
    (fp_text user "HEIGHT> 0.65mm" (at 4.18846 -3.23342) (layer B.SilkS))
    (pad A1 smd circle (at 1.24968 1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad A2 smd circle (at 0.7493 1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(LED3204-Pad3)"))
    (pad A3 smd circle (at 0.24892 1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 240 "Net-(LED3204-Pad1)"))
    (pad A4 smd circle (at -0.24892 1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(LED3204-Pad2)"))
    (pad A5 smd circle (at -0.7493 1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad A6 smd circle (at -1.24968 1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(LED3202-Pad3)"))
    (pad B1 smd circle (at 1.24968 0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(C3206-Pad2)"))
    (pad B2 smd circle (at 0.7493 0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad B3 smd circle (at 0.24892 0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 605 I2C3-SCL-CPU))
    (pad B4 smd circle (at -0.24892 0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1173 "Net-(U3202-PadB4)"))
    (pad B5 smd circle (at -0.7493 0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 865 "Net-(R3202-Pad2)"))
    (pad B6 smd circle (at -1.24968 0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(LED3202-Pad1)"))
    (pad C1 smd circle (at 1.24968 0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(C3208-Pad2)"))
    (pad C2 smd circle (at 0.7493 0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 867 "Net-(R3204-Pad2)"))
    (pad C3 smd circle (at 0.24892 0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 135 1V8-CPU))
    (pad C4 smd circle (at -0.24892 0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad C5 smd circle (at -0.7493 0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 606 I2C3-SDA-CPU))
    (pad C6 smd circle (at -1.24968 0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(LED3202-Pad2)"))
    (pad D1 smd circle (at 1.24968 -0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad D2 smd circle (at 0.7493 -0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1174 "Net-(U3202-PadD2)"))
    (pad D3 smd circle (at 0.24892 -0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 157 VSYS_UPPER))
    (pad D4 smd circle (at -0.24892 -0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1175 "Net-(U3202-PadD4)"))
    (pad D5 smd circle (at -0.7493 -0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(LED3206-Pad4)"))
    (pad D6 smd circle (at -1.24968 -0.24892 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(LED3206-Pad6)"))
    (pad E1 smd circle (at 1.24968 -0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 254 CHG_IND))
    (pad E2 smd circle (at 0.7493 -0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(LED3209-PadK)"))
    (pad E3 smd circle (at 0.24892 -0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 249 "Net-(LED3207-PadK)"))
    (pad E4 smd circle (at -0.24892 -0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad E5 smd circle (at -0.7493 -0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(LED3206-Pad5)"))
    (pad E6 smd circle (at -1.24968 -0.7493 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(D3202-PadK)"))
    (pad F1 smd circle (at 1.24968 -1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad F2 smd circle (at 0.7493 -1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1176 "Net-(U3202-PadF2)"))
    (pad F3 smd circle (at 0.24892 -1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 635 NRESWARM-CPU))
    (pad F4 smd circle (at -0.24892 -1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad F5 smd circle (at -0.7493 -1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 136 GND3))
    (pad F6 smd circle (at -1.24968 -1.24968 180) (size 0.29972 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(D3202-PadA)"))
  )
  (module neo900-legacy:SON-3X3 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr S-PVSON-N8)
    (tags S-PVSON-N8)
    (attr smd)
    (fp_text reference U3401 (at -0.78232 -1.50114) (layer F.SilkS))
    (fp_text value TPS73701DRB (at -0.57912 -0.9017) (layer F.SilkS))
    (pad 1 smd rect (at -0.97282 1.4732) (size 0.34798 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 164 "/BB-XM Adapter (CPU)/BB-VSYS"))
    (pad 2 smd rect (at -0.32258 1.4732) (size 0.34798 0.89916) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.32258 1.4732) (size 0.34798 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 871 "/BB-XM Adapter (CPU)/N$68"))
    (pad 4 smd rect (at 0.97282 1.4732) (size 0.34798 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 5 smd rect (at 0.97282 -1.4732) (size 0.34798 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 748 BB-1V8))
    (pad 6 smd rect (at 0.32258 -1.4732) (size 0.34798 0.89916) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -0.32258 -1.4732) (size 0.34798 0.89916) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -0.97282 -1.4732) (size 0.34798 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 162 BB-5V))
    (pad 9 smd rect (at 0 0) (size 1.74752 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 10 smd rect (at -1.37922 -0.3175) (size 1.01854 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 11 smd rect (at 1.37922 -0.3175) (size 1.01854 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 12 smd rect (at 1.37922 0.32004) (size 1.01854 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
    (pad 13 smd rect (at -1.37922 0.32004) (size 1.01854 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 163 GND4))
  )
  (module neo900-legacy:1PIN-HOLE (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr virtual)
    (fp_text reference VBATT3709 (at 0 0) (layer F.SilkS))
    (fp_text value - (at 0 0) (layer F.SilkS))
    (pad P$1 thru_hole oval (at 0 0 90) (size 2.99974 5.99948) (drill 1.99898) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 26 "Net-(BATT+3709-PadP)"))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference VIBRA+3709 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 1177 VIB+))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference VIBRA-3709 (at 0 0) (layer F.SilkS))
    (fp_text value ~ (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 1178 VIB-))
  )
  (module neo900-legacy:PREC-MICRO-304-106 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "PRECISION MICRO VIBRAMOTOR MODEL 304-106")
    (tags "PRECISION MICRO VIBRAMOTOR MODEL 304-106")
    (attr smd)
    (fp_text reference VIBRA3709 (at 4.52374 -0.70358) (layer F.SilkS))
    (fp_text value PREC-MICRO-304-106 (at 4.82854 0.79502) (layer F.SilkS))
    (pad 1 smd rect (at 0.6985 -1.4478) (size 1.39954 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 1178 VIB-))
    (pad 2 smd rect (at 0.6985 1.4478) (size 1.39954 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 1177 VIB+))
    (pad SHIE smd rect (at 4.54914 0) (size 4.699 4.699) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:TP-1.25 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference WAKEUP3709 (at 0 0) (layer F.SilkS))
    (fp_text value WAKEUP (at 1.9304 0) (layer F.SilkS))
    (pad P smd circle (at 0 0) (size 1.24968 1.24968) (layers F.Cu F.Paste F.Mask)
      (net 264 3G-WOE))
  )
  (module neo900-legacy:N900-SPRING-A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference WWAN-GND801 (at 0 0) (layer F.SilkS))
    (fp_text value CONNECT-POINTN900-A (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:N900-SPRING-A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference WWAN-GND802 (at 0 0) (layer F.SilkS))
    (fp_text value CONNECT-POINTN900-A (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
  (module neo900-legacy:N900-SPRING-A (layer F.Cu) (tedit 200000)
    (at 0 0)
    (attr smd)
    (fp_text reference WWAN3709 (at 0 0) (layer F.SilkS))
    (fp_text value CONNECT-POINTN900-A (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 180) (size 3.49758 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C802-Pad1)"))
  )
  (module neo900-legacy:XO-3225 (layer F.Cu) (tedit 200000)
    (at 0 0)
    (descr "HOSONIC HXO N SERIES")
    (tags "HOSONIC HXO N SERIES")
    (attr smd)
    (fp_text reference X1601 (at -0.28194 -0.9017) (layer F.SilkS))
    (fp_text value 13.56MHz (at -0.38354 -0.45212) (layer F.SilkS))
    (pad 1 smd rect (at -0.92456 0.7239) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.92456 0.7239) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at 0.92456 -0.7239) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -0.92456 -0.7239) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
  )
)
